Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

Tyan Thunder K8W (S2885), AMD Opteron (TM) 250

SPECfp_rate2000 = SPECfp_rate_base2000 =

36.3 35.6

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Apr-2004 Hardware Avail: May-2004 Software Avail: Apr-2004

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 10 20 30 40 50 60 70 168.wupwise 2 93.7 39.6 2 80.3 46.2

171.swim 2 181 39.7 2 181 39.7

172.mgrid 2 127 32.8 2 125 33.5

173.applu 2 154 31.6 2 176 27.6

177.mesa 2 79.8 40.7 2 75.5 43.0

178.galgel 2 106 63.5 2 98.5 68.3

179.art 2 181 33.3 2 179 33.6

183.equake 2 89.2 33.8 2 85.8 35.1

187.facerec 2 88.0 50.1 2 88.0 50.1

188.ammp 2 158 32.3 2 153 33.3

189.lucas 2 130 35.8 2 127 36.4

191.fma3d 2 140 34.8 2 140 34.8

200.sixtrack 2 150 17.0 2 150 17.0

301.apsi 2 185 32.6 2 185 32.6

Hardware

CPU: AMD Opteron (TM) 250 CPU MHz: 2400 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 2 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 4x512 MB PC3200 DDR SDRAM ECC Registered CL3.0 Disk Subsystem: SCSI, Ultra 320, 15k rpm Other Hardware: None

Software

Operating System: SuSE Linux 8.0 SLES 64 bit (SP3) SuSE NUMA kernel 2.4.21-143 Compiler: PGI Fortran 5.1-3

SuSE gcc33 optional compiler (from SLES8 SP3) AMD Core Math Library (Version 1.5) for AMD64

File System: Linux/ext3 System State: Multi-user SuSE Run level 3

Notes/Tuning Information

  +FDO: PASS1=-fprofile-arcs PASS2=-fbranch-probabilities
  +ACML is linking with AMD Core Math Library
  pgf90 is the PGI Fortran compiler
  gcc is the SuSE optional gcc 3.3 compiler (from SLES8 SP3)
  Portability:
                    PORTABILITY=-DSPEC_CPU2000_LP64 is applied to all the C benchmarks.
    178.galgel:     -Mfixed
  Baseline: C       gcc   -O3 -funroll-all-loops +FDO
  Baseline: Fortran pgf90 -fastsse  -Mipa=fast
  Peak tuning:
    168.wupwise:    pgf90 -fastsse -Mipa=fast -Minline=levels:2
    171.swim:       basepeak=true
    172.mgrid:      pgf90 -fast -Mipa=fast
    173.applu:      pgf90 -fast -Mipa=fast
    177.mesa:       gcc   -O3 -funroll-all-loops -finline-limit=2000 +FDO
    178.galgel:     pgf90 -fastsse -O3 -mp RM_SOURCES=lapak.f90 +ACML
    179.art:        gcc   -O3 -funroll-all-loops -ffast-math -finline-limit=1500 +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

Tyan Thunder K8W (S2885), AMD Opteron (TM) 250

SPECfp_rate2000 = SPECfp_rate_base2000 =

36.3 35.6

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Apr-2004 Hardware Avail: May-2004 Software Avail: Apr-2004

Notes/Tuning Information (Continued)

    183.equake:     gcc   -O3 -funroll-all-loops -ffast-math -finline-limit=2000
    187.facerec:    basepeak=true
    188.ammp:       gcc   -O3 -funroll-all-loops -ffast-math -finline-limit=2000 +FDO
    189.lucas:      pgf90 -fastsse -Mipa=fast -Mnosmart
    191.fma3d:      basepeak=true
    200.sixtrack:   basepeak=true
    301.apsi:       basepeak=true
  ONESTEP is used for all base and peak runs
Taskset utility used to bind processes to CPU(s)
BIOS rev.: 1.01