Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

ASUS SK8V Motherboard, AMD Opteron (TM) 150

SPECint2000 = SPECint_base2000 =

1655 1566

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: May-2004 Hardware Avail: Jun-2004 Software Avail: Feb-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

164.gzip 1400 105 1333 105 1339

175.vpr 1400 109 1282 105 1328

176.gcc 1100 62.0 1773 62.2 1768

181.mcf 1800 172 1048 138 1303

186.crafty 1000 63.8 1569 58.3 1717

197.parser 1800 121 1484 120 1498

252.eon 1300 57.4 2265 50.1 2597

253.perlbmk 1800 121 1491 108 1668

254.gap 1100 65.8 1672 64.9 1695

255.vortex 1900 75.6 2512 80.4 2363

256.bzip2 1500 119 1263 116 1289

300.twolf 3000 183 1641 167 1798

Hardware

CPU: AMD Opteron (TM)150 CPU MHz: 2400 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2x512 MB PC3200 DDR SDRAM ECC Reg CL2 Disk Subsystem: SATA, Western Digital WD360GD Other Hardware: None

Software

Operating System: Microsoft Windows XP Professional SP1a Compiler: Intel C++ 8.0 build 20031229Z

Microsoft Visual Studio .NET 7.0.9466 (libraries) MicroQuill Smartheap Library 6.0

File System: NTFS System State: Default

Notes/Tuning Information

Tested by AMD
  shlW32M6.lib is the SmartHeap library V6.0 from MicroQuill www.microquill.com
  +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
  Portability:
    176.gcc:      -Dalloca=_alloca /F10000000
    186.crafty:   -DNT_i386
    253.perlbmk:  -DSPEC_CPU2000_NTOS -DPERLDLL /MT
    254.gap:      -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO
  Baseline C:   -fast -arch:SSE2 -Oi- +FDO
  Baseline C++: -fast -arch:SSE2 -GX -GR
 Peak Tuning:
  164.gzip:     -fast -arch:SSE  +FDO shlW32M6.lib
  175.vpr:      -fast -arch:SSE2 +FDO
                -Qoption,c,-ip_ninl_max_stats=2000 -Qoption,c,-ip_ninl_max_total_stats=4500
  176.gcc:      -fast -arch:SSE2 +FDO -Oi- -Qunroll3
  181.mcf:      -fast -QaxN      +FDO
  186.crafty:   -fast -arch:SSE2 +FDO
  197.parser:         -arch:SSE2 +FDO -Oi- -Qipo
  252.eon:      -fast -arch:SSE2 +FDO -Qansi_alias

                -Qoption,c,-ip_ninl_max_stats=2000 -Qoption,c,-ip_ninl_max_total_stats=4500

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

ASUS SK8V Motherboard, AMD Opteron (TM) 150

SPECint2000 = SPECint_base2000 =

1655 1566

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: May-2004 Hardware Avail: Jun-2004 Software Avail: Feb-2004

Notes/Tuning Information (Continued)

  253.perlbmk:        -arch:SSE2 +FDO      -Qipo shlW32M6.lib
  254.gap:      -fast -arch:SSE2 +FDO -Oi- -Oa
                -Qoption,c,-ip_ninl_max_stats=500 -Qoption,c,-ip_ninl_max_total_stats=3000
  255.vortex:   -fast -arch:SSE  +FDO -Oi- shlW32M6.lib
                -Qoption,c,-ip_ninl_max_stats=2000 -Qoption,c,-ip_ninl_max_total_stats=4500
  256.bzip2:    -fast                      -Qunroll2
  300.twolf:    -fast -arch:SSE2 +FDO      -Qunroll3 shlW32M6.lib -Qansi_alias
 The tested system can be assembled using an ATX case such as the Antec KS-282,
 a 480W power supply, such as an Antec True Power 480 and a PCI or AGP video card.
 BIOS rev.: 1001
 Memory used is Corsair CMX512R-3200C2
 Cas Latency manually set to 2.0 in BIOS