Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Bull SAS

Bull Escala PL250R+ (2100 MHz, 1 CPU)

SPECint^®2006 = 12.8

SPECint_base2006 = 10.1

CPU2006 license: 20 Test date: Jan-2007 Test sponsor: Bull SAS Hardware Availability: Feb-2006 Tested by: Bull SAS Software Availability: Dec-2006

400.perlbench

401.bzip2

403.gcc

429.mcf

445.gobmk

456.hmmer

458.sjeng

462.libquantum

464.h264ref

471.omnetpp

473.astar

483.xalancbmk

SPECint2006 = 12.8

SPECint_base2006 = 10.1

0 50.0

2.00 4.00 6.00 8.00 10.0 12.0 14.0 16.0 18.0 20.0 22.0 24.0 26.0 28.0 30.0 32.0 34.0 36.0 38.0 40.0 42.0 44.0 46.0

7.72

8.28

9.70

10.3

12.1

13.0

21.3

26.9

10.8

14.2

7.62

8.62

9.82

10.2

13.3

49.0

18.2

19.2

7.74

8.89

8.49

9.50

4.64

6.32

Hardware

CPU Name: POWER5+ CPU Characteristics: CPU MHz: 2100 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 2 cores/chip CPU(s) orderable: 1 chip Primary Cache: 64 KB I + 32 KB D on chip per core Secondary Cache: 1920 KB I+D on chip per chip L3 Cache: 36 MB I+D off chip per chip Other Cache: None Memory: 32 GB (8x4 GB) Disk Subsystem: 1x73 GB SCSI, 15K RPM Other Hardware: None

Software

Operating System: AIX 5L V5.3 Compiler: XL C/C++ Enterprise Edition Version 8.0 for AIX

with the December 2006 PTF XL Fortran Enterprise Edition Version 10.1 for AIX with the November 2006 PTF

Auto Parallel: No File System: AIX/JFS2 System State: Multi-user Base Pointers: 32-bit Peak Pointers: 32/64-bit Other Software: ESSL 4.2.0.4

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Bull SAS

Bull Escala PL250R+ (2100 MHz, 1 CPU)

SPECint2006 = 12.8 SPECint_base2006 = 10.1

CPU2006 license: 20 Test date: Jan-2007 Test sponsor: Bull SAS Hardware Availability: Feb-2006 Tested by: Bull SAS Software Availability: Dec-2006

Results Table

Benchmark Seconds Ratio Seconds Ratio Seconds Ratio

Base Seconds Ratio Seconds Ratio Seconds Ratio

Peak

400.perlbench 1265 7.72 1268 7.71 1265 7.72 1180 8.28 1179 8.28 1179 8.29 401.bzip2 995 9.70 994 9.70 995 9.70 937 10.3 938 10.3 938 10.3 403.gcc 666 12.1 666 12.1 666 12.1 617 13.0 617 13.0 617 13.0 429.mcf 428 21.3 427 21.3 427 21.3 340 26.8 340 26.9 340 26.9 445.gobmk 975 10.8 974 10.8 974 10.8 738 14.2 737 14.2 738 14.2 456.hmmer 1225 7.62 1225 7.62 1219 7.65 1083 8.61 1083 8.62 1082 8.62 458.sjeng 1232 9.82 1232 9.82 1232 9.82 1187 10.2 1187 10.2 1187 10.2 462.libquantum 1554 13.3 1555 13.3 1554 13.3 423 49.0 423 49.0 423 49.0 464.h264ref 1218 18.2 1218 18.2 1217 18.2 1153 19.2 1153 19.2 1154 19.2 471.omnetpp 807 7.75 807 7.74 808 7.74 704 8.88 703 8.89 703 8.89 473.astar 826 8.49 827 8.49 827 8.49 739 9.50 739 9.49 739 9.50 483.xalancbmk 1486 4.64 1486 4.64 1485 4.65 1091 6.32 1091 6.33 1092 6.32

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Operating System Notes

 ulimits set to unlimited

 Large page mode was set as follows:
 vmo -r -o lgpg_regions=800 -o lgpg_size=16777216
 1 core was deconfigured and SMT disabled using the AIX commands
 smtctl -m off -w boot
 bosboot -aD
 shutdown -rF
 drmgr -r -c cpu

Base Compiler Invocation

C benchmarks:

/usr/vac/bin/xlc

C++ benchmarks:

/usr/vacpp/bin/xlC

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Bull SAS

Bull Escala PL250R+ (2100 MHz, 1 CPU)

SPECint2006 = 12.8

SPECint_base2006 = 10.1

CPU2006 license: 20 Test date: Jan-2007 Test sponsor: Bull SAS Hardware Availability: Feb-2006 Tested by: Bull SAS Software Availability: Dec-2006

Base Portability Flags

400.perlbench: -DSPEC_CPU_AIX 462.libquantum: -DSPEC_CPU_AIX 464.h264ref: -DSPEC_CPU_AIX -qchars=signed 483.xalancbmk: -DSPEC_CPU_AIX

Base Optimization Flags

C benchmarks:

-qlanglvl=extc99 -O4 -qlargepage -D_ILS_MACROS -qalloca
-qipa=noobject -blpdata -qipa=threads

C++ benchmarks:

-O4 -qlargepage -D_ILS_MACROS -qrtti=all -qipa=noobject -blpdata
-qipa=threads

Base Other Flags

C benchmarks:

-bmaxdata:0x50000000 -qalias=noansi -qsuppress=1500-036

C++ benchmarks:

-bmaxdata:0x20000000 -qsuppress=1500-036

Peak Compiler Invocation

C benchmarks:

/usr/vac/bin/xlc

C++ benchmarks:

/usr/vacpp/bin/xlC

Peak Portability Flags

400.perlbench: -DSPEC_CPU_AIX 462.libquantum: -DSPEC_CPU_AIX 464.h264ref: -DSPEC_CPU_AIX -qchars=signed 483.xalancbmk: -DSPEC_CPU_AIX

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Bull SAS

Bull Escala PL250R+ (2100 MHz, 1 CPU)

SPECint2006 = 12.8

SPECint_base2006 = 10.1

CPU2006 license: 20 Test date: Jan-2007 Test sponsor: Bull SAS Hardware Availability: Feb-2006 Tested by: Bull SAS Software Availability: Dec-2006

Peak Optimization Flags

C benchmarks:

400.perlbench: -qlanglvl=extc99 -qpdf1(pass 1) -qpdf2(pass 2) -O5

-qlargepage -D_ILS_MACROS -qipa=noobject -blpdata
-qipa=threads

401.bzip2: Same as 400.perlbench

403.gcc: -qlanglvl=extc99 -qpdf1(pass 1) -qpdf2(pass 2) -O5

-qlargepage -D_ILS_MACROS -qalloca -qipa=noobject
-blpdata -qipa=threads

429.mcf: -qlanglvl=extc99 -O5 -qlargepage -D_ILS_MACROS

-qarch=pwr4 -qipa=noobject -blpdata -qipa=threads

445.gobmk: -qlanglvl=extc99 -qpdf1(pass 1) -qpdf2(pass 2) -O4

-qlargepage -D_ILS_MACROS -qipa=noobject -blpdata
-qipa=threads

456.hmmer: -qlanglvl=extc99 -O4 -qlargepage -D_ILS_MACROS

-qipa=noobject -blpdata -qipa=threads

458.sjeng: Same as 445.gobmk

462.libquantum: -qlanglvl=extc99 -qpdf1(pass 1) -qpdf2(pass 2) -O4

-qlargepage -D_ILS_MACROS -q64 -qipa=noobject -blpdata
-qipa=threads

464.h264ref: Same as 400.perlbench

C++ benchmarks:

471.omnetpp: -qpdf1(pass 1) -qpdf2(pass 2) -O5 -qlargepage

-D_ILS_MACROS -qalign=natural -qrtti=all
-D__IBM_FAST_VECTOR -qipa=noobject -blpdata -qipa=threads

473.astar: -qpdf1(pass 1) -qpdf2(pass 2) -O5 -qlargepage

-D_ILS_MACROS -D__IBM_ENABLE_POOLED_ALLOCATORS__
-qipa=noobject -blpdata -qipa=threads

483.xalancbmk: Same as 473.astar

Peak Other Flags

C benchmarks (except as noted below):

-qfdpr -qsuppress=1500-036

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 5 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Bull SAS

Bull Escala PL250R+ (2100 MHz, 1 CPU)

SPECint2006 = 12.8 SPECint_base2006 = 10.1

CPU2006 license: 20 Test date: Jan-2007 Test sponsor: Bull SAS Hardware Availability: Feb-2006 Tested by: Bull SAS Software Availability: Dec-2006

Peak Other Flags (Continued)

400.perlbench: -bmaxdata:0x50000000 -qalias=noansi -qsuppress=1500-036 401.bzip2: -bmaxdata:0x50000000 -qsuppress=1500-036 403.gcc: -bmaxdata:0x50000000 -qsuppress=1500-036 429.mcf: -bmaxdata:0x50000000 -qfdpr -qsuppress=1500-036 458.sjeng: -qsuppress=1500-036 464.h264ref: -qsuppress=1500-036 C++ benchmarks:

-bmaxdata:0x20000000 -qsuppress=1500-036

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/CPU2006_flags.20090715.15.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/CPU2006_flags.20090715.15.xml

Originally published on 6 March 2007.

Report generated on Tue Jul 22 10:37:26 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.0.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECint are registered trademarks of the Standard Performance