Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Supermicro Motherboard X7DB8

SPECint^®_rate2006 = 90.9

SPECint_rate_base2006 = 83.7

CPU2006 license: 001176 Test date: Jun-2007 Test sponsor: Supermicro Hardware Availability: May-2007 Tested by: Supermicro Software Availability: Apr-2007

400.perlbench

401.bzip2

403.gcc

429.mcf

445.gobmk

456.hmmer

458.sjeng

462.libquantum

464.h264ref

471.omnetpp

473.astar

483.xalancbmk

Copies

SPECint_rate2006 = 90.9

SPECint_rate_base2006 = 83.7

0 225

10.0 20.0 30.0 40.0 50.0 60.0 70.0 80.0 90.0 100 110 120 130 140 150 160 170 180 190 200 210 8 142 8 162

8 77.0

8 78.9

8 29.2

8 45.8

8 66.8

8 132 8 146

8 109 8 110

8 121 8 135

8 49.2

8 51.5

8 209 8 221

8 46.9

8 47.8

8 66.0

8 68.7

8 99.4

8 100

Hardware

CPU Name: Intel Xeon X5355 CPU Characteristics: 2.67GHz 1333MHz System Bus CPU MHz: 2667 FPU: Integrated CPU(s) enabled: 8 cores, 2 chips, 4 cores/chip CPU(s) orderable: 1, 2 chips Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 8 MB I+D on chip per chip, 4 MB shared / 2 cores L3 Cache: None Other Cache: None Memory: 16 GB (8 X 2GB ECC PC2-5300, CL5, FBDIMM) Disk Subsystem: Seagate ST3750640AS 750GB SATA II, 7200RPM Other Hardware: None

Software

Operating System: Windows Server 2003 Enterprise Edition W/ SP1 Compiler: Intel C++ Compiler for IA32 version 10.0

Build 20070426 Package ID: W_CC_P_10.0.025 Microsoft Visual Studio .Net 2003 (for libraries)

Auto Parallel: No File System: NTFS System State: Default Base Pointers: 32-bit Peak Pointers: 32-bit Other Software: None SmartHeap Library Version 8.0 from http://www.microquill.com/

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Supermicro Motherboard X7DB8

SPECint_rate2006 = 90.9 SPECint_rate_base2006 = 83.7

CPU2006 license: 001176 Test date: Jun-2007 Test sponsor: Supermicro Hardware Availability: May-2007 Tested by: Supermicro Software Availability: Apr-2007

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

400.perlbench 8 549 142 549 142 549 142 8 484 162 484 162 484 162 401.bzip2 8 1001 77.1 1003 77.0 1002 77.0 8 979 78.8 979 78.9 978 78.9 403.gcc 8 2207 29.2 2203 29.2 2205 29.2 8 1406 45.8 1397 46.1 1410 45.7 429.mcf 8 1092 66.8 1091 66.9 1092 66.8 8 1092 66.8 1091 66.9 1092 66.8 445.gobmk 8 635 132 634 132 629 134 8 573 146 578 145 571 147 456.hmmer 8 684 109 684 109 684 109 8 677 110 677 110 677 110 458.sjeng 8 802 121 801 121 803 121 8 718 135 719 135 718 135 462.libquantum 8 3370 49.2 3371 49.2 3371 49.2 8 3222 51.4 3217 51.5 3219 51.5 464.h264ref 8 847 209 848 209 846 209 8 801 221 801 221 801 221 471.omnetpp 8 1065 47.0 1065 46.9 1065 46.9 8 1047 47.8 1047 47.8 1047 47.8 473.astar 8 851 66.0 851 66.0 851 66.0 8 817 68.7 818 68.6 818 68.7 483.xalancbmk 8 555 99.4 555 99.4 555 99.4 8 550 100 551 100 551 100

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

General Notes

 Tested systems can be used with CSE-825S2-R700LPV case,
 To ensure system stability,
 a 500W (minimum) ATX power supply [4-pin (+12V), 8-pin (+12V) and 24-pin are required]
 Product description located as of
 http://www.supermicro.com/products/motherboard/Xeon1333/5000P/X7DB8.cfm
 The system bus runs at 1333 MHz
 submit was used to bind processes to cores

Base Compiler Invocation

C benchmarks:

icl -Qvc7.1 -Qc99

C++ benchmarks:

icl -Qvc7.1

Base Portability Flags

403.gcc: -DSPEC_CPU_WIN32 464.h264ref: -DSPEC_CPU_NO_INTTYPES -DWIN32

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Supermicro Motherboard X7DB8

SPECint_rate2006 = 90.9

SPECint_rate_base2006 = 83.7

CPU2006 license: 001176 Test date: Jun-2007 Test sponsor: Supermicro Hardware Availability: May-2007 Tested by: Supermicro Software Availability: Apr-2007

Base Optimization Flags

C benchmarks:

-fast /F512000000 shlw32m.lib            -link /FORCE:MULTIPLE

C++ benchmarks:

-fast -Qcxx_features /F512000000 shlw32m.lib
           -link /FORCE:MULTIPLE

Base Other Flags

C benchmarks:

403.gcc: -Dalloca=_alloca

Peak Compiler Invocation

C benchmarks:

icl -Qvc7.1 -Qc99

C++ benchmarks:

icl -Qvc7.1

Peak Portability Flags

403.gcc: -DSPEC_CPU_WIN32 464.h264ref: -DSPEC_CPU_NO_INTTYPES -DWIN32

Peak Optimization Flags

C benchmarks:

400.perlbench: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qansi-alias

-Qprefetch /F512000000 shlw32m.lib
           -link /FORCE:MULTIPLE

401.bzip2: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast /F512000000

shlw32m.lib            -link /FORCE:MULTIPLE

403.gcc: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast /F512000000

           -link /FORCE:MULTIPLE

429.mcf: basepeak = yes

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Supermicro Motherboard X7DB8

SPECint_rate2006 = 90.9

SPECint_rate_base2006 = 83.7

CPU2006 license: 001176 Test date: Jun-2007 Test sponsor: Supermicro Hardware Availability: May-2007 Tested by: Supermicro Software Availability: Apr-2007

Peak Optimization Flags (Continued)

445.gobmk: -Qprof_gen(pass 1) -Qprof_use(pass 2) -QxT -O2 -Qipo

-Qprec_div- -Qansi-alias /F512000000
           -link /FORCE:MULTIPLE

456.hmmer: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qunroll2

-Qansi-alias /F512000000 shlw32m.lib
           -link /FORCE:MULTIPLE

458.sjeng: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qunroll4

/F512000000 shlw32m.lib            -link /FORCE:MULTIPLE

462.libquantum: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qunroll4

-Ob0 -Qprefetch -Qopt-streaming-stores:always /F512000000
shlw32m.lib            -link /FORCE:MULTIPLE

464.h264ref: Same as 456.hmmer

C++ benchmarks:

-Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qansi-alias
-Qcxx_features /F512000000 shlw32m.lib
           -link /FORCE:MULTIPLE

Peak Other Flags

C benchmarks:

403.gcc: -Dalloca=_alloca

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/Intel-ic10-ia32-intel64-linux-flags.20090714.18.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/Intel-ic10-ia32-intel64-linux-flags.20090714.18.xml

Originally published on 8 August 2007.

Report generated on Tue Jul 22 12:46:08 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.0.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECint are registered trademarks of the Standard Performance