Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation SGI SGI 3800 32X 400MHz R12K

SPECompLpeak2001 = SPECompLbase2001 = -- 59452

SPEC license #:HPG0014 Tested by: SGI Test site: SGI Test date: May-2002 Hardware Avail:Sep-2000 Software Avail:Apr-2002

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 30000 60000 90000

311.wupwise_l 9200 2294 64160

313.swim_l 12500 3659 54659

315.mgrid_l 13500 2620 82447

317.applu_l 13500 3071 70327

321.equake_l 13000 3775 55107

325.apsi_l 10500 3522 47701

327.gafort_l 11000 3086 57039

329.fma3d_l 23500 6606 56915

331.art_l 25000 7480 53477

Hardware

CPU: R12000 CPU MHz: 400 FPU: Integrated CPU(s) enabled: 32 CPU(s) orderable: 4-512 Primary Cache: 32KBI + 32KBD on chip Secondary Cache: 8MB(I+D) off chip L3 Cache: N/A Other Cache: N/A Memory: 32 GB Disk Subsystem: 1 x 9 GB FC, 24x 36 GB (striped) FC Other Hardware: None

Software

OpenMP Threads: 32 Parallel: OpenMP Operating System: IRIX 6.5.16f Compiler: MIPSpro 7.3.1.3m C, Fortran90 File System: xfs System State: Multi-user

Notes/Tuning Information

Baseline flags: -64 -mp -Ofast=ip35 -LNO:fusion=2

Baseline user environment:
   OMP_DYNAMIC=FALSE
   MPC_GANG=OFF
   _DSM_MUSTRUN=
   _DSM_WAIT=SPIN