Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

Copyright ©1999-2008, Standard Performance Evaluation Corporation

Fujitsu Limited Fujitsu SPARC Enterprise T5240

SPECompMpeak2001 = SPECompMbase2001 =

25488 21145

SPEC license #:HPG0003 Tested by: Sun Microsystems Test site: Hillsboro Test date: Mar-2008 Hardware Avail:Apr-2008 Software Avail:Apr-2008

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 30000 60000 90000

310.wupwise_m 6000 167 35939 166 36166

312.swim_m 6000 251 23893 247 24277

314.mgrid_m 7300 364 20074 306 23894

316.applu_m 4000 223 17968 190 21025

318.galgel_m 5100 503 10146 253 20143

320.equake_m 2600 228 11383 125 20832

324.apsi_m 3400 157 21658 153 22200

326.gafort_m 8700 268 32404 248 35060

328.fma3d_m 4600 274 16764 223 20632

330.art_m 6400 96.3 66449 96.7 66152

332.ammp_m 7000 518 13510 467 14997

Hardware

CPU: UltraSPARC T2 Plus CPU MHz: 1415 FPU: Integrated CPU(s) enabled: 16 cores, 2 chips, 8 cores/chip, 8 threads/core CPU(s) orderable: 2 Primary Cache: 16 KB I + 8 KB D on chip per core Secondary Cache: 4 MB I+D on chip per chip L3 Cache: None Other Cache: None Memory: 64 GB (16 x 4GB) Disk Subsystem: 2 X 146GB (Seagate ST914602SSUN146G) Other Hardware: None

Software

OpenMP Threads: 128 Parallel: OpenMP and Automatic Parallelization Operating System: Solaris 10 8/07 Compiler: Sun Studio 12 File System: UFS System State: Multi User

Notes/Tuning Information

 Base flags:
   C flags:   -fast -xopenmp -xalias_level=std -xipo=2
              -xprefetch_level=2 -m64 -lmtmalloc -xprofile
   f90 flags: -fast -autopar -openmp -xipo=2 -xprefetch_level=2
       -m64 -xprefetch=latx:3 -xprofile
   ONESTEP=yes for all benchmarks in base

   Extra Base C flags: -Xc
   318.galgel_m portability flags: -e -fixed
   328.fma3d_m srcalt: ompm2001-fma3dsqrtinit-20070912, fix race condition
   330.art_m extra flags: -DINTS_PER_CACHELINE=16 -DDBLS_PER_CACHELINE=8
 Peak flags:
   ONESTEP=yes for all benchmarks in peak

   310.wupwise: -fast -autopar -openmp -xipo=2 -m64
                -xprefetch=latx:3 -xprofile
   312.swim:    -fast -openmp -autopar -xunroll=7 -m64 -xipo=2
                -xpagesize=4m -xprefetch=latx:4 -xpad=common:1921
                -Qoption iropt -Atile:skewp
   314.mgrid:   -fast -openmp -xipo=2 -xprefetch_level=3 -m64
                -xpagesize=4m -xprefetch=latx:3 -xcode=abs32
                -xunroll=8 -xprofile

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

Copyright ©1999-2008, Standard Performance Evaluation Corporation

Fujitsu Limited Fujitsu SPARC Enterprise T5240

SPECompMpeak2001 = SPECompMbase2001 =

25488 21145

SPEC license #:HPG0003 Tested by: Sun Microsystems Test site: Hillsboro Test date: Mar-2008 Hardware Avail:Apr-2008 Software Avail:Apr-2008

Notes/Tuning Information (Continued)

                OMP_NUM_THREADS=128
                SUNW_MP_PROCBIND=true
   316.applu:   -fast -openmp -autopar -xipo=2 -xprefetch_level=3
                -m64 -xprefetch=latx:4  -xcode=abs32 -xunroll=2
                -xpagesize_heap=4m -xlinkopt=2
                OMP_NUM_THREADS = 80
                SUNW_MP_PROCBIND=
                  2   3   4   5   6  10  11  12  13  14
                 18  19  20  21  22  26  27  28  29  30
                 34  35  36  37  38  42  43  44  45  46
                 50  51  52  53  54  58  59  60  61  62
                 66  67  68  69  70  74  75  76  77  78
                 82  83  84  85  86  90  91  92  93  94
                 98  99 100 101 102 106 107 108 109 110
                114 115 116 117 118 122 123 124 125 126
   318.galgel:  -fast -xipo=2 -openmp -autopar -xlic_lib=sunperf
                -xprefetch=latx:3.0 -xunroll=8 -dbl_align_all=yes
                -stackvar -xlinkopt=2 -m64 -xprofile
                RM_SOURCES=lapk.f90
                OMP_NUM_THREADS = 64
                SUNW_MP_PROCBIND=
                  3   4   5   6  11  12  13  14
                 19  20  21  22  27  28  29  30
                 35  36  37  38  43  44  45  46
                 51  52  53  54  59  60  61  62
                 67  68  69  70  75  76  77  78
                 83  84  85  86  91  92  93  94
                 99 100 101 102 107 108 109 110
                115 116 117 118 123 124 125 126
   320.equake:  -fast -xopenmp -xipo=2 -xprefetch=latx:2
                -xprefetch_level=3 -m64 -xunroll=4 -lmtmalloc -xprofile
                -xpagesize=64K  -xautopar -xprofile
                srcalt=ompl.32
                OMP_NUM_THREADS = 96
                SUNW_MP_PROCBIND=
                  1   2   3   4   5   6   9  10  11  12  13  14
                 17  18  19  20  21  22  25  26  27  28  29  30
                 33  34  35  36  37  38  41  42  43  44  45  46
                 49  50  51  52  53  54  57  58  59  60  61  62
                 65  66  67  68  69  70  73  74  75  76  77  78
                 81  82  83  84  85  86  89  90  91  92  93  94
                 97  98  99 100 101 102 105 106 107 108 109 110
                113 114 115 116 117 118 121 122 123 124 125 126
   324.apsi:    -fast -openmp -xipo=2 -m64 -xpagesize=4M
                -xprefetch=latx:5 -xunroll=5 -xprofile
                OMP_NUM_THREADS = 128
                SUNW_MP_PROCBIND=
                3 11 19 27 35 43 51 59 67 75 83 91  99 107 115 123
                4 12 20 28 36 44 52 60 68 76 84 92 100 108 116 124
                5 13 21 29 37 45 53 61 69 77 85 93 101 109 117 125
                6 14 22 30 38 46 54 62 70 78 86 94 102 110 118 126
                2 10 18 26 34 42 50 58 66 74 82 90  98 106 114 122
                7 15 23 31 39 47 55 63 71 79 87 95 103 111 119 127
                1  9 17 25 33 41 49 57 65 73 81 89  97 105 113 121
                0  8 16 24 32 40 48 56 64 72 80 88  96 104 112 120
   326.gafort:  -fast -autopar -openmp -xipo=2 -xprefetch_level=3

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

Copyright ©1999-2008, Standard Performance Evaluation Corporation

Fujitsu Limited Fujitsu SPARC Enterprise T5240

SPECompMpeak2001 = SPECompMbase2001 =

25488 21145

SPEC license #:HPG0003 Tested by: Sun Microsystems Test site: Hillsboro Test date: Mar-2008 Hardware Avail:Apr-2008 Software Avail:Apr-2008

Notes/Tuning Information (Continued)

                -m64 -xpagesize=4m -xprefetch=latx:5 -xunroll=6
                -dbl_align_all=yes -stackvar -xprofile
                OMP_NUM_THREADS = 127
                SUNW_MP_PROCBIND=
                3 11 19 27 35 43 51 59 67 75 83 91  99 107 115 123
                4 12 20 28 36 44 52 60 68 76 84 92 100 108 116 124
                5 13 21 29 37 45 53 61 69 77 85 93 101 109 117 125
                6 14 22 30 38 46 54 62 70 78 86 94 102 110 118 126
                2 10 18 26 34 42 50 58 66 74 82 90  98 106 114 122
                7 15 23 31 39 47 55 63 71 79 87 95 103 111 119 127
                1  9 17 25 33 41 49 57 65 73 81 89  97 105 113 121
                0  8 16 24 32 40 48 56 64 72 80 88  96 104 112 120
   328.fma3d:   -fast -autopar -openmp -xipo=2 -xprefetch_level=3
                -xprefetch=latx:4 -m64 -xcode=abs32 -xprofile
                srcalt=ompl.32.sqrt.init
                ompm2001-fma3dsqrtinit-20070912, fix race condition
   330.art:     -fast -xopenmp -xautopar -xipo=2 -m64 -xprofile
                OMP_NUM_THREADS = 127
                SUNW_MP_PROCBIND=
                3 11 19 27 35 43 51 59 67 75 83 91  99 107 115 123
                4 12 20 28 36 44 52 60 68 76 84 92 100 108 116 124
                5 13 21 29 37 45 53 61 69 77 85 93 101 109 117 125
                6 14 22 30 38 46 54 62 70 78 86 94 102 110 118 126
                2 10 18 26 34 42 50 58 66 74 82 90  98 106 114 122
                7 15 23 31 39 47 55 63 71 79 87 95 103 111 119 127
                1  9 17 25 33 41 49 57 65 73 81 89  97 105 113 121
                0  8 16 24 32 40 48 56 64 72 80 88  96 104 112 120
   332.ammp:    -fast -xipo=2 -xopenmp -xalias_level=strong -lm
                -xprefetch=latx:2 -xlinkopt=2 -xpagesize_stack=8K
                -xpagesize_heap=4M
                -xprefetch_auto_type=indirect_array_access

 Feedback optimization (-xprofile) is done as follows,
 unless otherwise noted:
   fdo_pre0:  rm -rf ‘pwd‘/feedback.profile
   PASS1:     -xprofile=collect:./feedback
   PASS2:     -xprofile=use:./feedback

 The following user environment was used for base runs:
   ulimit -s 32768   (in /bin/sh)
   export OMP_DYNAMIC=FALSE
   export OMP_NUM_THREADS=127
   export SUNW_MP_PROCBIND="1-127"
   export SUNW_MP_THR_IDLE=SPIN
   export STACKSIZE=16384

 The following patches were applied to Solaris Operating system:
   patch 127111-08

 Sun Studio compiler patches are available at
   http://developers.sun.com/sunstudio/downloads/patches/ss12_patches.jsp
   The tested configuration included patch 124867-02, 124861-04,
   124863-01, 127000-01

 The user environment for peak runs was same as for base except
 as noted for each benchmark.

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

Copyright ©1999-2008, Standard Performance Evaluation Corporation

Fujitsu Limited Fujitsu SPARC Enterprise T5240

SPECompMpeak2001 = SPECompMbase2001 =

25488 21145

SPEC license #:HPG0003 Tested by: Sun Microsystems Test site: Hillsboro Test date: Mar-2008 Hardware Avail:Apr-2008 Software Avail:Apr-2008

Notes/Tuning Information (Continued)

 For a description of Sun Studio 12 Compiler flags, portability flags
 and system parameters used to generate this result, please refer to
 SUN-20071009-Studio-Solaris-sparc.txt file in the flags directory.

 This result was measured on a Sun SPARC Enterprise T5240
 Note that these systems are electricly equivalent:
   - Sun SPARC Enterprise T5240
   - Fujitsu SPARC Enterprise T5240