Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Intel Corporation

Intel D850MD motherboard (1.8 GHz, Pentium 4 processor)

SPECint2000 = SPECint_base2000 = 612 601 SPEC license #: 13 Tested by: Intel Corporation Test date: Nov-2001 Hardware Avail: Aug-2001 Software Avail: Oct-2001

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 300 600 900 1200

164.gzip 1400 214 654 212 660

175.vpr 1400 403 348 402 348

176.gcc 1100 171 642 171 643

181.mcf 1800 357 505 357 505

186.crafty 1000 172 581 171 584

197.parser 1800 313 574 313 575

252.eon 1300 158 825 135 963

253.perlbmk 1800 242 745 242 744

254.gap 1100 132 834 132 834

255.vortex 1900 202 942 198 958

256.bzip2 1500 308 487 303 496

300.twolf 3000 775 387 773 388

Hardware

CPU: Pentium 4 processor (1.8 GHz, 400 MHz bus) CPU MHz: 1800 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 12k micro-ops I + 8KBD on chip Secondary Cache: 256KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 256 MB (2 128 MB PC800 RDRAM non-ECC modules) Disk Subsystem: IBM DTLA-307030 ATA-100 Other Hardware: None

Software

Operating System: Windows XP Professional(Build 2600) Compiler: Intel C++ Compiler 5.0.1 Build 010525Z

Microsoft Visual C++ 6.0 SP5(for libraries)

File System: FAT32 System State: Default

Notes/Tuning Information

 +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
 Base tuning for C programs:   -QxW -Qipo  +FDO
 Base tuning for C++ programs: -QxW -Qipo -GX -GR
 Portability flags:
 176.gcc: -Dalloca=_alloca /F10000000
 186.crafy: -DNT_i386
 253.perlbmk: -DSPEC_CPU2000_NTOS -DPERLDLL /MT
 254.gap: -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO
 Peak tuning:
 164.gzip:     -QxW -Qipo -Oa  +FDO
 175.vpr:      -QxW -Qwp_ipo +FDO
 176.gcc:      -QxW -Qipo  +FDO
 181.mcf:      -QxW -Qipo  +FDO
 186.crafty:   -QxW -Qipo -Oa  +FDO
 197.parser:   -QxW -Qipo  +FDO
 252.eon:      -QxW -Qipo +FDO
 253.perlbmk:  -QxW -Qipo  +FDO
 254.gap:      -QxW -Qipo +FDO
 Tested systems can be used with Shin-G ATX case, Delta Inc. power supply PS-300GB-1 B
 Product description located as of 1/2002:

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Intel Corporation

Intel D850MD motherboard (1.8 GHz, Pentium 4 processor)

SPECint2000 = SPECint_base2000 = 612 601 SPEC license #: 13 Tested by: Intel Corporation Test date: Nov-2001 Hardware Avail: Aug-2001 Software Avail: Oct-2001

Notes/Tuning Information (Continued)

 http://developer.intel.com/design/motherbd/md/index.htm
 Motherboard ordering information is available at:
 http://program.intel.com/shared/products/boards/D850MD/index.htm
 The system bus runs at 400 MHz