Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

Asus A7M266-D Motherboard, AMD Athlon (TM) MP 2400+

SPECint_rate2000 = SPECint_rate_base2000 =

15.4 15.0

SPEC license #: 49 Tested by: AMD Austin, TX Test date: Dec-2002 Hardware Avail: Jan-2002 Software Avail: Feb-2002

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 5 10 15 20 25 30 35 40 45 164.gzip 2 152 21.4 2 150 21.7

175.vpr 2 387 8.40 2 361 9.00

176.gcc 2 285 8.97 2 263 9.70

181.mcf 2 853 4.89 2 853 4.89

186.crafty 2 89.2 26.0 2 89.1 26.0

197.parser 2 319 13.1 2 318 13.1

252.eon 2 80.5 37.5 2 72.8 41.4

253.perlbmk 2 161 25.9 2 161 25.9

254.gap 2 154 16.6 2 152 16.8

255.vortex 2 176 25.1 2 179 24.6

256.bzip2 2 307 11.3 2 297 11.7

300.twolf 2 668 10.4 2 660 10.5

Hardware

CPU: AMD Athlon (TM) MP 2400+ CPU MHz: 2000 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1, 2 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 256KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2x256MB PC2100 DDR SDRAM CL2 Disk Subsystem: Seagate ST320414A Other Hardware: None

Software

Operating System: Windows 2000 SP2 Compiler: Intel C++ 5.0.1 build 020125Z Microsoft Visual Studio 6.0 SP5 (libraries) MicroQuill Smartheap Library 5.0 File System: FAT32 System State: Default

Notes/Tuning Information

  shlW32M.lib is the SmartHeap library V5.0 from MicroQuill www.microquill.com
  +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
  Portability:
  176.gcc:    -Dalloca=_alloca /F10000000
  186.crafty:   -DNT_i386
  253.perlbmk:  -DSPEC_CPU2000_NTOS -DPERLDLL /MT
  254.gap:    -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO
  Baseline C:   -QxK -Qipo +FDO shlW32M.lib
  Baseline C++: -QxK -Qipo -GX -GR
  Peak tuning:
  164.gzip:     -O3 -QxK -Qwp_ipo -Oi- -Oa +FDO
  175.vpr:      -O3 -Qxi -QaxK -Qwp_ipo +FDO
  176.gcc:      -O3 -QxK -Qwp_ipo -Oi- +FDO shlW32M.lib
  181.mcf:      -O3 -QxK -Qwp_ipo +FDO shlW32M.lib
  186.crafty:   -O3 -QxK -Qwp_ipo -Oa +FDO shlW32M.lib
  197.parser:   -O3 -QxK -Qwp_ipo +FDO
  252.eon:      -O3 -QxK -Qwp_ipo +FDO
  253.perlbmk:  -O3 -QxK -Qipo +FDO shlW32M.lib
  254.gap:      -O3 -QxK -Qipo -Oi- +FDO
  255.vortex:   -O3 -QxK -Qwp_ipo +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

Asus A7M266-D Motherboard, AMD Athlon (TM) MP 2400+

SPECint_rate2000 = SPECint_rate_base2000 =

15.4 15.0

SPEC license #: 49 Tested by: AMD Austin, TX Test date: Dec-2002 Hardware Avail: Jan-2002 Software Avail: Feb-2002

Notes/Tuning Information (Continued)

  256.bzip2:    -O3 -QxK -Oa -Qwp_ipo
  300.twolf:    -O3 -QxK -Qipo -Oa +FDO shlW32M.lib
  ONESTEP is used for all base and peak runs
 The tested system can be assembled using an ATX case such as the Antec KS-282,
 a 400W power supply such as the Sparkle FSP400-60GN, and a PCI or AGP video card.
 The System bus runs at 266MHz