Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

NEC Corporation TX7/i9010(1000MHz, Itanium 2)

SPECfp_rate2000 = SPECfp_rate_base2000 = -- 159 SPEC license #: 1184 Tested by: NEC T.Kokubo Test date: Dec-2002 Hardware Avail: Aug-2002 Software Avail: Nov-2002

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 100 200 300 400 500 168.wupwise 16 193 154

171.swim 16 328 176

172.mgrid 16 282 118

173.applu 16 132 295

177.mesa 16 201 129

178.galgel 16 149 360

179.art 16 140 345

183.equake 16 202 120

187.facerec 16 202 175

188.ammp 16 285 143

189.lucas 16 324 115

191.fma3d 16 537 72.6

200.sixtrack 16 127 160

301.apsi 16 440 110

Hardware

CPU: Itanium2 CPU MHz: 1000 FPU: Integrated CPU(s) enabled: 16 cores, 16 chips, 1 core/chip CPU(s) orderable: 1-16 Parallel: No Primary Cache: 16KBI + 16KBD on chip Secondary Cache: 256KB on chip L3 Cache: 3MB on chip Other Cache: None Memory: 32GB Disk Subsystem: 4x32GB SCSI disk Other Hardware: Ethernet

Software

Operating System: NEC IA-64 Linux R3.2 Compiler: NEC FORTRAN95 R3.2 NEC C/C++ R3.2 File System: ext2 System State: Multi-user

Notes/Tuning Information

 Base tuning:
    Fortran:    -O3 -ipo -ftz  +FDO
    C:          -O3 -ipo -ftz  +FDO
 +FDO:
    PASS1:      -prof_gen
    PASS2:      -prof_use
 Portability:
    178.galgel: -FI