Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company AlphaServer ES47 7/1000

SPECfp2000 = SPECfp_base2000 =

1288 975 SPEC license #: 2 Tested by: HP Test date: Dec-2002 Hardware Avail: Jan-2003 Software Avail: Jan-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 210 760 86.7 1846

171.swim 3100 99.1 3130 99.1 3130

172.mgrid 1800 293 614 192 938

173.applu 2100 159 1318 156 1345

177.mesa 1400 173 808 145 965

178.galgel 2900 158 1830 157 1851

179.art 2600 149 1741 92.4 2814

183.equake 1300 290 449 94.2 1381

187.facerec 1900 198 961 178 1069

188.ammp 2200 345 638 299 735

189.lucas 2000 150 1331 138 1453

191.fma3d 2100 238 883 177 1186

200.sixtrack 1100 272 404 252 437

301.apsi 2600 241 1078 225 1158

Hardware

CPU: Alpha 21364 CPU MHz: 1000 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 2 to 4 Parallel: No Primary Cache: 64KB(I)+64KB(D) on chip Secondary Cache: 1.75MB on chip per CPU L3 Cache: None Other Cache: None Memory: 4GB Disk Subsystem: 36GB SCSI Other Hardware: None

Software

Operating System: Tru64 UNIX V5.1B (Rev. 2650) +IPK Compiler: Compaq C V6.5-011-48C5K Spike V5.2 (506A) Compaq Fortran V5.5-2602-48C8L Compaq Fortran 77 V5.5-2602-48C8L KAP Fortran V4.3 k3105171 000607 KAP Fortran 77 V4.1 k310440 980926 KAP C V4.1 k010726 000607 File System: ufs System State: Multi-user

Notes/Tuning Information

 Baseline   C: cc  -arch ev7 -fast -O4 ONESTEP
      Fortran: f90 -arch ev7 -fast -O5 ONESTEP

 Peak:
   All use -arch ev7 -non_shared ONESTEP
   except these (which use only the tunings shown below):
        173.applu 188.ammp 191.fma3d

   Individual benchmark tuning:
   168.wupwise: kf77 -call_shared -inline all -tune ev67
                -unroll 12 -automatic -align commons -arch ev67
                -fkapargs=’ -aggressive=c -fuse
                -fuselevel=1 -so=2 -r=1 -o=1 -interleave
                -ur=6 -ur2=060 ’ +PFB
       171.swim: same as base
      172.mgrid: kf90 -call_shared -arch generic -O5 -inline

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company AlphaServer ES47 7/1000

SPECfp2000 = SPECfp_base2000 =

1288 975 SPEC license #: 2 Tested by: HP Test date: Dec-2002 Hardware Avail: Jan-2003 Software Avail: Jan-2003

Notes/Tuning Information (Continued)

                 manual -nopipeline -transform_loops -unroll 9 -automatic
                 -fkapargs=’-aggressive=a -fuse -interleave
                 -ur=2 -ur3=5 -cachesize=128,16000 ’ +PFB
     173.applu: kf90  -O5 -transform_loops
                -fkapargs=’ -o=0 -nointerleave -ur=14
                -ur2=260 -ur3=18’ +PFB
      177.mesa: kcc -fast -O4 +CFB +IFB
    178.galgel: f90 -O5 -fast -unroll 5 -automatic
       179.art: kcc  -assume whole_program -ldensemalloc
                -call_shared -assume restricted_pointers
                -unroll 16 -inline none -ckapargs=’
                -fuse -fuselevel=1 -ur=3’ +PFB
    183.equake: cc -call_shared -arch generic -fast -O4
                -ldensemalloc -assume restricted_pointers
                -inline speed -unroll 13 -xtaso_short +PFB
   187.facerec: f90 -O4 -nopipeline -inline all
                -non_shared -speculate all -unroll 7
                -automatic -assume accuracy_sensitive
                -math_library fast +IFB
      188.ammp: cc -arch host -O4 -ifo -assume nomath_errno
                -assume trusted_short_alignment -fp_reorder
                -readonly_strings -ldensemalloc -xtaso_short
                -assume restricted_pointers -unroll 9
                -inline speed +CFB +IFB +PFB
     189.lucas: kf90 -O5 -fkapargs=’-ur=1’ +PFB
     191.fma3d: kf90 -arch ev6 -non_shared -O4 -transform_loops
                -fkapargs=’-cachesize=128,16000 ’ +PFB
  200.sixtrack: f90 -fast -O5 -assume accuracy_sensitive
                -notransform_loops +PFB
      301.apsi: kf90 -O5 -inline none -call_shared -speculate all
                -align commons -fkapargs=’ -aggressive=ab
                -tune=ev5 -fuse -ur=1 -ur2=60 -ur3=20
                -cachesize=128,16000’

 Most benchmarks are built using one or more types of
 profile-driven feedback.  The types used are designated
 by abbreviations in the notes:

 +CFB: Code generation is optimized by the compiler, using
       feedback from a training run.  These commands are
       done before the first compile (in phase "fdo_pre0"):

            mkdir /tmp/pp
            rm -f /tmp/pp/${baseexe}*

       and these flags are added to the first and second compiles:

            PASS1_CFLAGS = -prof_gen_noopt -prof_dir /tmp/pp
            PASS2_CFLAGS = -prof_use       -prof_dir /tmp/pp

      (Peak builds use /tmp/pp above; base builds use /tmp/pb.)

 +IFB: Icache usage is improved by the post-link-time optimizer
       Spike, using feedback from a training run.  These commands
       are used (in phase "fdo_postN"):

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company AlphaServer ES47 7/1000

SPECfp2000 = SPECfp_base2000 =

1288 975 SPEC license #: 2 Tested by: HP Test date: Dec-2002 Hardware Avail: Jan-2003 Software Avail: Jan-2003

Notes/Tuning Information (Continued)

            mv ${baseexe} oldexe
            spike oldexe -feedback oldexe -o ${baseexe}

 +PFB: Prefetches are improved by the post-link-time optimizer
       Spike, using feedback from a training run.  These
       commands are used (in phase "fdo_post_makeN"):

            rm -f *Counts*
            mv ${baseexe} oldexe
            pixie -stats dstride oldexe 1>pixie.out 2>pixie.err
            mv oldexe.pixie ${baseexe}

       A training run is carried out (in phase "fdo_runN"), and
       then this command (in phase "fdo_postN"):

            spike oldexe -fb oldexe -stride_prefetch -o ${baseexe}

 When Spike is used for both Icache and Prefetch improvements,
 only one spike command is actually issued, with the Icache
 options followed by the Prefetch options.

 vm:
         vm_bigpg_enabled = 1
         vm_bigpg_thresh=16
         vm_swap_eager = 0

 proc:
         max_per_proc_address_space = 0x40000000000
         max_per_proc_data_size = 0x40000000000
         max_per_proc_stack_size = 0x40000000000
         max_proc_per_user = 2048
         max_threads_per_user = 0
         maxusers = 16384
         per_proc_address_space = 0x40000000000
         per_proc_data_size = 0x40000000000
         per_proc_stack_size = 0x40000000000

 Portability: galgel: -fixed

 Information on UNIX V5.1B Patches can be found at
 http://ftp1.service.digital.com/public/unix/v5.1b/

 In the ES47, there are two cpus per shelf.  Each cpu has
 its own 4GB of memory.  Neither of the cpus can be
 physically removed.  For 1 cpu results measured on a 2 cpu
 system, one cpu was turned off at boot time using the
 /etc/sysconfigtab setting "cpu_enabled_mask=0".  The cpu’s
 4GB of memory was also physically removed.