Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Intel Corporation

Intel D875PBZ motherboard (AA-301) (3.2E GHz, Pentium 4 Processor with Hyper-Threading Technology)

SPECint2000 = SPECint_base2000 =

1420 1363

SPEC license #: 13 Tested by: Intel Corporation Test date: Jan-2004 Hardware Avail: Feb-2004 Software Avail: Dec-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

164.gzip 1400 132 1065 131 1065

175.vpr 1400 148 945 148 946

176.gcc 1100 63.6 1728 63.7 1728

181.mcf 1800 146 1232 146 1232

186.crafty 1000 84.5 1184 84.4 1184

197.parser 1800 144 1246 144 1246

252.eon 1300 83.2 1563 69.8 1863

253.perlbmk 1800 120 1499 107 1681

254.gap 1100 64.2 1713 64.3 1710

255.vortex 1900 77.6 2450 77.6 2450

256.bzip2 1500 147 1021 143 1050

300.twolf 3000 232 1295 194 1545

Hardware

CPU: Intel Pentium 4 Processor with Hyper-Threading Technology(3.2E GHz, 800 MHz bus) CPU MHz: 3200 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip (Hyper-Threading Technology enabled) CPU(s) orderable: 1 Parallel: No Primary Cache: 12k micro-ops I + 16KBD on chip Secondary Cache: 1MB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 1 GB(2 512MB PC3200 Samsung Double-sided CL3-3-3 DIMMs) Disk Subsystem: Seagate ST3160023AS 160 GB Serial ATA (7200 RPM, 8MB cache) Other Hardware: None

Software

Operating System: Windows XP Professional Service Pack 1a Compiler: Intel C++ Compiler 8.0 Build 20031017Z

Microsoft Visual Studio .Net 7.0(for libraries) MicroQuill SmartHeap library V6.0

File System: NTFS System State: Default

Notes/Tuning Information

 ONESTEP=yes for all base and peak runs    +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use (Qxp not used in PASS1)

 Base tuning for C programs:   -QxP -fast -Qansi_alias +FDO
 Base tuning for C++ programs: -QxP -fast -GX -GR
 Portability flags:
 176.gcc: -Dalloca=_alloca /F10000000
 186.crafy: -DNT_i386
 253.perlbmk: -DSPEC_CPU2000_NTOS -DPERLDLL /MT
 254.gap: -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO
 Peak tuning:
 164.gzip:     -QxP -fast -Qansi_alias -Oa  +FDO
 175.vpr:      -QxP -fast -Qansi_alias +FDO
 176.gcc:      -QxP -fast -Qansi_alias +FDO
 181.mcf:      -QxP -fast -Qansi_alias +FDO
 186.crafty:   -QxP -fast -Qansi_alias -Oa +FDO
 197.parser:   -QxP -fast -Qansi_alias  +FDO
 252.eon:      -QxP -O2 -Qipo +FDO
 253.perlbmk:  -QxP -fast -Qansi_alias +FDO shlW32M.lib
 254.gap:      -QxP -fast -Qunroll1 -Zp8 +FDO
 255.vortex    basepeak=yes
 256.bzip2:    -fast -Oa -Qunroll1 +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Intel Corporation

Intel D875PBZ motherboard (AA-301) (3.2E GHz, Pentium 4 Processor with Hyper-Threading Technology)

SPECint2000 = SPECint_base2000 =

1420 1363

SPEC license #: 13 Tested by: Intel Corporation Test date: Jan-2004 Hardware Avail: Feb-2004 Software Avail: Dec-2003

Notes/Tuning Information (Continued)

 300.twolf:    -QxP -fast -O3 +FDO shlW32M.lib
 Tested systems can be used with Shin-G ATX case, Delta Inc. power supply PS-300GB-1
 Product description located as of 9/2003:
 http://developer.intel.com/design/motherbd/bz/index.htm
 Motherboard is available through Intel OEM Distribution Channel. See

 http://www.intel.com/cd/channel/reseller/asmo-na/eng/products/box_desktop_boards/p4_boards/p4_dsk_board_d875pbz/index.htm

 The system bus runs at 800 MHz
 shlW32M.lib is the SmartHeap library V6.0 from http://www.microquill.com/smartheap/index.html
 An AGP video card is installed and Hyper-Threading Technologyis enabled