Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

ASUS SK8N Motherboard, AMD Opteron (TM) Model 248

SPECint2000 = SPECint_base2000 =

1452 1338

SPEC license #: 2323 Tested by: PathScale, Inc. Test date: Apr-2004 Hardware Avail: Jan-2004 Software Avail: May-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

164.gzip 1400 108 1295 105 1329

175.vpr 1400 129 1086 126 1109

176.gcc 1100 72.3 1522 72.3 1522

181.mcf 1800 231 779 153 1179

186.crafty 1000 52.8 1894 52.8 1894

197.parser 1800 173 1041 157 1148

252.eon 1300 80.7 1610 74.3 1750

253.perlbmk 1800 119 1511 110 1636

254.gap 1100 87.4 1258 85.8 1282

255.vortex 1900 86.1 2207 80.3 2367

256.bzip2 1500 121 1244 120 1246

300.twolf 3000 251 1195 212 1414

Hardware

CPU: AMD Opteron 248 CPU MHz: 2200 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB (I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 4x512MB, DDR400, PC3200, Corsair, CL2 Disk Subsystem: IDE, 80 GB Other Hardware: None

Software

Operating System: SuSE Linux 9.0 (AMD64) 2.4.21-102-default Compiler: PathScale EKO Compiler Suite, Release 1.0 File System: Linux/ext3 System State: Multi-user, run level 3

Notes/Tuning Information

Tested by PathScale, Inc.

 +FDO: PASS1= -fb_create fbdata  PASS2= -fb_opt fbdata

 Baseline optimization flags:
   C programs:       -O3 -ipa +FDO
   C++ programs:     -Ofast +FDO

 Portability Flags:
   164.gzip: -DNO_STRING_H
   175.vpr: -DSPEC_CPU2000
   181.mcf: -DWANT_STDC_PROTO
   186.crafty: -DLINUX_i386 -DSPEC_CPU2000
   252.eon: -DHAS_ERRLIST -DFMAX_IS_DOUBLE -DSPEC_CPU2000_LP64 -DNDEBUG
   253.perlbmk: -DSPEC_CPU2000_LINUX_I386 -DSPEC_CPU2000_NEED_BOOL
                -DSPEC_CPU2000_GLIBC22 -DSPEC_CPU2000_LP64
   254.gap: -DSYS_IS_USG -DSYS_HAS_IOCTL_PROTO -DSYS_HAS_TIME_PROTO
            -DSYS_HAS_SIGNAL_PROTO  -DSYS_HAS_ANSI -DSYS_HAS_CALLOC_PROTO
            -DSPEC_CPU2000_LP64
   255.vortex: -DSPEC_CPU2000_LP64

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

ASUS SK8N Motherboard, AMD Opteron (TM) Model 248

SPECint2000 = SPECint_base2000 =

1452 1338

SPEC license #: 2323 Tested by: PathScale, Inc. Test date: Apr-2004 Hardware Avail: Jan-2004 Software Avail: May-2004

Notes/Tuning Information (Continued)

   300.twolf: -DSPEC_CPU2000 -DHAVE_SIGNED_CHAR

 Peak Tuning:
 164.gzip: -O3 -ipa -WOPT:val=0 -CG:p2align_freq=10000 +FDO
 175.vpr: -O2 -ipa -OPT:alias=disjoint -LNO:prefetch_ahead=2 -CG:p2align_freq=500000
          -INLINE:aggressive=on -IPA:space=300:plimit=10000:callee_limit=5000:linear=on
          +FDO
 186.crafty: basepeak = true
 181.mcf: -O3 -static -OPT:Ofast -m32 +FDO
 197.parser: -O3 -ipa -m32 -IPA:ctype=on +FDO
 252.eon: -Ofast -CG:gcm=off:p2align_freq=1:prefetch=off
          -OPT:unroll_times_max=16:treeheight=on -TENV:X=4:frame_pointer=off
          -fno-exceptions +FDO
 253.perlbmk: -O3 -ipa -TENV:X=3 +FDO -IPA:min_hotness=5:plimit=20000
 254.gap:  -O3 -ipa +FDO -IPA:min_hotness=7
 255.vortex: -Ofast -LNO:opt=0 -TENV:X=4
     -OPT:goto=off:unroll_analysis=off:unroll_size=0:unroll_times_max=8
     +FDO -IPA:min_hotness=14:space=500:plimit=3600
 256.bzip2: -O3 -ipa -OPT:unroll_times=8:unroll_size=256 +FDO
 300.twolf: -O2 -CG:gcm=off:p2align_freq=100000 -TENV:X=4 +FDO -m32
            -OPT:unroll_times=8:unroll_size=256:alias=disjoint:Ofast

Notes
a) Software availability date: PathScale EKO Compilers generate
   64-bit code by default. The -m32 flag generates 32-bit code and
   is used as a peak flag for some codes above. This -m32 flag will
   be available and supported with PathScale EKO Compilers v1.0 in April,
   but will not be fully documented until May 2004.
b) The tested system can be assembled using an ATX case such as
   the Antec KS-282, a 480W power supply, and a AGP video card.
c) AMIBIOS version 08.00.09