Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

ASUS SK8V Motherboard, AMD Opteron (TM) 150

SPECint2000 = SPECint_base2000 =

1487 1369

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Apr-2004 Hardware Avail: Jun-2004 Software Avail: Apr-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

164.gzip 1400 113 1237 109 1289

175.vpr 1400 120 1168 118 1182

176.gcc 1100 68.0 1616 67.2 1636

181.mcf 1800 268 672 165 1089

186.crafty 1000 47.1 2123 45.6 2191

197.parser 1800 148 1220 137 1311

252.eon 1300 64.3 2023 61.1 2128

253.perlbmk 1800 115 1564 115 1571

254.gap 1100 83.0 1326 83.0 1326

255.vortex 1900 122 1559 113 1687

256.bzip2 1500 117 1277 115 1304

300.twolf 3000 235 1276 195 1535

Hardware

CPU: AMD Opteron (TM) 150 CPU MHz: 2400 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2x512 MB PC3200 DDR SDRAM ECC Reg CL2 Disk Subsystem: IDE, Western Digital WD2000 Other Hardware: None

Software

Operating System: SuSE Linux 8.0 SLES 64 bit (SP3) Compiler: SuSE optional gcc 3.3 compiler (20030312)

(from SLES8 SP3)

File System: Linux/ext3 System State: Multi-user SuSE Run level 3

Notes/Tuning Information

  +FDO: PASS1=-fprofile-arcs PASS2=-fbranch-probabilities
  Portability:
                PORTABILITY=-DSPEC_CPU2000_LP64 is applied to all benchmarks,
                except for peak runs of 181.mcf, 197.parser and 300.twolf, which
                are compiled for 32-bit in peak.
   186.crafty:  CPORTABILITY=-DLINUX_i386
   176.gcc:     Approved src.alt is used
   252.eon:     CXXPORTABILITY=-DHAS_ERRLIST -DFMAX_IS_DOUBLE
                Approved src.alt is used.
   253.perlbmk: CPORTABILITY=-DSPEC_CPU2000_LINUX_I386 -DSPEC_CPU2000_NEED_BOOL
                             -DSPEC_CPU2000_GLIBC22
   254.gap:     CPORTABILITY=-DSYS_IS_USG -DSYS_HAS_IOCTL_PROTO -DSYS_HAS_TIME_PROTO
                             -DSYS_HAS_SIGNAL_PROTO -DSYS_HAS_ANSI -DSYS_HAS_CALLOC_PROTO
  Baseline C:   gcc -O3 -funroll-all-loops +FDO
  Baseline C++: g++ -O3 -funroll-all-loops +FDO
  Peak tuning:
   164.gzip:    -O3 -funroll-all-loops -finline-limit=900 -freduce-all-givs +FDO
   175.vpr:     -O3 -funroll-loops -finline-limit=1000 +FDO
   176.gcc:     -O3 -funroll-all-loops -finline-limit=900 +FDO
   181.mcf:     -O3 -funroll-all-loops -m32 +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

ASUS SK8V Motherboard, AMD Opteron (TM) 150

SPECint2000 = SPECint_base2000 =

1487 1369

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Apr-2004 Hardware Avail: Jun-2004 Software Avail: Apr-2004

Notes/Tuning Information (Continued)

   186.crafty:  -O3 -funroll-loops -fprefetch-loop-arrays
   197.parser:  -O3 -funroll-all-loops -m32 +FDO
   252.eon:     -O3 -funroll-all-loops -ffast-math -finline-limit=3000 +FDO
   253.perlbmk: -O3 -funroll-all-loops -finline-limit=1800 +FDO
   254.gap:     basepeak=true
   255.vortex:  -O3 -funroll-all-loops -finline-limit=1000 +FDO
   256.bzip2:   -O3 -funroll-all-loops -freduce-all-givs -finline-limit=2700 +FDO
   300.twolf:   -O3 -funroll-all-loops -finline-limit=2000 -m32 +FDO
  ONESTEP is used for all base and peak runs
  BIOS rev.: 1001
  Memory used is Corsair CMX512R-3200C2
  Cas Latency manually set to 2.0 in BIOS