Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

CELSIUS V810, Opteron (TM) 250, Linux 64-bit

SPECfp2000 = SPECfp_base2000 =

1689 1652

SPEC license #: 22 Tested by: Fujitsu Siemens Computers Test date: Aug-2004 Hardware Avail: Aug-2004 Software Avail: Jul-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 90.3 1773 72.6 2205

171.swim 3100 129 2400 129 2400

172.mgrid 1800 121 1493 118 1530

173.applu 2100 144 1454 147 1425

177.mesa 1400 78.5 1784 78.9 1775

178.galgel 2900 97.2 2983 87.9 3300

179.art 2600 168 1551 171 1519

183.equake 1300 89.1 1460 87.6 1484

187.facerec 1900 79.2 2398 79.2 2398

188.ammp 2200 157 1402 157 1401

189.lucas 2000 121 1658 122 1645

191.fma3d 2100 132 1595 132 1595

200.sixtrack 1100 149 737 149 737

301.apsi 2600 168 1550 168 1550

Hardware

CPU: AMD Opteron (TM) 250 CPU MHz: 2400 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1, 2 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 4 x 512 MB PC3200 CL3-3-3 DDR SDRAM Disk Subsystem: S-ATA 7200 rpm Other Hardware: None

Software

Operating System: SuSE Linux 9.1 (AMD64) 2.6.4-52-default Compiler: For C and C++ : GNU gcc Compiler

- taken from SuSE’s Linux distribution For Fortran: PGI Fortran 5.2-1 ACML (AMD Core Math Library) for AMD64 - distributed with PGI compiler

File System: Linux/Reiser System State: Multi-user SuSE Run level 3

Notes/Tuning Information

Tested by Fujitsu Siemens Computers
  +FDO: PASS1=-fprofile-arcs PASS2=-fbranch-probabilities
  +ACML is linking with AMD Core Math Library
  pgf90 is the PGI Fortran compiler
  gcc is the GNU compiler, taken from SuSE’s Linux distribution

  Portability:
                    PORTABILITY=-DSPEC_CPU2000_LP64 is applied to all the C benchmarks.
    178.galgel:     -Mfixed

  Baseline: C       gcc   -O3 -funroll-all-loops +FDO
  Baseline: Fortran pgf90 -fastsse  -Mipa=fast

  Peak tuning:
    168.wupwise:    pgf90 -fastsse -Mipa=fast -Minline=levels:2
    171.swim:       basepeak=true
    172.mgrid:      pgf90 -fast -Mipa=fast

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

CELSIUS V810, Opteron (TM) 250, Linux 64-bit

SPECfp2000 = SPECfp_base2000 =

1689 1652

SPEC license #: 22 Tested by: Fujitsu Siemens Computers Test date: Aug-2004 Hardware Avail: Aug-2004 Software Avail: Jul-2004

Notes/Tuning Information (Continued)

    173.applu:      pgf90 -fast -Mipa=fast
    177.mesa:       gcc   -O3 -funroll-all-loops -finline-limit=2000 +FDO
    178.galgel:     pgf90 -fastsse -O3 -mp RM_SOURCES=lapak.f90 +ACML
    179.art:        gcc   -O3 -funroll-all-loops -ffast-math -finline-limit=1500 +FDO
    183.equake:     gcc   -O3 -funroll-all-loops -ffast-math -finline-limit=2000
    187.facerec:    basepeak=true
    188.ammp:       gcc   -O3 -funroll-all-loops -ffast-math -finline-limit=2000 +FDO
    189.lucas:      pgf90 -fastsse -Mipa=fast -Mnosmart
    191.fma3d:      basepeak=true
    200.sixtrack:   basepeak=true
    301.apsi:       basepeak=true

  ONESTEP is used for all base and peak runs

  System tested with only one CPU present.
  BIOS default settings have been used. These include:
  ECC memory checking disabled,
  node interleave disabled, SRAT enabled.

  For information about Fujitsu Siemens Computers in your country please see:
  http://www.fujitsu-siemens.com/countries