Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

MSI K8T Neo2-FIR (MS-6702E) Motherboard, AMD Athlon (TM) 64 FX-53

SPECfp2000 = SPECfp_base2000 =

1634 1595

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Aug-2004 Hardware Avail: Jun-2004 Software Avail: Aug-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 66.6 2402 66.6 2402

171.swim 3100 139 2224 139 2236

172.mgrid 1800 137 1314 137 1314

173.applu 2100 154 1363 154 1363

177.mesa 1400 79.0 1771 74.4 1881

178.galgel 2900 113 2573 107 2702

179.art 2600 137 1905 137 1903

183.equake 1300 82.7 1572 82.7 1572

187.facerec 1900 111 1708 111 1708

188.ammp 2200 177 1241 168 1313

189.lucas 2000 111 1810 104 1927

191.fma3d 2100 157 1339 141 1493

200.sixtrack 1100 151 728 151 728

301.apsi 2600 185 1409 184 1415

Hardware

CPU: AMD Athlon (TM) 64 FX-53 (ADAFX53DEP5AS) CPU MHz: 2400 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2x512 MB PC3200 CL2 Disk Subsystem: SATA, Western Digital WD360 Other Hardware: None

Software

Operating System: Microsoft Windows XP Professional SP1a Compiler: Intel C++ 8.0 build 20040611Z, Intel Fortran 8.0 build 20040519Z,

PGI Fortran compiler 5.2-1 for Windows XP, AMD Core Math library Version 2.0 (ACML), Microsoft Visual Studio .NET 7.0.9466 (libraries), MicroQuill Smartheap Library 7.0

File System: NTFS System State: Default

Notes/Tuning Information

  +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
  +ACML is the AMD Core Math Library V2.0
  ONESTEP is set for all peak runs.
  ifort is the Intel Fortran compiler, icl is the Intel C++ compiler and
  pgf90 is the PGI Fortran compiler.
  Portability:
    178.galgel: -Mfixed
  Baseline: C      : icl   -fast -arch:SSE2 -QaxW +FDO
  Baseline: Fortran: pgf90 -fastsse -Mipa=fast,inline
  Peak tuning:
  168.wupwise:       pgf90 basepeak=yes
  171.swim:          ifort       -O3        -QxW  +FDO
  172.mgrid:         pgf90 basepeak=yes
  173.applu:         pgf90 basepeak=yes
  177.mesa:          icl   -Qipo -arch:SSE2       +FDO -Qunroll1 -Qansi_alias
                           -Qoption,f,-ip_ninl_max_stats=1500,-ip_ninl_max_total_stats=4500
  179.art:           icl   -Qipo            -Zp4  +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

MSI K8T Neo2-FIR (MS-6702E) Motherboard, AMD Athlon (TM) 64 FX-53

SPECfp2000 = SPECfp_base2000 =

1634 1595

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Aug-2004 Hardware Avail: Jun-2004 Software Avail: Aug-2004

Notes/Tuning Information (Continued)

  183.equake:        icl   basepeak=yes
  178.galgel:        pgf90 -fastsse -Mipa=fast,safe -mp RM_SOURCES=lapak.f90 -Munix +ACML
  187.facerec:       pgf90 basepeak=yes
  188.ammp:          icl   -Oa   -arch:SSE2 -Zp4       -Qansi_alias
  189.lucas:         ifort                  -QxW       -Qunroll1
  191.fma3d:         ifort -fast            -QxW  +FDO -Qscalar_rep-
                           -Qoption,f,-ip_ninl_max_stats=1000,-ip_ninl_max_total_stats=3500
  200.sixtrack:      pgf90 basepeak=yes
  301.apsi:          pgf90 -fastsse -Mipa=fast,align
 The tested system can be assembled using an ATX case such as the Antec KS-282,
 a 480W power supply such as the Antec True Power 480, and a PCI or AGP video card.
 BIOS rev. V3.0
 High Performance Settings set to "Optimized" in BIOS
 Memory timings manually set in BIOS:  CAS=2.0, TRCD=2, TRAS=5, TRP=2
 Dynamic Overclocking Disabled in BIOS
 Memory used: Corsair CMX512-3200XLPRO
 Memory configured in dual channel mode