Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company

HP Integrity rx4640-8 (1.5GHz/4MB Itanium 2)

SPECint2000 = SPECint_base2000 =

1372 1372

SPEC license #: 3 Tested by: HP Richardson Test date: Nov-2004 Hardware Avail: Dec-2004 Software Avail: Dec-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

164.gzip 1400 139 1007 139 1007

175.vpr 1400 123 1134 123 1134

176.gcc 1100 65.6 1676 65.6 1676

181.mcf 1800 120 1499 120 1499

186.crafty 1000 81.1 1233 81.1 1233

197.parser 1800 178 1011 178 1011

252.eon 1300 70.6 1841 70.6 1841

253.perlbmk 1800 134 1340 134 1340

254.gap 1100 95.4 1154 95.4 1154

255.vortex 1900 89.8 2116 89.8 2116

256.bzip2 1500 111 1355 111 1355

300.twolf 3000 197 1522 197 1522

Hardware

CPU: Intel Itanium 2 CPU MHz: 1500 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1-4 Parallel: no Primary Cache: 16KBI + 16KBD on chip, per core Secondary Cache: 256KB (I+D) on chip, per core L3 Cache: 4.0MB (I+D) on chip, per core Other Cache: N/A Memory: 32GB (16x2GB DIMMs) Disk Subsystem: 1x36GB 15K SCSI Other Hardware: N/A

Software

Operating System: HPUX11i-TCOE B.11.23.0409 Compiler: HP C/ANSI C Compiler C.06.00 HP aC++ Compiler C.06.00 File System: vxfs System State: Multi-user

Notes/Tuning Information

 Portability Flags
 176.gcc     : -DHOST_WORDS_BIG_ENDIAN
 186.crafty  : -DHP
 252.eon     : -DFMAX_IS_DOUBLE
 253.perlbmk : -DSPEC_CPU2000_HP
 254.gap     : -DSPEC_CPU2000_HP -DSYS_IS_USG -DSYS_HAS_IOCTL_PROTO
               -DSYS_HAS_TIME_PROTO -DSYS_HAS_CALLOC_PROTO

 Base Flags
   all       : +Oprofile=collect:all/+Oprofile=use
   C         : +Ofaster -exec +Otype_safety=ansi
   C++       : +Ofaster +Otype_safety=ansi

 Peak Flags
   same as base (basepeak=true set globally)

 Kernel Tunables:
   dbc_max_pct=20
   dbc_min_pct=20
   maxdsiz=3221225472

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company

HP Integrity rx4640-8 (1.5GHz/4MB Itanium 2)

SPECint2000 = SPECint_base2000 =

1372 1372

SPEC license #: 3 Tested by: HP Richardson Test date: Nov-2004 Hardware Avail: Dec-2004 Software Avail: Dec-2004

Notes/Tuning Information (Continued)

   maxssiz=401604608
   maxdsiz_64bit=4396972761584
   maxssiz_64bit=1073741824
   vps_pagesize=4096
   vps_ceiling=16384

 Notes:

 The system under test had the HP-UX 11i v2 (version 11.23.0409,
   September, 2004) Technical Computing Operating Environment and
   AR1204 compilers installed, along with the following patches:

   PHSS_31849 linker + fdp cumulative patch
   PHSS_31850 assembler patch
   PHSS_31851 Integrity Unwind Library
   PHSS_31852 aC++ Runtime (IA: A.05.60, PA A.03.60)
   PHSS_31853 Math Library Cumulative Patch
   PHSS_31854 milli cumulative patch

 EFI command "cpuconfig" used prior to booting to
   deconfigure other processors if necessary