Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer OpenPower 710 (1650MHz, 1 CPU, Linux)

SPECint2000 = SPECint_base2000 =

1144 1129

SPEC license #: 11 Tested by: IBM Test date: Jan-2005 Hardware Avail: Feb-2005 Software Avail: Mar-2005

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 500 1000 1500 2000

164.gzip 1400 181 774 181 774

175.vpr 1400 141 991 138 1011

176.gcc 1100 80.0 1375 80.0 1375

181.mcf 1800 96.6 1863 95.7 1881

186.crafty 1000 97.2 1029 96.9 1032

197.parser 1800 196 917 196 917

252.eon 1300 109 1192 109 1192

253.perlbmk 1800 222 813 219 823

254.gap 1100 110 1003 108 1022

255.vortex 1900 107 1781 107 1781

256.bzip2 1500 148 1012 138 1086

300.twolf 3000 227 1320 222 1350

Hardware

CPU: POWER5 CPU MHz: 1650 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 2 cores/chip (SMT off) CPU(s) orderable: 1,2 Parallel: No Primary Cache: 64KBI+32KBD (on chip)/core Secondary Cache: 1920KB unified (on chip)/chip L3 Cache: 36MB unified (off chip)/DCM, 1 DCM/SUT Other Cache: None Memory: 8x2 GB Disk Subsystem: 1X73GB SCSI, 15K RPM Other Hardware: None

Software

Operating System: Red Hat Enterprise Linux AS 4 Compiler: XL C/C++ Enterprise Edition Version 7.0 for Linux File System: EXT2 System State: Multi-User, run level 3

Notes/Tuning Information

 Integer Portability Flags:
   gcc:     -DHOST_WORDS_BIG_ENDIAN
   crafty:  -DLINUX_PPC32
   eon:     -DHAS_ERRLIST
    srcalt=fmax_errno
   perlbmk: -DSPEC_CPU2000_LINUX_PPC32 -DSPEC_CPU2000_NEED_BOOL -DHAS_FGETPOS -DHAS_FSETPOS
   gap:     -DSYS_STRING_H -DSYS_IS_USG -DSYS_HAS_IOCTL_PROTO -DSYS_HAS_CALLOC_PROTO
   twolf:   -DHAVE_SIGNED_CHAR
   mcf:     None
   parser:  None
   vortex:  srcalt=closed_files
   bzip2:   None
 Base Optimization Flags:
   C:
    -qpdf1/pdf2
    -O5
   C++:
    -qpdf1/pdf2
    -O5

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer OpenPower 710 (1650MHz, 1 CPU, Linux)

SPECint2000 = SPECint_base2000 =

1144 1129

SPEC license #: 11 Tested by: IBM Test date: Jan-2005 Hardware Avail: Feb-2005 Software Avail: Mar-2005

Notes/Tuning Information (Continued)

 Integer Peak Optimization Flags
 164.gzip
 basepeak=1
 175.vpr:  -qpdf1/qpdf2
  -O5 -qhot=arraypad -Q
 176.gcc
  basepeak=1
 181.mcf
  -O4 -qarch=pwr4 -qtune=pwr4
 186.crafty:  -qpdf1/pdf2
  -O4 -qarch=pwr3 -qtune=pwr3
 197.parser
  basepeak=1
 252.eon:
  basepeak=1
 253.perlbmk:  -qpdf1/pdf2
    -O4 -qarch=pwr5 -qtune=pwr5
 254.gap: -qpdf1/pdf2
  -O5  -qarch=pwr4 -qtune=pwr4
 255.vortex:  -qpdf1/pdf2
  -O4  -qarch=pwr4 -qtune=pwr4
 256.bzip2:
  -O5  -qtune=pwr5 -qarch=pwr5
 300.twolf:
         "C invoked as /opt/ibmcmp/vac/7.0/bin/xlc"
  -O4 -qarch=pwr5 -qtune=pwr5

 SMT: Acronym for "Simultaneous Multi-Threading". A processor technology that allows
      the simultaneous execution of multiple thread contexts within a single processor
      core. (Enabled by default)
 DCM: Acronym for "Dual-Chip Module" (one dual-core processor chip + one L3-cache chip)
 SUT: Acronym for "System Under Test"
 Stack size set to unlimited using "ulimit -s unlimited"
 C:   IBM XL C/C++ for Linux invoked as cc unless explicitly reassigned
 C:   IBM XL C/C++ for Linux invoked as xlc where noted
 C++: IBM XL C/C++ for Linux invoked as xlC
 SMT was disabled at the Linux boot prompt, using the command smt-enabled=off
 Benchmark was run in a 1 CPU partition created using the Hardware Management Console
 cleanpdf used with -qpdf1/pdf2 to erase the information in the PDF directory if any
      exists to ensure no feedback information is reused between compilations.
 Flag file: IBM-20050209-Linux.txt