Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Fujitsu Limited PRIMEPOWER900 (2160MHz)

SPECfp_rate2000 = SPECfp_rate_base2000 = 174 127 SPEC license #: 19 Tested by: Fujitsu Limited Test date: Apr-2005 Hardware Avail: Jun-2005 Software Avail: Apr-2004

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio

1000

2000

3000

4000

168.wupwise 8 172 86.2 8 108 138

171.swim 8 330 87.3 8 98.4 292

172.mgrid 8 217 77.0 8 205 81.4

173.applu 8 302 64.5 8 120 162

177.mesa 8 119 109 8 97.9 133

178.galgel 8 77.9 346 8 52.1 516

179.art 8 12.1 1999 8 11.9 2034

183.equake 8 78.5 154 8 77.5 156

187.facerec 8 147 120 8 79.6 222

188.ammp 8 160 128 8 143 142

189.lucas 8 227 81.8 8 202 92.1

191.fma3d 8 231 84.4 8 231 84.4

200.sixtrack 8 169 60.3 8 158 64.4

301.apsi 8 232 104 8 184 131

Hardware

CPU: SPARC64 V CPU MHz: 2160 FPU: Integrated CPU(s) enabled: 8 cores, 8 chips, 1 core/chip CPU(s) orderable: 1 to 16 (increments of 1) Parallel: None Primary Cache: 128KBI + 128KBD on chip Secondary Cache: 4MB(I+D) on chip L3 Cache: None Other Cache: None Memory: 32768MB Disk Subsystem: 1 x 36.4GB SCSI (10000rpm) Other Hardware: None

Software

Operating System: Solaris 9 4/04 Compiler: (Fortran)_{Fujitsu Parallelnavi 2.3 with patch 913221-03}

Sun Studio 9 Sun Performance Library 9 (C) Sun Studio 9

File System: ufs System State: multi user

Notes/Tuning Information

 FDO: (for Parallelnavi 2.3)
 fdo_pre0=rm -rf ‘pwd‘/*.f.d
 PASS1=-Kpg
 PASS2=-Kpu
 FDO: (for Sun Studio 9)
 fdo_pre0=rm -rf ./feedback.profile ./SunWS_cache
 PASS1=-xprofile=collect:./feedback
 PASS2=-xprofile=use:./feedback

 Floating point base flags:
 (using Fortran compiler of Parallelnavi 2.3)
 -Kfast_GP2=3,prefetch_infer,GREG_SYSTEM -O5
 (using C compiler of Sun Studio 9)
 -fast -xtarget=ultra3 -xipo=2 ONESTEP=yes FDO

 Floating point peak flags:

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Fujitsu Limited PRIMEPOWER900 (2160MHz)

SPECfp_rate2000 = SPECfp_rate_base2000 = 174 127 SPEC license #: 19 Tested by: Fujitsu Limited Test date: Apr-2005 Hardware Avail: Jun-2005 Software Avail: Apr-2004

Notes/Tuning Information (Continued)

 (using Fortran compiler of Parallelnavi 2.3)
 172.mgrid:    -Kfast_GP2=2,GREG_SYSTEM -O4 -Kcommonpad=180,alignc=64
 189.lucas:    -Kfast_GP2=3 -O5 -x dir=./ -Kunroll=2 FDO
 191.fma3d:    -Am -Kfast_GP2=3,GREG_SYSTEM -O4 -x dir=./ -x70 -Kprefetch_infer FDO
 200.sixtrack: -Kfast_GP2=3 -O4 -x dir=./ -Kunroll=3 -fs FDO

 (using Fortran compiler of Sun Studio 9)
 168.wupwise:  -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xipo=1 -Qoption iropt -Ainline:inc=800:cp=1
               ONESTEP=yes FDO
 171.swim:     -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xpad=common:1700 -Qoption iropt -Ainline:cs=700,Atile:skewp:b10
 173.applu:    -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xipo=2 -Qoption cg -Qlp=1-av=192-t=4-fa=1-fl=0
               -Qoption iropt -Aujam:inner=g ONESTEP=yes FDO
 178.galgel:   -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xipo=2 -Qoption iropt -Addint:sf=9 -xlic_lib=sunperf
               RM_SOURCES=lapak.f90 ONESTEP=yes FDO
 187.facerec:  -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xprefetch=latx:1.6 ONESTEP=yes FDO
 301.apsi:     -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xipo=2 ONESTEP=yes FDO

 (using C compiler of Sun Studio 9)
 177.mesa:     -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xchip=ultra2 -xalias_level=strong -xipo=2 -xrestrict
               ONESTEP=yes FDO
 179.art:      -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xipo=2 ONESTEP=yes FDO
 183.equake:   -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xalias_level=strong -W2,-whole -Wc,-Qms_pipe-pref,
               -Qlp=1-av=512-t=6-fa=1-fl=1 ONESTEP=yes FDO
 188.ammp:     -fast -xalias_level=std -xipo=2 ONESTEP=yes FDO

 Portability:
 178.galgel(base):   -Am -Fixed
 178.galgel(peak):   -e -fixed
 187.facerec(base):  -Am
 191.fma3d(base):    -Am

 System Tunables:
 (for /etc/system)
       set consistent_coloring=1
       set tune_t_fsflushr=86400
       set autoup=86400

 Shell Environments:
       Stack size set to unlimited via "ulimit -s unlimited"
       MPSSHEAP=4M
       MPSSSTACK=4M
       LD_PRELOAD=mpss.so.1

 Processes were bound to CPUs using "submit=pbind"

 Extended Interleave Mode enabled.

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Fujitsu Limited PRIMEPOWER900 (2160MHz)

SPECfp_rate2000 = SPECfp_rate_base2000 = 174 127 SPEC license #: 19 Tested by: Fujitsu Limited Test date: Apr-2005 Hardware Avail: Jun-2005 Software Avail: Apr-2004

Notes/Tuning Information (Continued)

 4 CPUs each on 2 system board. Unused CPUs have physically removed.

 Sun Studio 9, posted at URL http://www.sun.com/software/products/studio/previous/9/index.xml
 was used for this submission.