Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

PRIMERGY RX600 S2, 64-bit Intel Xeon MP processor 3.33 GHz

SPECint_rate2000 = SPECint_rate_base2000 =

72.8 72.8

SPEC license #: 22 Tested by: Fujitsu Siemens Computers Test date: Apr-2005 Hardware Avail: Jul-2005 Software Avail: Jan-2005

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 20 40 60 80 100 120 164.gzip 8 197 66.1 8 197 66.1

175.vpr 8 274 47.4 8 274 47.4

176.gcc 8 122 83.4 8 122 83.4

181.mcf 8 273 61.2 8 273 61.2

186.crafty 8 158 58.6 8 158 58.6

197.parser 8 227 73.5 8 227 73.5

252.eon 8 125 96.2 8 125 96.2

253.perlbmk 8 202 82.8 8 202 82.8

254.gap 8 143 71.2 8 143 71.2

255.vortex 8 151 117 8 151 117

256.bzip2 8 215 64.8 8 215 64.8

300.twolf 8 369 75.5 8 369 75.5

Hardware

CPU: 64-bit Intel Xeon MP processor (3.33 GHz, 667 MHz bus) CPU MHz: 3333 FPU: Integrated CPU(s) enabled: 4 cores, 4 chips, 1 core/chip (Hyper-Threading Technology enabled) CPU(s) orderable: 1,2,4 Parallel: No Primary Cache: 12k micro-ops I + 16KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: 8 MB Other Cache: N/A Memory: 16x1024 MB DDRII-RAM PC2-3200R Disk Subsystem: Fujitsu MAS3367NC (SCSI U320 15 krpm) Other Hardware:

Software

Operating System: Windows Server 2003 Enterprise Edition Compiler: Intel C++ Compiler 8.1 Build 20050405Z

Microsoft Visual Studio .Net 2003 7.1.3088 (for libraries) SmartHeap Library Version 6.03a from http://www.microquill.com

File System: NTFS System State: default

Notes/Tuning Information

 GENERAL
 +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use

 Portability flags
    176.gcc:     -Dalloca=_alloca /F10000000
    186.crafy:   -DNT_i386
    252.eon:     Approved srcalt stdcpp is used
    253.perlbmk: -DSPEC_CPU2000_NTOS -DPERLDLL /MT
    254.gap:     -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO

 Base tuning flags
    for C programs:   -fast +FDO shlW32M.lib
    for C++ programs: -fast -Qcxx_features +FDO

 Peak tuning flags
    same as baseline (basepeak=yes set globally)

The system bus runs at 667 MHz

This result was measured with 32-bit binaries using the 32-bit version of

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

PRIMERGY RX600 S2, 64-bit Intel Xeon MP processor 3.33 GHz

SPECint_rate2000 = SPECint_rate_base2000 =

72.8 72.8

SPEC license #: 22 Tested by: Fujitsu Siemens Computers Test date: Apr-2005 Hardware Avail: Jul-2005 Software Avail: Jan-2005

Notes/Tuning Information (Continued)

the operating system.

For information about Fujitsu Siemens Computers in your country please see:
http://www.fujitsu-siemens.com/countries