Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

HITACHI

HITACHI BladeSymphony (1.6GHz/9MB Itanium 2)

SPECint_rate2000 = SPECint_rate_base2000 = -- 137 SPEC license #: 872 Tested by: HITACHI Test date: Jul-2005 Hardware Avail: Aug-2005 Software Avail: Aug-2005

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 50 100 150 200 250 300 164.gzip 8 137 95.1

175.vpr 8 115 113

176.gcc 8 64.3 159

181.mcf 8 66.5 251

186.crafty 8 76.2 122

197.parser 8 159 105

252.eon 8 65.6 184

253.perlbmk 8 126 133

254.gap 8 126 81.0

255.vortex 8 86.1 205

256.bzip2 8 104 134

300.twolf 8 185 151

Hardware

CPU: Intel Itanium 2 CPU MHz: 1600 FPU: Integrated CPU(s) enabled: 8 cores, 8 chips, 1 core/chip CPU(s) orderable: 1,2,4,8 Parallel: No Primary Cache: 16KBI + 16KBD on chip, per core Secondary Cache: 256KB(I+D) on chip, per core L3 Cache: 9.0MB(I+D) on chip, per core Other Cache: N/A Memory: 16GB (1GB DIMM x 16) Disk Subsystem: Fujitsu Ultra320 MAS3735NC (73GBx1), 15000rpm Other Hardware: None

Software

Operating System: HPUX11i-MCOE B.11.23.0409 Compiler: HP C/ANSI C Compiler C.06.00 HP aC++ Compiler C.06.00 File System: vxfs System State: Multi-user run level 3

Notes/Tuning Information

 Base tuning flags
  C         : +Ofaster -exec +Otype_safety=ansi +FDO
  C++       : +Ofaster +Otype_safety=ansi +FDO
 +FDO: PASS1=+Oprofile=collect:all PASS2=+Oprofile=use

 Portability flags
  176.gcc     : -DHOST_WORDS_BIG_ENDIAN
  186.crafty  : -DHP
  252.eon     : -DFMAX_IS_DOUBLE
  253.perlbmk : -DSPEC_CPU2000_HP
  254.gap     : -DSPEC_CPU2000_HP -DSYS_IS_USG -DSYS_HAS_IOCTL_PROTO
                -DSYS_HAS_TIME_PROTO -DSYS_HAS_CALLOC_PROTO

 Kernel Parameters
  dbc_max_pct = 20
  dbc_min_pct = 20
  maxdsiz = 0x7b03a000
  maxdsiz_64bit = 0x4000000000
  maxssiz = 0x10000000
  maxssiz_64bit = 0x40000000

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

HITACHI

HITACHI BladeSymphony (1.6GHz/9MB Itanium 2)

SPECint_rate2000 = SPECint_rate_base2000 = -- 137 SPEC license #: 872 Tested by: HITACHI Test date: Jul-2005 Hardware Avail: Aug-2005 Software Avail: Aug-2005

Notes/Tuning Information (Continued)

  swapmem_on = 0
  vps_ceiling = 16384
  vps_pagesize = 4096

 Following patches were installed.
  PHCO_32622 LVM commands patch
  PHCO_32784 VxVM 3.5~IA.014 Command Patch 01
  PHKL_32095 11.23 LVM Cumulative Patch; OLdR enablement
  PHKL_32233 Hang during dump after a main memory MCA
  PHKL_32247 VxVM 3.5~IA.014 Kernel Cumulative Patch 01
  PHKL_32359 Prevents loss of dump on some Itanium MCA’s
  PHKL_32425 VM pagecache leaks on I/O errors
  PHKL_32518 FSS
  PHKL_33046 Claim devices on Hitachi BladeSymphony
  PHNE_31118 IETHER 1000Base-SX/T B.11.23.[01-0505] patch
  PHSS_31850 assembler patch
  PHSS_31851 Integrity Unwind Library
  PHSS_31852 aC++ Runtime (IA: A.05.60, PA A.03.60)
  PHSS_31853 Math Library Cumulative Patch
  PHSS_31854 milli cumulative patch
  PHSS_32502 Aries cumulative patch
  PHSS_32765 linker + fdp cumulative patch