LAMMPS WWW Site - LAMMPS Documentation - LAMMPS Commands

### kspace_modify command

Syntax:

    kspace_modify keyword value ...

- one or more keyword/value pairs may be listed
- keyword = mesh or order or order/disp or overlap or minorder or force or gewald or gewald/disp or slab or (nozforce or compute or cutoff/adjust or diff

        mesh value = x y z
          x,y,z = grid size in each dimension for long-range Coulombics
        mesh/disp value = x y z
          x,y,z = grid size in each dimension for 1/r^6 dispersion
        order value = N
          N = extent of Gaussian for PPPM or MSM mapping of charge to grid
        order/disp value = N
          N = extent of Gaussian for PPPM mapping of dispersion term to grid
        overlap = yes or no = whether the grid stencil for PPPM is allowed to overlap into more than the nearest-neighbor processor
        minorder value = M
          M = min allowed extent of Gaussian when auto-adjusting to minimize grid communication
        force value = accuracy (force units)
        gewald value = rinv (1/distance units)
          rinv = G-ewald parameter for Coulombics
        gewald/disp value = rinv (1/distance units)
          rinv = G-ewald parameter for dispersion
        slab value = volfactor or nozforce
          volfactor = ratio of the total extended volume used in the
            2d approximation compared with the volume of the simulation domain
        nozforce turns off kspace forces in the z direction
        compute value = yes or no
        cutoff/adjust value = yes or no
        fftbench value = yes or no
        diff value = ad or ik = 2 or 4 FFTs for PPPM in smoothed or non-smoothed mode

Examples:

    kspace_modify mesh 24 24 30 order 6
    kspace_modify slab 3.0

Description:

Set parameters used by the kspace solvers defined by the kspace_style command. Not all parameters are relevant to all kspace styles.

The mesh keyword sets the grid size for kspace style pppm or msm. In the case of PPPM, this is the FFT mesh, and each dimension must be factorizable into powers of 2, 3, and 5. In the case of MSM, this is the finest scale real-space mesh, and each dimension must be factorizable into powers of 2. When this option is not set, the PPPM or MSM solver chooses its own grid size, consistent with the user-specified accuracy and pairwise cutoff. Values for x,y,z of 0,0,0 unset the option.

The mesh/disp keyword sets the grid size for kspace style pppm/disp. This is the FFT mesh for long-range dispersion and ach dimension must be factorizable into powers of 2, 3, and 5. When this option is not set, the PPPM solver chooses its own grid size, consistent with the user-specified accuracy and pairwise cutoff. Values for x,y,z of 0,0,0 unset the option.

The order keyword determines how many grid spacings an atom's charge extends when it is mapped to the grid in kspace style pppm or msm. The default for this parameter is 5 for PPPM and 8 for MSM, which means each charge spans 5 or 4 grid cells in each dimension, respectively. For the LAMMPS implementation of MSM, the order can range from 4 to 10 and must be even. For PPPM, the minimum allowed setting is 2 and the maximum allowed setting is 7. The larger the value of this parameter, the smaller that LAMMPS will set the grid size, to achieve the requested accuracy. Conversely, the smaller the order value, the larger the grid size will be. Note that there is an inherent trade-off involved: a small grid will lower the cost of FFTs or MSM direct sum, but a larger order parameter will increase the cost of interpolating charge/fields to/from the grid.

The order/disp keyword determines how many grid spacings an atom's dispersion term extends when it is mapped to the grid in kspace style pppm/disp. It has the same meaning as the order setting for Coulombics.

The overlap keyword can be used in conjunction with the minorder keyword with the PPPM styles to adjust the amount of communication that occurs when values on the FFT grid are exchangeed between processors. This communication is distinct from the communication inherent in the parallel FFTs themselves, and is required because processors interpolate charge and field values using grid point values owned by neighboring processors (i.e. ghost point communication). If the overlap keyword is set to yes then this communication is allowed to extend beyond nearest-neighbor processors, e.g. when using lots of processors on a small problem. If it is set to no then the communication will be limited to nearest-neighbor processors and the order setting will be reduced if necessary, as explained by the minorder keyword discussion. The overlap keyword is always set to yes in MSM.

The minorder keyword allows LAMMPS to reduce the order setting if necessary to keep the communication of ghost grid point limited to exchanges between nearest-neighbor processors. See the discussion of the overlap keyword for details. If the overlap keyword is set to yes, which is the default, this is never needed. If it set to no and overlap occurs, then LAMMPS will reduce the order setting, one step at a time, until the ghost grid overlap only extends to nearest neighbor processors. The minorder keyword limits how small the order setting can become. The minimum allowed value for PPPM is 2, which is the default. If minorder is set to the same value as order then no reduction is allowed, and LAMMPS will generate an error if the grid communcation is non-nearest-neighbor and overlap is set to no. The minorder keyword is not currently supported in MSM.

The PPPM order parameter may be reset by LAMMPS when it sets up the FFT grid if the implied grid stencil extends beyond the grid cells owned by neighboring processors. Typically this will only occur when small problems are run on large numbers of processors. A warning will be generated indicating the order parameter is being reduced to allow LAMMPS to run the problem. Automatic adjustment of the order parameter is not supported in MSM.

The force keyword overrides the relative accuracy parameter set by the kspace_style command with an absolute accuracy. The accuracy determines the RMS error in per-atom forces calculated by the long-range solver and is thus specified in force units. A negative value for the accuracy setting means to use the relative accuracy parameter. The accuracy setting is used in conjunction with the pairwise cutoff to determine the number of K-space vectors for style ewald, the FFT grid size for style pppm, or the real space grid size for style msm.

The gewald keyword sets the value of the Ewald or PPPM G-ewald parameter for charge as rinv in reciprocal distance units. Without this setting, LAMMPS chooses the parameter automatically as a function of cutoff, precision, grid spacing, etc. This means it can vary from one simulation to the next which may not be desirable for matching a KSpace solver to a pre-tabulated pairwise potential. This setting can also be useful if Ewald or PPPM fails to choose a good grid spacing and G-ewald parameter automatically. If the value is set to 0.0, LAMMPS will choose the G-ewald parameter automatically. MSM does not use the gewald parameter.

The gewald/disp keyword sets the value of the Ewald or PPPM G-ewald parameter for dispersion as rinv in reciprocal distance units. It has the same meaning as the gewald setting for Coulombics.

The slab keyword allows an Ewald or PPPM solver to be used for a systems that are periodic in x,y but non-periodic in z - a boundary setting of "boundary p p f". This is done by treating the system as if it were periodic in z, but inserting empty volume between atom slabs and removing dipole inter-slab interactions so that slab-slab interactions are effectively turned off. The volfactor value sets the ratio of the extended dimension in z divided by the actual dimension in z. The recommended value is 3.0. A larger value is inefficient; a smaller value introduces unwanted slab-slab interactions. The use of fixed boundaries in z means that the user must prevent particle migration beyond the initial z-bounds, typically by providing a wall-style fix. The methodology behind the slab option is explained in the paper by (Yeh). An alternative slab option can be invoked with the nozforce keyword in lieu of the volfactor. This turns off all kspace forces in the z direction. The nozforce option is not supported by MSM. For MSM, any combination of periodic, non-periodic, or shrink-wrapped boundaries can be set using boundary (the slab approximation in not needed).

The compute keyword allows Kspace computations to be turned off, even though a kspace_style is defined. This is not useful for running a real simulation, but can be useful for debugging purposes or for computing only partial forces that do not include the Kspace contribution. You can also do this by simply not defining a kspace_style, but a Kspace-compatible pair_style requires a kspace style to be defined. This keyword gives you that option.

The cutoff/adjust keyword applies only to MSM. If this option is turned on, the Coulombic cutoff will be automatically adjusted at the beginning of the run to give the desired estimated error. Other cutoffs such as LJ will not be affected. If the grid is not set using the mesh command, this command will also attempt to use the optimal grid that minimizes cost using an estimate given by (Hardy). Note that this cost estimate is not exact, somewhat experimental, and still may not yield the optimal parameters.

The fftbench keyword applies only to PPPM. It is on by default. If this option is turned off, LAMMPS will not take the time at the end of a run to give FFT benchmark timings, and will finish a few seconds faster than it would if this option were on.

The diff keyword specifies the differentiation scheme used by the PPPM method to compute forces on particles given electrostatic potentials on the PPPM mesh. The ik approach is the default for PPPM and is the original formulation used in (Hockney). It performs differentiation in Kspace, and uses 3 FFTs to transfer each component of the computed fields back to real space for total of 4 FFTs per timestep.

The analytic differentiation ad approach uses only 1 FFT to transfer information back to real space for a total of 2 FFTs per timestep. It then performs analytic differentiation on the single quantity to generate the 3 components of the electric field at each grid point. This is sometimes referred to as "smoothed" PPPM. This approach requires a somewhat larger PPPM mesh to achieve the same accuracy as the ik method. The ad method is always used for MSM.

IMPORTANT NOTE: Currently, not all PPPM styles support the ad option. Support for those PPPM variants will be added later.

Restrictions: none

Related commands:

kspace_style, boundary

Default:

The option defaults are mesh = mesh/disp = 0 0 0, order = order/disp = 5 (PPPM), order = 8 (MSM), minorder = 2, overlap = yes, force = -1.0, gewald = gewald/disp = 0.0, slab = 1.0, compute = yes, cutoff/adjust = yes (MSM), fftbench = yes (PPPM), and diff = ik (PPPM).

(Hockney) Hockney and Eastwood, Computer Simulation Using Particles, Adam Hilger, NY (1989).

(Yeh) Yeh and Berkowitz, J Chem Phys, 111, 3155 (1999).

(Hardy) David Hardy thesis: Multilevel Summation for the Fast Evaluation of Forces for the Simulation of Biomolecules, University of Illinois at Urbana-Champaign, (2006).