Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Compaq Computer Corporation

DIGITAL Personal Workstation 500au

SPECfp2000 = SPECfp_base2000 = -- 158 SPEC license #: 2 Tested by: Compaq NH Test date: Nov-1999 Hardware Avail: May-1997 Software Avail: Feb-2000

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 50 100 150 200 250

168.wupwise 1600 963 166

171.swim 3100 1611 192

172.mgrid 1800 1389 130

173.applu 2100 1967 107

177.mesa 1400 719 195

178.galgel 2900 1784 163

179.art 2600 1268 205

183.equake 1300 1203 108

187.facerec 1900 1065 178

188.ammp 2200 1587 139

189.lucas 2000 954 210

191.fma3d 2100 1356 155

200.sixtrack 1100 803 137

301.apsi 2600 1477 176

Hardware

CPU: Alpha 21164 CPU MHz: 500 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 8KB(I)+8KB(D) on chip Secondary Cache: 96KB on chip L3 Cache: 2MB off chip Other Cache: None Memory: 384MB Disk Subsystem: 2x2GB Other Hardware: Ethernet

Software

Operating System: Tru64 UNIX V4.0F Compiler: Compaq C X6.2-259-449AT Compaq Fortran T5.3 (ft2) KAP Fortran V4.2 File System: ufs System State: Multi-user

Notes/Tuning Information

 Baseline       C: ONESTEP cc   -arch ev56 -fast -O4
          Fortran: ONESTEP kf90 -arch ev56 -O5 -fkapargs=’-ur=-1’

 Portability: galgel: -fixed
 The C compiler used here will be available to customers as V6.3
 at http://www.unix.digital.com/dtk/ .  It will be available as an
 ADK (Advanced Developers’ Kit) in February, 2000 and as the final
 version in July, 2000.