Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Intel Corporation

Intel VC820(1 GHz Pentium III processor)

SPECfp2000 = SPECfp_base2000 = 314 304 SPEC license #: 13 Tested by: Intel Corporation Test date: Jun-2000 Hardware Avail: Mar-2000 Software Avail: Oct-2000

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 100 200 300 400 500 600

168.wupwise 1600 400 400 400 400

171.swim 3100 760 408 759 408

172.mgrid 1800 725 248 652 276

173.applu 2100 846 248 840 250

177.mesa 1400 275 508 275 510

178.galgel 2900 994 292 888 327

179.art 2600 691 376 691 376

183.equake 1300 559 232 465 279

187.facerec 1900 634 300 633 300

188.ammp 2200 773 285 755 292

189.lucas 2000 657 304 661 303

191.fma3d 2100 754 278 754 278

200.sixtrack 1100 628 175 633 174

301.apsi 2600 758 343 732 355

Hardware

CPU: Pentium III processor (1 GHz, 133 MHz bus) CPU MHz: 1000 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 16KBI + 16KBD on-die Secondary Cache: 256KB(I+D) on-die ECC L3 Cache: N/A Other Cache: N/A Memory: 256 MB PC800 RDRAM Disk Subsystem: IBM DTLA 307030 ATA-66+ Other Hardware: Creative Labs Annihalator Pro GeForce 256 DDR

Software

Operating System: Windows 2000(Build 2195) Compiler: Intel C++ and Fortran Compiler 5.0, for Windows NT 4.0/Windows 2000 Microsoft Visual C++ 6.0 (for libraries), SmartHeap library V5.0 File System: FAT32 System State: Default

Notes/Tuning Information

 +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
 Base tuning: -QxK -Qipo_wp -O3 +FDO
 Portability:
 178.galgel: -FI -Fe$@ -link -stack:32000000
 Peak tuning:
 168.wupwise: -QxK -Qipo_wp -O3 +FDO
 171.swim:    -QxK -Qipo_wp -O3 +FDO
 172.mgrid:   -QxK -Qipo_wp -O3 +FDO
 173.applu:   -QxK -Qipo_wp -O3 +FDO
 177.mesa:    -QxK -Qipo_wp -O3 -Oa +FDO
 178.galgel:  -QxK -Qipo_wp -O3 +FDO -Zi shlW32M.lib
 179.art:     -QxK -Qipo_wp -O3 -Oa +FDO
 183.equake:  -QxK -Qipo_wp -Qrcd -Oa +FDO shlW32M.lib
 187.facerec: -QxK -Qipo_wp -O3 +FDO -Zi shlW32M.lib
 188.ammp:    -QxK -Qipo_wp -O3 -Oa +FDO
 189.lucas:   -QxK -Qipo_wp -O3 +FDO -Zi shlW32M.lib
 191.fma3d:   -QxK -Qipo_wp -O3 +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Intel Corporation

Intel VC820(1 GHz Pentium III processor)

SPECfp2000 = SPECfp_base2000 = 314 304 SPEC license #: 13 Tested by: Intel Corporation Test date: Jun-2000 Hardware Avail: Mar-2000 Software Avail: Oct-2000

Notes/Tuning Information (Continued)

 200.sixtrack:-QxK -Qipo_wp +FDO
 301.apsi:    -QxK -Qipo_wp +FDO
 Tested systems can be used with Shin-G ATX case, Sparkle Inc. power supply
 Product description as of 06/2000:
 http://developer.intel.com/design/motherbd/vc/
 Motherboard available through Intel OEM Distribution channel. See
 http://channel.intel.com/ for more information
The system bus runs at 133 MHz