Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer pSeries 620 Model 6F1 (668MHz,8MB L2)

SPECfp_rate2000 = SPECfp_rate_base2000 =

17.3 16.9

SPEC license #: 11 Tested by: IBM, Austin, TX Test date: Mar-2001 Hardware Avail: Apr-2001 Software Avail: Apr-2001

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 10 20 30 40 50 60 70 168.wupwise 6 454 24.5 6 446 25.0

171.swim 6 2050 10.5 6 2025 10.7

172.mgrid 6 1326 9.45 6 1244 10.1

173.applu 6 1576 9.28 6 1550 9.43

177.mesa 6 547 17.8 6 534 18.3

178.galgel 6 472 42.7 6 452 44.6

179.art 6 278 65.2 6 282 64.1

183.equake 6 769 11.8 6 765 11.8

187.facerec 6 586 22.6 6 582 22.7

188.ammp 6 651 23.5 6 613 25.0

189.lucas 6 1370 10.2 6 1363 10.2

191.fma3d 6 1184 12.3 6 1162 12.6

200.sixtrack 6 866 8.84 6 865 8.85

301.apsi 6 885 20.5 6 883 20.5

Hardware

CPU: RS64 IV CPU MHz: 668 FPU: Integrated CPU(s) enabled: 6 cores, 6 chips, 1 core/chip CPU(s) orderable: 6 Parallel: No Primary Cache: 128KBI+128KBD (on chip) Secondary Cache: 8MB unified (off chip) L3 Cache: None Other Cache: None Memory: 4GB Disk Subsystem: 2x9.1GB SCSI Other Hardware: Ethernet

Software

Operating System: AIX 4.3.3 Compiler: Fortran 77 and 90: IBM xl Fortran 7.1 invoked

as ’xlf90’; C: IBM VAC++ 5.0.1 invoked as ’xlc’

File System: AIX/JFS System State: Multi-user

Notes/Tuning Information

 Portability Flags
   -qfixed used in: wupwise, swim, mgrid, applu, galgel, sixtrack, apsi
   -qsuffix=f=f90 used in: galgel, facerec, lucas, fma3d
 Base Flags:
   Fortran: -O5 -lmass
   C: -O5 -lmass
 Peak Flags:
    168.wupwise: -qpdf1/pdf2 -O4 -qipa=level=2 -lmass, fdpr -v -R3
    171.swim:    -qpdf1/pdf2 -O4 -qipa=level=2 -lmass -qhot, fdpr -v -R3
    172.mgrid:   -O4 -qarch=pwr3
    173.applu:   -O3
    177.mesa:    -qpdf1/pdf2 -O3 -qarch=rs64c    -L/usr/vac/lib, fdpr -v -R3
    178.galgel:  -qpdf1/pdf2 -O3 -lmass, fdpr -v -R3
    179.art:     -O5 -lmass
    183.equake:  -O5 -lmass
    187.facerec: -O5 -lmass
    188.ammp:    -qpdf1/pdf2 -O3 -lhmu -lmass  -L/usr/vac/lib, fdpr -v -R3

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer pSeries 620 Model 6F1 (668MHz,8MB L2)

SPECfp_rate2000 = SPECfp_rate_base2000 =

17.3 16.9

SPEC license #: 11 Tested by: IBM, Austin, TX Test date: Mar-2001 Hardware Avail: Apr-2001 Software Avail: Apr-2001

Notes/Tuning Information (Continued)

    189.lucas:   -qpdf1/pdf2 -O3 -qarch=rs64b -lmass, fdpr -v -R3
    191.fma3d:   -qpdf1/pdf2 -O3 -lmass
    200.sixtrack:-O3  -qarch=rs64c
    301.apsi:    -O5 -lmass
    Tests were run with APAR IY 17356 applied to AIX 4.3.3 to enable new hardware support.
    fdpr: Feedback directed program restructuring tool