Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell Dell PowerEdge 7150

SPECfp2000 = SPECfp_base2000 = -- 710 SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: May-2001 Hardware Avail: Jul-2001 Software Avail: Jun-2001

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 270 593

171.swim 3100 225 1376

172.mgrid 1800 238 757

173.applu 2100 205 1025

177.mesa 1400 424 330

178.galgel 2900 283 1024

179.art 2600 101 2584

183.equake 1300 156 836

187.facerec 1900 294 645

188.ammp 2200 429 512

189.lucas 2000 238 840

191.fma3d 2100 648 324

200.sixtrack 1100 191 576

301.apsi 2600 751 346

Hardware

CPU: Itanium processor (800 MHz) CPU MHz: 800 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1,2,4 Parallel: No Primary Cache: 16KBI + 16KBD on chip Secondary Cache: 96KB(I+D) on chip L3 Cache: 4MB(I+D) off chip per CPU Other Cache: N/A Memory: 16 GB (64 x 256MB PC100 SDRAM) Disk Subsystem: Seagate Ultra-2 SCSI Other Hardware:

Software

Operating System: Windows XP Advanced Server, 64-bit Edition (build 2479) Compiler: Intel C++ and Fortran Compiler 5.0.1 Build 20010507

Microsoft Platform SDK (2462)

File System: NTFS System State: Default

Notes/Tuning Information

 FEEDBACK-DIRECTED OPTIMIZATION
   +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
 BASE TUNING
   C:       -Qipo -O3 +FDO
   F77/F90: -Qipo -O3 -Qftz +FDO
 PORTABILITY
   178.galgel: -FI