Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire 6800

SPECfp2000 = SPECfp_base2000 = -- 278 SPEC license #: 597 Tested by: Verlag Heinz Heise (iX) Test date: May-2001 Hardware Avail: Mar-2001 Software Avail: May-2001

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 200 400 600 800

168.wupwise 1600 522 306

171.swim 3100 1446 214

172.mgrid 1800 1119 161

173.applu 2100 1445 145

177.mesa 1400 350 400

178.galgel 2900 384 754

179.art 2600 355 733

183.equake 1300 922 141

187.facerec 1900 324 587

188.ammp 2200 819 269

189.lucas 2000 1270 157

191.fma3d 2100 1011 208

200.sixtrack 1100 407 270

301.apsi 2600 1067 244

Hardware

CPU: UltraSPARC-III CPU MHz: 750 FPU: Integrated CPU(s) enabled: 24 cores, 24 chips, 1 core/chip CPU(s) orderable: 2-24 Parallel: No Primary Cache: 32KBI+64KBD on chip Secondary Cache: 8MB(I+D) off chip L3 Cache: None Other Cache: None Memory: 48GB Disk Subsystem: 8x36GB (RAID 10)

Other Hardware:

Software

Operating System: Solaris 8 Compiler: Forte Developer 6 update 2 C 5.3 File System: UFS System State: Multi User

Notes/Tuning Information

 Portability: 178.galgel: -e -fixed

 C   flags: -fast -xcrossfile -xprofile
 F90 flags: -fast -xcrossfile -xprofile