Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer pSeries 610 Mod 6E1 333MHz

SPECint_rate2000 = SPECint_rate_base2000 =

5.57 5.21

SPEC license #: 11 Tested by: IBM Corp. Test date: Jan-2002 Hardware Avail: Feb-2002 Software Avail: Feb-2002

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 1 2 3 4 5 6 7 8 9 164.gzip 2 718 4.53 2 705 4.61

175.vpr 2 630 5.15 2 623 5.21

176.gcc 2 446 5.72 2 446 5.72

181.mcf 2 609 6.85 2 609 6.85

186.crafty 2 489 4.74 2 379 6.12

197.parser 2 1238 3.37 2 1125 3.71

252.eon 2 444 6.79 2 441 6.83

253.perlbmk 2 1065 3.92 2 923 4.52

254.gap 2 532 4.80 2 531 4.81

255.vortex 2 873 5.05 2 690 6.39

256.bzip2 2 662 5.26 2 641 5.43

300.twolf 2 872 7.98 2 851 8.17

Hardware

CPU: POWER3-II CPU MHz: 333 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1,2 Parallel: No Primary Cache: 32KBI+64KBD (on chip) Secondary Cache: 4MB unified (off chip) L3 Cache: None Other Cache: None Memory: 2GB Disk Subsystem: 2x18GB 10000RPM Other Hardware: None

Software

Operating System: AIX 5L V5.1 Compiler: IBM VisualAge C++ for AIX, Version 5.0.2.1 File System: AIX/JFS System State: Multi-user

Notes/Tuning Information

 Portability Flags:
   gcc:     -ma -qlanglvl=ansi -DHOST_WORDS_BIG_ENDIAN
   crafty:  -DAIX
   eon:     -DNEED_EXPLICIT_SPECIALIZATION
             EXTRA_LDFLAGS=-I. -DNDEBUG
   perlbmk: -DSPEC_CPU2000_AIX
   gap:     -DSYS_IS_BSD -DSYS_STRING_H -DSYS_HAS_TIME_PROTO
            -DSYS_HAS_MALLOC_PROTO -DSYS_HAS_CALLOC_PROTO
   twolf:   -DHAVE_SIGNED_CHAR
 Base Optimization Flags:
   C:           -O4 -lmass
   C++:         -O4 -lmass
 Peak Optimization Flags
   164.gzip:    -O4 -lhmu, fdpr -v -R3 -p -x
   175.vpr:     -O5 -qunroll=8
   176.gcc:     (basepeak=1)
   181.mcf:     (basepeak=1)
   186.crafty:  -O3 -lhmu -q64
   197.parser:  -qpdf1/pdf2 -O4 -lpdf
                -bnso -bI:/lib/syscalls.exp, fdpr -v -R3  -p -x

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer pSeries 610 Mod 6E1 333MHz

SPECint_rate2000 = SPECint_rate_base2000 =

5.57 5.21

SPEC license #: 11 Tested by: IBM Corp. Test date: Jan-2002 Hardware Avail: Feb-2002 Software Avail: Feb-2002

Notes/Tuning Information (Continued)

   252.eon:     -O4 -lmass, fdpr -v -R3 -p -x
   253.perlbmk: -qpdf1/pdf2 -O3 -lhmu -lpdf -qarch=pwr3
                -qdatalocal -qunroll=8, fdpr -R3 -p -x
   254.gap:     -O4 -qarch=pwr3, fdpr -v -R3 -p -x
   255.vortex:  -O3 -lhmu -lmass -qipa=partition=large,
                fdpr -v -R3 -p -x
   256.bzip2:   -O5 -qunroll=8
   300.twolf:   -qpdf1/pdf2 -O5 -lpdf, fdpr -v -R3 -p -x
                 CC=/usr/vac/bin/xlc
 fpdr: Feedback directed program restructuring tool
 APAR IY22854 was applied to AIX 5L V5.1 to enable new hardware support
 ulimits set to unlimited.
 C: IBM VAC++ 5.0.2.1 invoked as cc except where noted as xlc
 C++: IBM VAC++ 5.0.2.1 invoked as xlC