Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

Asus A7M266-D Motherboard, AMD Athlon (TM) MP 2000+

SPECfp_rate2000 = SPECfp_rate_base2000 =

6.91 6.35

SPEC license #: 49 Tested by: AMD Austin TX Test date: Feb-2002 Hardware Avail: Jan-2002 Software Avail: Feb-2002

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 2 4 6 8 10 12 168.wupwise 1 198 9.36 1 198 9.39

171.swim 1 374 9.62 1 366 9.82

172.mgrid 1 347 6.01 1 337 6.19

173.applu 1 435 5.61 1 426 5.72

177.mesa 1 158 10.3 1 157 10.3

178.galgel 1 593 5.68 1 330 10.2

179.art 1 663 4.55 1 629 4.80

183.equake 1 268 5.63 1 224 6.73

187.facerec 1 307 7.17 1 306 7.19

188.ammp 1 559 4.56 1 519 4.92

189.lucas 1 350 6.63 1 346 6.70

191.fma3d 1 343 7.09 1 342 7.13

200.sixtrack 1 262 4.87 1 255 5.00

301.apsi 1 590 5.12 1 502 6.01

Hardware

CPU: AMD Athlon (TM) MP 2000+ CPU MHz: 1667 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1, 2 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 256KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2x256MB PC2100 DDR SDRAM CL2 Disk Subsystem: Seagate ST318451LW Other Hardware: None

Software

Operating System: Windows 2000 SP2 Compiler: Intel C++ 5.0.1 build 020125Z

Intel Fortran 5.0.1 build 020125Z and Compaq Visual Fortran 6.6 Microsoft Visual Studio 6.0 SP5 (libraries) MicroQuill Smartheap Library 5.0

File System: FAT32 System State: Default

Notes/Tuning Information

  +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
  icl and ifl are the Intel C++ and Fortran compilers
  f90 is the Compaq Fortran compiler
  shlW32M.lib is the SmartHeap library V5.0 from MicroQuill www.microquill.com
  Portability:
  178.galgel: -FI -Fe$@ -link -stack:32000000
  Baseline: C       icl -QxK -Qipo +FDO shlW32M.lib
  Baseline: Fortran ifl -O3 -QxK -Qipo +FDO
  Peak tuning:
  168.wupwise:  ifl -O3 -QxK -Qwp_ipo +FDO
  171.swim:     ifl -O3 -QxK -Qwp_ipo +FDO
  172.mgrid:    ifl -O3 -QxK -Qwp_ipo +FDO
  173.applu:    ifl -O3 -QxK -Qwp_ipo -Qscalar_rep- -Qauto +FDO
  177.mesa:     icl -O3 -QxK -Qwp_ipo -Oa +FDO shlw32M.lib
  178.galgel:   f90 -Optimize:5 -fast
  179.art:      icl -O3 -QxK -QaxW -Qwp_ipo -Oa +FDO shlW32M.lib
  183.equake:   icl -O3 -QxK -Qwp_ipo -Qrcd -Oa +FDO shlW32M.lib

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

Asus A7M266-D Motherboard, AMD Athlon (TM) MP 2000+

SPECfp_rate2000 = SPECfp_rate_base2000 =

6.91 6.35

SPEC license #: 49 Tested by: AMD Austin TX Test date: Feb-2002 Hardware Avail: Jan-2002 Software Avail: Feb-2002

Notes/Tuning Information (Continued)

  187.facerec:  ifl -O3 -QxK -Qipo +FDO
  188.ammp:     icl -O3 -QxK -Qwp_ipo -Oa +FDO
  189.lucas:    ifl -O3 -QxK -Qwp_ipo +FDO shlW32M.lib
  191.fma3d:    ifl -O3 -QxK -Qwp_ipo +FDO
  200.sixtrack: ifl -QxK -QaxW -Qwp_ipo -Qprefetch +FDO
  301.apsi:     f90 -Optimize:5 -fast
  Library ordering for 189.lucas (to include SmartHeap correctly with default libs):
  LIBS=libIEPCF90.lib libintrins.lib libF90.lib
  libqwind.lib libm.lib shlW32M.lib LIBC.lib libirc.lib OLDNAMES.lib
  ONESTEP is used for all base and peak runs
 The tested system can be assembled using an ATX case such as the Antec KS-282,
 a 420W power supply such as the NSpire MSP-420P4B, and a PCI or AGP video card.
 The System bus runs at 266MHz