Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company

hp server rx5670 (1000 MHz, Itanium 2)

SPECfp_rate2000 = SPECfp_rate_base2000 =

30.7 30.7

SPEC license #: 3 Tested by: HP Richardson Test date: Nov-2002 Hardware Avail: Sep-2002 Software Avail: Nov-2002

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 20 40 60 80 100 120 168.wupwise 2 160 23.2 2 160 23.2

171.swim 2 135 53.1 2 135 53.1

172.mgrid 2 123 34.0 2 123 34.0

173.applu 2 99.0 49.2 2 99.0 49.2

177.mesa 2 193 16.8 2 193 16.8

178.galgel 2 114 58.8 2 114 58.8

179.art 2 58.6 103 2 58.6 103

183.equake 2 80.6 37.4 2 80.6 37.4

187.facerec 2 161 27.3 2 161 27.3

188.ammp 2 244 20.9 2 244 20.9

189.lucas 2 171 27.2 2 171 27.2

191.fma3d 2 290 16.8 2 290 16.8

200.sixtrack 2 122 20.9 2 122 20.9

301.apsi 2 392 15.4 2 392 15.4

Hardware

CPU: Intel Itanium 2 CPU MHz: 1000 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1-4 Parallel: no Primary Cache: 16KBI + 16KBD (on chip) per CPU Secondary Cache: 256KB (on chip) per CPU L3 Cache: 3.0MB (on chip) per CPU Other Cache: N/A Memory: 12GB (48 * 256MB DIMMs - 2 memory carriers) Disk Subsystem: 1x73GB SCSI disk Other Hardware: N/A

Software

Operating System: Red Hat Linux Advanced Server 2.1 for the Itanium Processor Compiler: Intel(R) C++ Compiler for Linux 7.0 Intel(R) Fortran Compiler for Linux 7.0 File System: ext3 System State: Multi-user

Notes/Tuning Information

 +FDO: PASS1=-prof_gen  PASS2=-prof_use
 Base tuning:
 C programs:       -ipo -O3 +FDO -ansi_alias
 Fortran programs: -ipo -O3 +FDO
 Portability:
 178.galgel: -FI

 Peak flags same as baseline (basepeak=true set globally)

 Note:
   EFI shell utility ’cpuconfig’ used
   to deconfigure other processors