Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Intel Corporation

Intel D850EMVR motherboard (3.06 GHz, Pentium 4 processor with Hyper-Threading Technology)

SPECfp_rate2000 = SPECfp_rate_base2000 =

13.7 13.6

SPEC license #: 13 Tested by: Intel Corporation Test date: Oct-2002 Hardware Avail: Nov-2002 Software Avail: Apr-2002

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 3 6 9 12 15 18 21 24 168.wupwise 2 210 17.7 2 207 17.9

171.swim 2 365 19.7 2 358 20.1

172.mgrid 2 351 11.9 2 347 12.0

173.applu 2 361 13.5 2 363 13.4

177.mesa 2 219 14.8 2 213 15.3

178.galgel 2 306 22.0 2 305 22.1

179.art 2 770 7.83 2 768 7.85

183.equake 2 195 15.4 2 188 16.1

187.facerec 2 228 19.4 2 227 19.4

188.ammp 2 569 8.98 2 558 9.15

189.lucas 2 314 14.8 2 315 14.7

191.fma3d 2 361 13.5 2 361 13.5

200.sixtrack 2 290 8.80 2 286 8.93

301.apsi 2 567 10.6 2 564 10.7

Hardware

CPU: Intel Pentium 4 Processor with Hyper-Threading Technology(3.06 GHz, 533 MHz bus) CPU MHz: 3067 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip (Hyper-Threading Technology enabled) CPU(s) orderable: 1 Parallel: No Primary Cache: 12k micro-ops I + 8KBD on chip Secondary Cache: 512KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 256 MB (2 128 MB PC1066-32 RDRAM non-ECC modules) Disk Subsystem: IBM 120GXP 80 GB IC35L080AVVA07-0 ATA-100 Other Hardware: None

Software

Operating System: Windows XP Professional(Build 2600) Compiler: Intel C++ Compiler 6.0 Build 020321Z

Intel Fortran Compiler 6.0 Build 020321Z Microsoft Visual C++ 6.0 SP5(for libraries)

File System: FAT32 System State: Default

Notes/Tuning Information

 +FDO: PASS1=  -Qprof_gen  PASS2=-Qprof_use
 Base tuning:  -Qipo -QxW -O3 +FDO
 Portability:
 178.galgel:   -FI /F32000000
 Peak tuning:
 168.wupwise:  -Qipo -QxW  -O3 +FDO
 171.swim:     -Qipo -QxW  -O3 +FDO
 172.mgrid:    -Qipo -QaxW -O3 +FDO
 173.applu:    -Qipo -QxW  -O3 -Qscalar_rep- -Qauto +FDO
 177.mesa:     -Qipo -Oa -QxW -O3 +FDO
 178.galgel:   -Qipo -QxW  -O3 +FDO
 179.art:      -Qipo -QxW  -O3 -Oa +FDO
 183.equake:   -Qipo -QxW  -Oa -Qrcd +FDO
 187.facerec:  -Qipo -QxW  -O3 +FDO
 188.ammp:     -Qipo -QxW  -O3 -Oa +FDO
 189.lucas:    -Qipo -QxW  -O3 +FDO
 191.fma3d:    -Qipo -QxW  -O3 +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Intel Corporation

Intel D850EMVR motherboard (3.06 GHz, Pentium 4 processor with Hyper-Threading Technology)

SPECfp_rate2000 = SPECfp_rate_base2000 =

13.7 13.6

SPEC license #: 13 Tested by: Intel Corporation Test date: Oct-2002 Hardware Avail: Nov-2002 Software Avail: Apr-2002

Notes/Tuning Information (Continued)

 200.sixtrack: -Qipo -QxW  +FDO
 301.apsi:     -Qipo -QxW  -O3 +FDO
 Tested systems can be used with Shin-G ATX case, Delta Inc. power supply PS-300GB-1 B
 Product description located as of 10/2002:
 http://developer.intel.com/design/motherbd/mv2/index.htm
 Motherboard ordering information is available at:
 http://program.intel.com/shared/products/boards/d850emv2/index.htm
 The system bus runs at 533 MHz