Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

NEC Corporation TX7/i9510(1000MHz, Itanium 2)

SPECfp2000 = SPECfp_base2000 = -- 1259

SPEC license #: 1184 Tested by: NEC T.Kokubo Test date: Dec-2002 Hardware Avail: Aug-2002 Software Avail: Nov-2002

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 171 933

171.swim 3100 104 2987

172.mgrid 1800 103 1747

173.applu 2100 107 1958

177.mesa 1400 198 707

178.galgel 2900 116 2496

179.art 2600 85.8 3030

183.equake 1300 88.8 1463

187.facerec 1900 176 1082

188.ammp 2200 249 885

189.lucas 2000 209 955

191.fma3d 2100 323 649

200.sixtrack 1100 121 907

301.apsi 2600 416 625

Hardware

CPU: Itanium2 CPU MHz: 1000 FPU: Integrated CPU(s) enabled: 32 cores, 32 chips, 1 core/chip CPU(s) orderable: 1-32 Parallel: No Primary Cache: 16KBI + 16KBD on chip Secondary Cache: 256KB on chip L3 Cache: 3MB on chip Other Cache: None Memory: 64GB Disk Subsystem: 3x32GB + 11x73GB SCSI disk Other Hardware: Ethernet

Software

Operating System: NEC IA-64 Linux R3.2 Compiler: NEC FORTRAN95 R3.2 NEC C/C++ R3.2 File System: ext2 System State: Multi-user

Notes/Tuning Information

 Base tuning:
    Fortran:    -O3 -ipo -ftz  +FDO
    C:          -O3 -ipo -ftz  +FDO
 +FDO:
    PASS1:      -prof_gen
    PASS2:      -prof_use
 Portability:
    178.galgel: -FI

 11x73GB SCSI disk system setup as big work area with no striping.
 3x32GB SCSI disk system setup: 1 disk for OS installing area, 2
 disks for users area, and both disks are no striping. The SPEC
 benchmark environment was on the users area, and the compiler
 was located on the same disk with the OS installing area.