Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer pSeries 630 Model 6C4 (1450 Mhz, 1 CPU)

SPECfp2000 = SPECfp_base2000 = -- 984 SPEC license #: 11 Tested by: IBM, Austin, Tx Test date: Mar-2003 Hardware Avail: Feb-2003 Software Avail: Feb-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 110 1460

171.swim 3100 268 1157

172.mgrid 1800 258 697

173.applu 2100 263 800

177.mesa 1400 236 594

178.galgel 2900 105 2756

179.art 2600 187 1394

183.equake 1300 121 1073

187.facerec 1900 165 1151

188.ammp 2200 280 785

189.lucas 2000 211 947

191.fma3d 2100 283 742

200.sixtrack 1100 178 620

301.apsi 2600 296 877

Hardware

CPU: POWER4+ CPU MHz: 1450 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 2 cores/chip, 1 chip/SCM CPU(s) orderable: 1,2,4 (order by # cores) Parallel: No Primary Cache: 64KBI+32KBD (on chip) per core Secondary Cache: 1536KB unified (on chip) per chip L3 Cache: 8MB unified (off-chip) per SCM, 1 SCM in SUT Other Cache: None Memory: 8 GB Disk Subsystem: 1x36GB SCSI Other Hardware: None

Software

Operating System: SLES 8 for pSeries w/2.4.19 kernel Compiler: IBM VisualAge C++ Version 6.0 for Linux on pSeries

IBM XL Fortran Version 8.1 for Linux on pSeries

File System: ext2 System State: Multi-user

Notes/Tuning Information

 cfg file:  ppc32-linux-ibm-ref-o5.cfg

 Compiled 32-bit applications

 CC  = /opt/ibmcmp/vac/6.0/bin/xlc
 CXX = /opt/ibmcmp/vacpp/6.0/bin/xlC
 FC  = /opt/ibmcmp/xlf/8.1/bin/xlf90
 F77 = /opt/ibmcmp/xlf/8.1/bin/xlf90

 SCM: Acronym for "Single-chip module"
 SUT: Acronym for "System under test"

 SLES: SuSE Linux Enterprise Server

 3 processors were deconfigured through the configuration menu.

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer pSeries 630 Model 6C4 (1450 Mhz, 1 CPU)

SPECfp2000 = SPECfp_base2000 = -- 984 SPEC license #: 11 Tested by: IBM, Austin, Tx Test date: Mar-2003 Hardware Avail: Feb-2003 Software Avail: Feb-2003

Notes/Tuning Information (Continued)

 Floating point optimization flags
    FP: -O5

 Floating point portability flags
    wupwise: -qfixed
    swim: -qfixed
    mgrid: -qfixed
    applu: -qfixed
    mesa: none
    galgel: -qfixed -qsuffix=f=f90
    facerec: -qsuffix=f=f90
    lucas: -qsuffix=f=f90
    fma3d: -qsuffix=f=f90
    sixtrack: -qfixed
    apsi: -qfixed