Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Einux A4800

SPECfp2000 = SPECfp_base2000 =

1012 934 SPEC license #: 49 Tested by: AMD Austin TX Test date: Apr-2003 Hardware Avail: Jul-2003 Software Avail: May-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 500 1000 1500 2000

168.wupwise 1600 169 944 152 1050

171.swim 3100 205 1509 178 1739

172.mgrid 1800 208 863 206 875

173.applu 2100 262 802 237 886

177.mesa 1400 144 974 140 997

178.galgel 2900 222 1305 175 1654

179.art 2600 213 1222 200 1300

183.equake 1300 164 794 133 979

187.facerec 1900 180 1055 171 1109

188.ammp 2200 247 891 242 909

189.lucas 2000 163 1230 161 1239

191.fma3d 2100 230 913 230 913

200.sixtrack 1100 314 351 288 382

301.apsi 2600 306 851 286 910

Hardware

CPU: AMD Opteron 140, 1.4 GHz CPU MHz: 1400 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1,2,4 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 4x512MB PC2700 DDR ECC Reg SDRAM CL2.5 Disk Subsystem: IDE 7200 RPM Other Hardware: None

Software

Operating System: Windows Server 2003 Enterprise Edition Compiler: Intel C/C++ 7.0 build 20021212Z and

Intel Fortran 7.0 build 20021212Z Compaq Visual Fortran Compiler Version 6.6 (Update B) Microsoft Visual Studio .NET (libraries)7.0.9466 MicroQuill Smartheap Library 6.0

File System: NTFS System State: Default

Notes/Tuning Information

  +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
  icl and ifl are the Intel C/C++ and Fortran compilers
  f90 is the Compaq Fortran compiler
  shlW32M6.lib is the SmartHeap library V6.0 from MicroQuill www.microquill.com
  Portability:
    178.galgel: -FI -Fe$@ -link -stack:32000000
  Baseline: C       icl +FD0 -O3 -QxW  -Qipo
  Baseline: Fortran ifl +FDO -O3 -QxW  -Qipo
  Peak tuning:
    168.wupwise:    ifl +FD0     -QxK  -Qipo -Ow
    171.swim:       f90 -Optimize:5 -alignment:dcommons -alignment:records
                        -alignment:sequence -architecture:k7
                        -assume:noaccuracy_sensitive -math_library:fast -tune:k7
    172.mgrid:      ifl +FD0 -O3 -QaxW -Qipo -Oa -Qprefetch-
    173.applu:      ifl +FD0 -O3 -QxK  -Qipo     -Qscalar_rep-           -Zp8
    177.mesa:       icl +FD0 -O3 -QxW  -Qipo -Oa -Qscalar_rep-
    178.galgel:     f90 -Optimize:5 -fast

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Einux A4800

SPECfp2000 = SPECfp_base2000 =

1012 934 SPEC license #: 49 Tested by: AMD Austin TX Test date: Apr-2003 Hardware Avail: Jul-2003 Software Avail: May-2003

Notes/Tuning Information (Continued)

    179.art:        icl                -Qipo -Oa               -Qunroll4 -Zp4
    183.equake:     icl      -O3 -QxK  -Qipo -Oa shlW32M6.lib            -Zp4
    187.facerec:    ifl +FD0 -O3 -QaxW -Qipo     -Qscalar_rep- -Qunroll1
    188.ammp:       icl          -QxW        -Oa
    189.lucas:      ifl +FD0 -O3 -QxW  -Qipo     -Qprefetch-
    191.fma3d:      ifl basepeak=1
    200.sixtrack:   ifl                -Qipo -Oa                         -Zp4
    301.apsi:       f90 -Optimize:5 -fast
  ONESTEP is used for all base and peak runs