Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

ASUS SK8N Motherboard, AMD Opteron (TM) 146

SPECfp2000 = SPECfp_base2000 =

1339 1250

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Sep-2003 Hardware Avail: Sep-2003 Software Avail: Feb-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 119 1348 108 1485

171.swim 3100 171 1818 142 2186

172.mgrid 1800 161 1118 159 1134

173.applu 2100 194 1080 182 1155

177.mesa 1400 99.3 1410 97.4 1437

178.galgel 2900 157 1843 134 2160

179.art 2600 168 1551 155 1679

183.equake 1300 118 1104 103 1267

187.facerec 1900 128 1484 124 1528

188.ammp 2200 180 1222 176 1247

189.lucas 2000 142 1412 142 1411

191.fma3d 2100 170 1239 170 1239

200.sixtrack 1100 225 489 201 547

301.apsi 2600 234 1110 224 1160

Hardware

CPU: AMD Opteron (TM) 146 CPU MHz: 2000 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2x512MB PC3200 DDR SDRAM ECC Registered CL2.5 Disk Subsystem: SATA, Western Digital WD360GD, 10k rpm Other Hardware: None

Software

Operating System: Microsoft Windows XP Professional (SP1a) Compiler: Intel C/C++ 7.0 build 20021212Z and Intel Fortran 7.0 build 20021212Z

Compaq Visual Fortran Compiler Version 6.6 (Update B) Microsoft Visual Studio .NET 7.0.9466 (for libraries) MicroQuill Smartheap Library 6.0

File System: NTFS System State: Default

Notes/Tuning Information

  +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
  icl and ifl are the Intel C/C++ and Fortran compilers
  f90 is the Compaq Fortran compiler
  shlW32M6.lib is the SmartHeap library V6.0 from MicroQuill www.microquill.com
  Portability:
    178.galgel: -FI -Fe$@ -link -stack:32000000
  Baseline: C       icl +FDO -O3 -QxW  -Qipo
  Baseline: Fortran ifl +FDO -O3 -QxW  -Qipo
  Peak tuning:
    168.wupwise:    ifl +FDO     -QxK  -Qipo -Ow
    171.swim:       f90 -Optimize:5 -alignment:dcommons -alignment:records
                        -alignment:sequence -architecture:k7
                        -assume:noaccuracy_sensitive -math_library:fast -tune:k7
    172.mgrid:      ifl +FDO -O3 -QaxW -Qipo -Oa -Qprefetch-
    173.applu:      ifl +FDO -O3 -QxK  -Qipo     -Qscalar_rep-           -Zp8
    177.mesa:       icl +FDO -O3 -QxW  -Qipo -Oa -Qscalar_rep-
    178.galgel:     f90 -Optimize:5 -fast

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

ASUS SK8N Motherboard, AMD Opteron (TM) 146

SPECfp2000 = SPECfp_base2000 =

1339 1250

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Sep-2003 Hardware Avail: Sep-2003 Software Avail: Feb-2003

Notes/Tuning Information (Continued)

    179.art:        icl                -Qipo -Oa               -Qunroll4 -Zp4
    183.equake:     icl      -O3 -QxK  -Qipo -Oa shlW32M6.lib            -Zp4
    187.facerec:    ifl +FDO -O3 -QaxW -Qipo     -Qscalar_rep- -Qunroll1
    188.ammp:       icl          -QxW        -Oa
    189.lucas:      ifl +FDO -O3 -QxW  -Qipo     -Qprefetch-
    191.fma3d:      ifl basepeak=1
    200.sixtrack:   ifl                -Qipo -Oa                         -Zp4
    301.apsi:       f90 -Optimize:5 -fast
  ONESTEP is used for all base and peak runs
  ECC on, ECC scrubbing off