Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

ASUS SK8N Motherboard, AMD Opteron (TM) 148

SPECfp2000 = SPECfp_base2000 =

1514 1505

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Nov-2003 Hardware Avail: Dec-2003 Software Avail: Nov-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 95.6 1674 95.6 1674

171.swim 3100 138 2254 138 2254

172.mgrid 1800 143 1254 137 1318

173.applu 2100 156 1344 154 1360

177.mesa 1400 87.3 1603 84.3 1660

178.galgel 2900 108 2679 108 2679

179.art 2600 177 1468 176 1474

183.equake 1300 91.4 1422 94.1 1381

187.facerec 1900 94.2 2016 94.2 2016

188.ammp 2200 169 1299 169 1303

189.lucas 2000 131 1529 130 1543

191.fma3d 2100 146 1438 146 1438

200.sixtrack 1100 161 684 161 684

301.apsi 2600 190 1366 190 1366

Hardware

CPU: AMD Opteron (TM) 148 CPU MHz: 2200 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2 x 512MB PC3200 DDR SDRAM, ECC Registered Disk Subsystem: Western Digital WD2000, IDE Other Hardware: None

Software

Operating System: SuSE Linux 9.0 (AMD64) 2.4.21-102-default Compiler: PGI Fortran 5.1-0 and SuSE gcc 3.3.1 compiler (from SuSE Linux 9.0) File System: Linux/ext3 System State: Multi-user SuSE Run level 3

Notes/Tuning Information

Tested by Advanced Micro Devices
  +FDO: PASS1=-fprofile-arcs PASS2=-fbranch-probabilities
  pgf90 is the PGI Fortran 5.1 compiler
  gcc is the SuSE gcc 3.3.1 compiler
  Portability:
                    PORTABILITY=-DSPEC_CPU2000_LP64 is applied to all the C benchmarks.
    178.galgel:     -Mfixed
  Baseline: C       gcc  -O3 -funroll-all-loops +FDO
  Baseline: Fortran pgf90 -fastsse  -Mipa=fast
  Peak tuning:
    168.wupwise:    basepeak=true
    171.swim:       basepeak=true
    172.mgrid:      pgf90 -fast -Mipa=fast
    173.applu:      pgf90 -fast -Mipa=fast
    177.mesa:       gcc -O3 -funroll-all-loops -finline-limit=2000 +FDO
    178.galgel:     basepeak=true
    179.art:        gcc -O3 -funroll-all-loops -ffast-math -finline-limit=1500 +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

ASUS SK8N Motherboard, AMD Opteron (TM) 148

SPECfp2000 = SPECfp_base2000 =

1514 1505

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Nov-2003 Hardware Avail: Dec-2003 Software Avail: Nov-2003

Notes/Tuning Information (Continued)

    183.equake:     gcc -O3 -funroll-all-loops -ffast-math -finline-limit=2000
    187.facerec:    basepeak=true
    188.ammp:       gcc -O3 -funroll-all-loops -ffast-math -finline-limit=2000 +FDO
    189.lucas:      pgf90 -fastsse -Mipa=fast -Mnosmart
    191.fma3d:      basepeak=true
    200.sixtrack:   basepeak=true
    301.apsi:       basepeak=true
  ONESTEP is used for all base and peak runs
 The tested system can be assembled using an ATX case such as the Antec KS-282,
 a 480W power supply, and a PCI or AGP video card.