Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer pSeries 655 (1700 MHz, 8 CPU)

SPECint_rate2000 = SPECint_rate_base2000 =

92.0 83.5

SPEC license #: 11Tested by: IBM Austin Test date: Dec-2003 Hardware Avail: Feb-2004 Software Avail: Oct-2003

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 30 60 90 120 150 164.gzip 8 183 71.0 8 183 71.0

175.vpr 8 182 71.3 8 182 71.3

176.gcc 8 102 99.7 8 102 99.7

181.mcf 8 218 76.6 8 214 77.9

186.crafty 8 113 82.1 8 90.2 103

197.parser 8 361 46.2 8 198 84.3

252.eon 8 103 117 8 103 117

253.perlbmk 8 234 71.3 8 208 80.5

254.gap 8 113 90.7 8 113 90.7

255.vortex 8 131 135 8 124 142

256.bzip2 8 152 91.4 8 149 93.6

300.twolf 8 331 84.1 8 295 94.5

Hardware

CPU: POWER4+ CPU MHz: 1700 FPU: Integrated CPU(s) enabled: 8 cores, 4 chips, 2 cores/chip, 4 chips/MCM CPU(s) orderable: 4,8 (order by # cores) Parallel: No Primary Cache: 64KBI+32KBD (on chip) per core Secondary Cache: 1536KB unified (on chip) per chip L3 Cache: 128MB unified (off-chip) per MCM, 1 MCM in SUT (4 chips per MCM) Other Cache: None Memory: 32 GB Disk Subsystem: 2x36GB SCSI, 10K RPM Other Hardware: None

Software

Operating System: AIX 5L V5.2 5765-E62 (05/2003) Compiler: IBM C for AIX, Version 6.0

IBM VisualAge C++ Professional for AIX, Version 6.0

File System: AIX/JFS2 System State: Multi-User

Notes/Tuning Information

 Portability Flags:
   176.gcc:      -ma -DHOST_WORDS_BIG_ENDIAN
   186.crafty:   -DAIX
   252.eon:      srcalt=fmax_errno
                 -I. -DNDEBUG
   253.perlbmk:  -DSPEC_CPU2000_AIX
   254.gap:      -DSYS_IS_BSD -DSYS_STRING_H -DSYS_HAS_TIME_PROTO
                 -DSYS_HAS_MALLOC_PROTO -DSYS_HAS_CALLOC_PROTO
   300.twolf:    -DHAVE_SIGNED_CHAR

 Base Optimization Flags:
   C:    -qpdf1/pdf2
         -O5 -blpdata -qalign=natural
   C++:  -qpdf1/pdf2
         -O5 -lhmu -qalign=natural

 Peak Optimization Flags
   164.gzip:     basepeak = 1

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer pSeries 655 (1700 MHz, 8 CPU)

SPECint_rate2000 = SPECint_rate_base2000 =

92.0 83.5

SPEC license #: 11Tested by: IBM Austin Test date: Dec-2003 Hardware Avail: Feb-2004 Software Avail: Oct-2003

Notes/Tuning Information (Continued)

   175.vpr:      basepeak = 1
   176.gcc:      basepeak = 1
   181.mcf:      fdpr -v -R3
                 -O5 -blpdata -D_ILS_MACROS
   186.crafty:   -qpdf1/pdf2
                 fdpr -v -R3
                 -O3 -q64
   197.parser:   -O5 -blpdata -D_ILS_MACROS
   252.eon:      basepeak = 1
   253.perlbmk:  -qpdf1/pdf2
                 -O5 -lhmu -qalign=natural
   254.gap:      basepeak = 1
   255.vortex:   -qpdf1/pdf2
                 -O5 -lhmu -qalign=natural
   256.bzip2:    -qpdf1/pdf2
                 -O5 -blpdata -qarch=pwr3 -qtune=pwr3
   300.twolf:    -qpdf1/pdf2
                 -O5 -lhmu -qalign=natural -blpdata
                 "CC      = /usr/vac/bin/xlc"

 Approved alternate-source file 252.eon.fmax_errno.src.alt.tar.gz
 was used with 252.eon for POSIX-compatibility.

 C:   IBM VAC++ invoked as cc except where noted as xlc
 C++: IBM VAC++ invoked as xlC

 fpdr: Feedback directed program restructuring tool
 ulimits set to unlimited.
 Large page mode and memory affinity were set as follows:
    vmo -r -o lgpg_regions=400 -o lgpg_size=16777216 -o memory_affinity=1
    chuser capabilities=CAP_BYPASS_RAC_VMM,CAP_PROPAGATE $USER
    shutdown -r
    export MEMORY_AFFINITY=MCM

 MCM: Acronym for "Multi-Chip Module"
 SUT: Acronym for "System Under Test"

 Form used to submit "rate" runs:
    submit = let "MYCPU=$SPECUSERNUM"; bindprocessor $$ $MYCPU; $command