Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Supermicro

SUPER X5DPA-GG (3.06GHz, 533MHz bus)

SPECfp_rate2000 = SPECfp_rate_base2000 =

12.4 12.1

SPEC license #:001176 Tested by:Super Micro computer, Inc., San Jose, CA Test date: Jan-2004 Hardware Avail: Nov-2003 Software Avail: Aug-2003

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 3 6 9 12 15 18 21 24 168.wupwise 2 176 21.1 2 186 20.0

171.swim 2 608 11.8 2 609 11.8

172.mgrid 2 448 9.32 2 447 9.35

173.applu 2 444 11.0 2 443 11.0

177.mesa 2 174 18.6 2 168 19.4

178.galgel 2 370 18.2 2 378 17.8

179.art 2 1028 5.87 2 983 6.13

183.equake 2 227 13.3 2 179 16.9

187.facerec 2 236 18.7 2 229 19.3

188.ammp 2 628 8.12 2 630 8.10

189.lucas 2 404 11.5 2 400 11.6

191.fma3d 2 367 13.3 2 367 13.3

200.sixtrack 2 246 10.4 2 234 10.9

301.apsi 2 665 9.06 2 648 9.30

Hardware

CPU: Intel Xeon (3.06GHz, 533MHz bus) CPU MHz: 3066 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip (Hyper-Threading Technology enabled) CPU(s) orderable: 1,2 Parallel: No Primary Cache: 12K(I) micro-ops + 8KB(D) on chip Secondary Cache: 512KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2x1024MB PC2100 Registered ECC Double-sided CL2 Disk Subsystem: 1 x IBM Deskstar 123.5GB IDE Other Hardware:

Software

Operating System: Windows XP Professional W/ SP1a Compiler: Intel C++ and Fortran Compiler 7.1 Build 20030224Z

Microsoft Visual Studio Enterprise Edition 6.0(for libraries) MicroQuill Smartheap Library 7.0

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
 Base tuning: -QxW -Qipo -O3 +FDO
 Portability:
 178.galgel: -FI /F32000000
 Peak tuning:
 168.wupwise:    -Qipo -QxW  +FDO
 171.swim:       -Qipo -QxW  -O3 +FDO
 172.mgrid:      -Qipo -QaxW -O3 +FDO
 173.applu:      -Qipo -QxW  -O3 -Qscalar_rep- +FDO
 177.mesa:       -Qipo -QxW  -O3 +FDO
 178.galgel:     -Qipo -QxW  -O3 +FDO
 179.art:        -Qipo -Oa -Qunroll4 -Zp4
 183.equake:     -Qipo -QxW  -Oa +FDO shlw32M.lib
 187.facerec:    -Qipo -QxW  -O3 -Qunroll1 -Qscalar_rep- +FDO
 188.ammp:       -QxW  -Oa
 189.lucas:      -Qipo -QaxW
 191.fma3d:      basepeak=1

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Supermicro

SUPER X5DPA-GG (3.06GHz, 533MHz bus)

SPECfp_rate2000 = SPECfp_rate_base2000 =

12.4 12.1

SPEC license #:001176 Tested by:Super Micro computer, Inc., San Jose, CA Test date: Jan-2004 Hardware Avail: Nov-2003 Software Avail: Aug-2003

Notes/Tuning Information (Continued)

 200.sixtrack:   -Qipo -QxW  +FDO
 301.apsi:       -Qipo -QxW  -O3 +FDO
 Hyper-Threading Technology is turned ON
 ONESTEP is used for all base and peak runs
 The tested system can be assembled using an 1U Chassis such as the Supermicro SC811i-350,
with 350W power supply.  See Link for more chassis compatibility lists at
http://www.supermicro.com/PRODUCT/Chassis/compatibility.htm.
The System bus runs up to 8GB ECC registered DDR-200/266 memory in 4 DIMM slots.
 shlW32M.lib is the SmartHeap library V7.0 from MicroQuill www.microquill.com