Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell PowerEdge 6600 (3.0 GHz Xeon MP)

SPECfp2000 = SPECfp_base2000 =

1283 1270

SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Dec-2003 Hardware Avail: Jan-2004 Software Avail: Apr-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 120 1339 119 1342

171.swim 3100 230 1350 230 1351

172.mgrid 1800 170 1060 169 1062

173.applu 2100 232 906 231 909

177.mesa 1400 115 1213 114 1228

178.galgel 2900 94.9 3055 95.0 3054

179.art 2600 83.8 3102 82.8 3139

183.equake 1300 120 1081 114 1139

187.facerec 1900 136 1393 132 1435

188.ammp 2200 160 1373 160 1377

189.lucas 2000 167 1199 165 1209

191.fma3d 2100 213 987 213 987

200.sixtrack 1100 196 562 193 570

301.apsi 2600 252 1033 252 1033

Hardware

CPU: Intel Xeon MP (400 MHz system bus) CPU MHz: 3000 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip (Hyper-Threading Technology disabled) CPU(s) orderable: 1,2,4 Parallel: No Primary Cache: 12K(I) micro-ops + 8KB(D) on chip Secondary Cache: 512KB(I+D) on chip L3 Cache: 4096KB(I+D) on chip Other Cache: N/A Memory: 4 x 1024MB DDR200 Disk Subsystem: 1 x 36GB SEAGATE SCSI Other Hardware:

Software

Operating System: Windows 2000 Advanced Server (SP2) Compiler: Intel C++ Compiler 7.1 (20030402Z) Intel Fortran Compiler 7.1 (20030402Z) Microsoft Visual Studio .NET (7.0.9466) File System: NTFS System State: Default

Notes/Tuning Information

 PORTABILITY
   178.galgel:   -FI /F32000000
 FEEDBACK DIRECTED OPTMIZATION
   FDO:          PASS1=  -Qprof_gen  PASS2=-Qprof_use
 BASE TUNING
   C/F77/F90:    -Qipo -QxW -O3 +FDO
 PEAK TUNING
   168.wupwise:  -Qipo -QxW  -O3 +FDO
   171.swim:     -Qipo -QxW  -O3 +FDO
   172.mgrid:    -Qipo -QaxW -O3 +FDO
   173.applu:    -Qipo -QxW  -O3 -Qscalar_rep- -Qauto +FDO
   177.mesa:      PASS1= -Qprof_gen PASS2= -Qipo -Qprof_use -QxW -O3 -Oa
   178.galgel:   -Qipo -QxW  -O3 +FDO
   179.art:      -Oa -Qipo -Qunroll4 -Zp4
   183.equake:   -QxW -Oa -Qrcd -Qipo +FDO
   187.facerec:  -O3 -QaxW -Qipo -Qunroll1 -Qscalar_rep- +FDO
   188.ammp:     -Oa -QxW

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell PowerEdge 6600 (3.0 GHz Xeon MP)

SPECfp2000 = SPECfp_base2000 =

1283 1270

SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Dec-2003 Hardware Avail: Jan-2004 Software Avail: Apr-2003

Notes/Tuning Information (Continued)

   189.lucas:    -Qipo -QaxW
   191.fma3d:    basepeak=yes
   200.sixtrack: -Qipo -QxW  +FDO
   301.apsi:     -Qipo -QxW  -O3 +FDO
 ONESTEP=YES is set for all benchmarks
 Hyper-Threading Technology disabled in BIOS