Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Unisys Corporation

ES7000 ORION 540 (3.0GHz Xeon MP)

SPECint_rate2000 = SPECint_rate_base2000 = 169 162 SPEC license #: 15 Tested by: Unisys Corporation Test date: Jul-2004 Hardware Avail: Apr-2004 Software Avail: Aug-2004

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 50 100 150 200 250 300 164.gzip 16 189 138 16 189 138

175.vpr 16 243 107 16 217 120

176.gcc 16 86.0 237 16 86.0 237

181.mcf 16 359 92.9 16 359 92.9

186.crafty 16 99.2 187 16 89.4 208

197.parser 16 180 185 16 173 193

252.eon 16 91.9 262 16 91.9 262

253.perlbmk 16 149 224 16 138 241

254.gap 16 357 57.2 16 354 57.7

255.vortex 16 192 184 16 167 211

256.bzip2 16 153 181 16 153 181

300.twolf 16 213 261 16 207 269

Hardware

CPU: Intel Xeon MP(400MHz system bus) CPU MHz: 3000 FPU: Integrated CPU(s) enabled: 16 cores, 16 chips, 1 core/chip (HT Technology disabled) CPU(s) orderable: 16,20,24,28,32 Parallel: No Primary Cache: 12K(I) micro-ops + 8KB(D) on chip Secondary Cache: 512KB (I+D) on chip L3 Cache: 4096KB (I+D) on chip Other Cache: 32MB L4 Cache off chip per 4 CPUs Memory: 4 GB Disk Subsystem: 1X36GB SCSI DISK (15K rpm) Other Hardware:

Software

Operating System: Suse Linux Enterprise Server release 9.0 RC 5, 2.6.5-7.97-bigsmp Compiler: Intel(R) C++ Compiler for Linux 7.1 (Build 20040309Z)

Intel(R) C++ Compiler for Linux 8.0 (Build 20040412Z)

File System: ext2 System State: Multi-user (init 3)

Notes/Tuning Information

 Portability Flags:
       176.gcc: -Dalloca=_alloca -DUSG
    186.crafty: -DLINUX_i386
       252.eon: -DHAS_ERRLIST
       252.eon: srcalt=fmax_errno
   253.perlbmk: -DSPEC_CPU2000_LINUX_I386 -DSPEC_CPU2000_NEED_BOOL
                -DSPEC_CPU2000_GLIBC22
       254.gap: -DSYS_IS_USG -DSYS_HAS_IOCTL_PROTO -DSYS_HAS_TIME_PROTO
                -DSYS_HAS_SIGNAL_PROTO -DSYS_HAS_ANSI -DSYS_HAS_CALLOC_PROTO
    255.vortex: srcalt=closed_files

 Baseline tuning flags:
       C programs  : -xi     -ipo -fp_port
       CXX programs: -xW -O3 -ipo +FDO

 Peak tuning flags:
       164.gzip: basepeak=yes
        175.vpr: PASS1= -xW          -prof_gen PASS2= -xW -O3 -ipo          -prof_use
        176.gcc: basepeak=yes

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Unisys Corporation

ES7000 ORION 540 (3.0GHz Xeon MP)

SPECint_rate2000 = SPECint_rate_base2000 = 169 162 SPEC license #: 15 Tested by: Unisys Corporation Test date: Jul-2004 Hardware Avail: Apr-2004 Software Avail: Aug-2004

Notes/Tuning Information (Continued)

        181.mcf: basepeak=yes
     186.crafty: PASS1= -xW          -prof_gen PASS2= -xW -O3 -ipo          -prof_use
     197.parser: PASS1= -xW          -prof_gen PASS2= -xW -O3 -ipo          -prof_use
        252.eon: basepeak=yes
    253.perlbmk: PASS1= -xW          -prof_gen PASS2= -xW -O3 -ipo          -prof_use
        254.gap: PASS1= -xi          -prof_gen PASS2= -xi     -ipo -fp_port -prof_use
     255.vortex: PASS1= -xi          -prof_gen PASS2= -xi     -ipo -fp_port -prof_use
      256.bzip2: basepeak=yes
      300.twolf: PASS1= -xW          -prof_gen PASS2= -xW -ipo -Oa -O3      -prof_use

 HyperThreading disabled in BIOS

 Enabled two user settings in the BIOS:
 1. "Adjacent Sector Prefetch"
 2. "Prefetch Queue"
 The Intel 8.0 and 7.1 compilers were invoked using their fully qualified paths;
 the environment setting scripts were not used during compilation or runtime.