Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation IBM xSeries 336 (3.6GHz Xeon)

SPECfp_rate2000 = SPECfp_rate_base2000 =

28.6 28.2

SPEC license #: 11 Tested by: IBM Corporation Test date: Sep-2004 Hardware Avail: Aug-2004 Software Avail: Sep-2004

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 10 20 30 40 50 60 168.wupwise 2 67.3 55.2 2 67.3 55.2

171.swim 2 281 25.6 2 281 25.6

172.mgrid 2 189 22.1 2 189 22.1

173.applu 2 213 22.9 2 199 24.5

177.mesa 2 74.3 43.7 2 74.3 43.7

178.galgel 2 182 37.0 2 182 37.0

179.art 2 151 40.0 2 151 40.0

183.equake 2 108 28.0 2 108 28.0

187.facerec 2 130 33.9 2 130 33.9

188.ammp 2 248 20.6 2 241 21.2

189.lucas 2 196 23.7 2 196 23.7

191.fma3d 2 187 26.0 2 187 26.0

200.sixtrack 2 174 14.7 2 164 15.6

301.apsi 2 241 25.0 2 241 25.0

Hardware

CPU: Intel Xeon processor, 800MHz FSB CPU MHz: 3600 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip (HyperThreading Disabled) CPU(s) orderable: 1,2 Parallel: No Primary Cache: 12K(I) micro-ops + 16KB(D) on chip Secondary Cache: 1024KB (I+D) on chip L3 Cache: None Other Cache: None Memory: 8GB (8x1024GB DDR-II 400 DIMMs) Disk Subsystem: 1 x 72GB SCSI Other Hardware: None

Software

Operating System: SUSE Linux SLES 9 (64-bit), kernel 2.6.5-7.97-smp Compiler: Intel(R) C Compiler for Intel(R) EM64T-based applications

Version 8.1 Build 20040708 Intel(R) Fortran Compiler for Intel(R) EM64T-based applications Version 8.1 Build 20040708

File System: Reiserfs System State: Multi-user, run level 3

Notes/Tuning Information

 Portability Flags:
   178.galgel:  -FI
 Base Tuning for C and Fortran Programs:
   -xP -fast -ansi_alias +FDO
   +FDO for C and Fortran programs:
     PASS1=-prof_gen
     PASS2=-prof_use
 Peak Tuning:
   168.wupwise:  basepeak=yes
   171.swim:     basepeak=yes
   172.mgrid:    basepeak=yes
   173.applu:    -xP -fast -scalar_rep- -auto  +FDO
   177.mesa:     -xP -fast -alias_args -scalar_rep- +FDO
   178.galgel:   basepeak=yes
   179.art:      basepeak=yes
   183.equake:   basepeak=yes
   187.facerec:  basepeak=yes

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation IBM xSeries 336 (3.6GHz Xeon)

SPECfp_rate2000 = SPECfp_rate_base2000 =

28.6 28.2

SPEC license #: 11 Tested by: IBM Corporation Test date: Sep-2004 Hardware Avail: Aug-2004 Software Avail: Sep-2004

Notes/Tuning Information (Continued)

   188.ammp:     -xP -alias_args
   189.lucas:    basepeak=yes
   191.fma3d:    basepeak=yes
   200.sixtrack: -xP -ipo +FDO
   301.apsi:     basepeak=yes
 BIOS Information:
   Version 1.00
   Date 08/31/04
   Build Level APE115AUS
   HyperThreading Disabled