Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

MSI K8N Neo2 Platinum Motherboard, AMD Athlon (TM) 64 FX-55

SPECfp2000 = SPECfp_base2000 =

1878 1695

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Oct-2004 Hardware Avail: Oct-2004 Software Avail: Aug-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 83.6 1915 70.7 2262

171.swim 3100 134 2320 135 2303

172.mgrid 1800 112 1606 102 1763

173.applu 2100 120 1754 105 2005

177.mesa 1400 88.9 1575 64.4 2174

178.galgel 2900 101 2874 91.8 3159

179.art 2600 141 1848 100 2597

183.equake 1300 82.8 1570 82.8 1570

187.facerec 1900 94.8 2004 88.0 2160

188.ammp 2200 144 1532 137 1607

189.lucas 2000 126 1583 112 1788

191.fma3d 2100 136 1542 132 1586

200.sixtrack 1100 139 792 138 795

301.apsi 2600 157 1661 155 1677

Hardware

CPU: AMD Athlon (TM) 64 FX-55 (ADAFX55DEI5AS) CPU MHz: 2600 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2x512 MB PC3200 DDR SDRAM CL2.0 Disk Subsystem: IDE, Western Digital WD1200 Other Hardware: None

Software

Operating System: SuSE Linux Enterprise Sever for AMD64 (SP3) Compiler: PathScale EKO Compiler Suite, Release 1.3 File System: Linux/ext3 System State: Multi-user SuSE Run level 3

Notes/Tuning Information

 +FDO: PASS1= -fb_create fbdata  PASS2= -fb_opt fbdata
 +ACML is linking with AMD Core Math Library

 Baseline optimization
   C programs:       -Ofast -WOPT:mem_opnds=on +FDO
   Fortran programs: -Ofast -LNO:fusion=2
 Portability Flags:
   178.galgel: -fixedform

Peak Tuning:
 168.wupwise: -Ofast -LNO:prefetch_ahead=5:prefetch=3
              -OPT:unroll_times_max=8:unroll_size=128:IEEE_NaN_Inf=off:ro=3 -TENV:X=4
              -IPA:space=1000:linear=on:plimit=50000:callee_limit=5000
              -INLINE:aggressive=on
 171.swim:    -Ofast -LNO:fusion=2:prefetch=2

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Advanced Micro Devices

MSI K8N Neo2 Platinum Motherboard, AMD Athlon (TM) 64 FX-55

SPECfp2000 = SPECfp_base2000 =

1878 1695

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Oct-2004 Hardware Avail: Oct-2004 Software Avail: Aug-2004

Notes/Tuning Information (Continued)

 172.mgrid:   -O3 -LNO:fusion=2:blocking=off:prefetch=2
              -OPT:Ofast:unroll_times_max=8:unroll_size=256:ro=3
              -CG:gcm=off:cflow=off
 173.applu:   -Ofast -CG:local_fwd_sched=on
              -LNO:fusion=2:fission=2:full_unroll_size=10000:prefetch=3
              -OPT:ro=3 -TENV:X=3 -WOPT:val=2
 177.mesa:    -O2 -ipa -OPT:Ofast -fno-math-errno -CG:local_fwd_sched=on +FDO
 178.galgel:  -Ofast -OPT:fast_complex -CG:load_exe=0:use_movlpd=on +ACML
 179.art:     -O3 -OPT:ro=2:div_split=on:alias=typed -fno-math-errno -m32 +FDO
 183.equake:  basepeak = true
 187.facerec:  -Ofast -OPT:treeheight=on:IEEE_NaN_Inf=off:ro=3 -CG:load_exe=0
               -LNO:fusion=2:prefetch=0 +FDO -IPA:plimit=1800
 188.ammp: -O3 -OPT:alias=disjoint:unroll_times_max=8:Ofast:ro=3 -LNO:prefetch=0
           -fno-math-errno -TENV:X=4 +FDO
189.lucas: -Ofast -CG:prefetch=off:load_exe=2:local_fwd_sched
           -TENV:X=4 -WOPT:retype_expr=on +FDO
 191.fma3d: -O2 -ipa -WOPT:mem_opnds=on:retype_expr=on -OPT:Ofast:IEEE_arith=3:ro=3
            +FDO -IPA:pu_reorder=1
 200.sixtrack:= -Ofast +FDO
 301.apsi: -Ofast -TENV:X=4 -LNO:fusion=2:prefetch=0
 The tested system can be assembled using an ATX case such as the Antec P160,
 a 550W power supply such as the Antec True Power 550, and a PCI or AGP video card.
 BIOS rev. v1.3
 High Performance defaults set in BIOS
 Memory timings manually set in BIOS: CAS=2.0, TRCD=2, TRAS=5, TRP=2
 Dynamic Overclocking Disabled in BIOS
 Memory used is Corsair CMX512-3200XLPRO, configured in dual channel mode