Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company

HP Integrity rx4640-8 (1.5GHz/4MB Itanium 2)

SPECfp_rate2000 = SPECfp_rate_base2000 =

70.5 70.5

SPEC license #: 3 Tested by: HP Richardson Test date: Nov-2004 Hardware Avail: Dec-2004 Software Avail: Nov-2004

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 100 200 300 400 500 600 168.wupwise 4 93.2 79.7 4 93.2 79.7

171.swim 4 293 49.1 4 293 49.1

172.mgrid 4 253 33.1 4 253 33.1

173.applu 4 92.7 105 4 92.7 105

177.mesa 4 119 54.5 4 119 54.5

178.galgel 4 51.5 261 4 51.5 261

179.art 4 22.3 541 4 22.3 541

183.equake 4 115 52.6 4 115 52.6

187.facerec 4 144 61.1 4 144 61.1

188.ammp 4 153 66.8 4 153 66.8

189.lucas 4 289 32.2 4 289 32.2

191.fma3d 4 250 39.0 4 250 39.0

200.sixtrack 4 76.0 67.1 4 76.0 67.1

301.apsi 4 304 39.6 4 304 39.6

Hardware

CPU: Intel Itanium 2 CPU MHz: 1500 FPU: Integrated CPU(s) enabled: 4 cores, 4 chips, 1 core/chip CPU(s) orderable: 1-4 Parallel: no Primary Cache: 16KBI + 16KBD on chip, per core Secondary Cache: 256KB (I+D) on chip, per core L3 Cache: 4.0MB (I+D) on chip, per core Other Cache: N/A Memory: 32GB (16x2GB DIMMs) Disk Subsystem: 1x36GB 15K SCSI Other Hardware: N/A

Software

Operating System: Red Hat Linux Advanced Server release 3.0AS (Update 3) Compiler: Intel C++ Compiler 8.1 for Linux (Build 20041021)

Intel Fortran Compiler 8.1 for Linux (Build 20041021)

File System: ext3 System State: Multi-user

Notes/Tuning Information

 Base tuning flags:
          C programs: -fast -ansi_alias +FDO -IPF_fp_relaxed
    Fortran programs: -fast +FDO -IPF_fp_relaxed

 Portability:
          178.galgel:  -FI
          187.facerec: srcalt=AllocShape

 Peak flags same as baseline (basepeak=true set globally)
 +FDO: PASS1=-prof_gen  PASS2=-prof_use

 Note:
   EFI command "cpuconfig" used prior to booting to
   deconfigure other processors if necessary