Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Intel(R) Corporation

Intel(R) D925XECV2 motherboard( 3.73 GHz, Intel(R) Pentium(R) 4 processor Extreme Edition supporting Hyper-Threading Technology)

SPECfp_rate2000 = SPECfp_rate_base2000 =

23.9 23.8

SPEC license #: 13 Tested by: Intel(R) Corporation Test date: Mar-2005 Hardware Avail: Feb-2005 Software Avail: Sep-2004

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 5 10 15 20 25 30 35 40 45 168.wupwise 2 103 36.2 2 103 36.1

171.swim 2 224 32.1 2 224 32.1

172.mgrid 2 193 21.7 2 193 21.7

173.applu 2 263 18.5 2 263 18.5

177.mesa 2 165 19.7 2 165 19.7

178.galgel 2 176 38.3 2 176 38.3

179.art 2 140 43.0 2 140 43.0

183.equake 2 105 28.8 2 110 27.3

187.facerec 2 155 28.5 2 154 28.5

188.ammp 2 307 16.6 2 289 17.6

189.lucas 2 193 24.0 2 187 24.8

191.fma3d 2 248 19.6 2 248 19.6

200.sixtrack 2 245 10.4 2 244 10.5

301.apsi 2 319 18.9 2 321 18.8

Hardware

CPU: Intel(R) Pentium(R) 4 processor Extreme Edition supporting Hyper-Threading Technology( 3.73 GHz, 1066 MHz bus) CPU MHz: 3733 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip (Hyper-Threading Technology enabled) CPU(s) orderable: 1 Parallel: No Primary Cache: 12k micro-ops I + 16KBD on chip Secondary Cache: 2MB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 1 GB (2 512MB Corsair CM2X512-4300C3 DDR2 533 CL3-3-3 DIMMs) Disk Subsystem: Seagate ST3160023AS 160 GB Serial ATA (7200 RPM, 8MB cache) Other Hardware: N/A

Software

Operating System: Windows XP Professional SP2 Compiler: Intel(R) C++ and Fortran Compiler 8.1 Build 20040802Z

Microsoft Visual Studio .Net 2002(for libraries) SmartHeap Library Version 6.0 from http://www.microquill.com/

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=  -Qprof_gen  PASS2=-Qprof_use
 Base tuning:  -fast -Qansi_alias +FDO
 Portability:
 178.galgel:   -FI /F32000000
 Peak tuning:
 168.wupwise:  -fast -Qansi_alias +FDO
 171.swim:     -fast -Qansi_alias +FDO
 172.mgrid:    -fast -Qansi_alias +FDO
 173.applu:  -fast -Qscalar_rep- -Qauto  +FDO
 177.mesa:   basepeak=yes
 178.galgel:   -fast -Qansi_alias +FDO
 179.art:      basepeak=yes
 183.equake:   -QxP -Oa -Qrcd -Qipo +FDO
 187.facerec:  -fast -Qunroll1 -Qscalar_rep- +FDO
 188.ammp:     -Oa -QxP
 189.lucas:    -fast -Qprefetch- +FDO
 191.fma3d:    basepeak=yes

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Intel(R) Corporation

Intel(R) D925XECV2 motherboard( 3.73 GHz, Intel(R) Pentium(R) 4 processor Extreme Edition supporting Hyper-Threading Technology)

SPECfp_rate2000 = SPECfp_rate_base2000 =

23.9 23.8

SPEC license #: 13 Tested by: Intel(R) Corporation Test date: Mar-2005 Hardware Avail: Feb-2005 Software Avail: Sep-2004

Notes/Tuning Information (Continued)

 200.sixtrack: -Qipo -QxP +FDO
 301.apsi:     -fast +FDO
 Tested systems can be used with Shin-G ATX case, Antec NeoPower 480W power supply
 Product description located as of 2/2005
 http://www.intel.com/design/motherbd/cv2/index.htm?iid=ipp_browse+motherbd_d925xecv2&_
 Motherboard is available through Intel(R) Reseller Channel. See

 http://www.intel.com/cd/channel/reseller/asmo-na/eng/products/box_desktop_boards/intel_boards/p4_boards/p4_dsk_board_D925XECV2/index.htm

 The system bus runs at 1066 MHz
 The tested system has a PCIe graphics card installed