Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Advanced Micro Devices

ASUS A8N-SLI Deluxe, AMD Athlon (TM) 64 FX-57

SPECfp2000 = SPECfp_base2000 =

1894 1814

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Jun-2005 Hardware Avail: Jun-2005 Software Avail: Jan-2005

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 54.4 2942 54.4 2942

171.swim 3100 136 2280 129 2396

172.mgrid 1800 117 1539 117 1539

173.applu 2100 138 1523 123 1704

177.mesa 1400 67.4 2078 63.8 2194

178.galgel 2900 98.3 2952 91.1 3184

179.art 2600 134 1939 131 1988

183.equake 1300 72.1 1802 72.1 1802

187.facerec 1900 90.7 2094 88.8 2140

188.ammp 2200 155 1418 146 1512

189.lucas 2000 103 1933 91.7 2181

191.fma3d 2100 136 1547 125 1682

200.sixtrack 1100 127 863 127 863

301.apsi 2600 161 1612 161 1612

Hardware

CPU: AMD Athlon (TM) 64 FX-57 CPU MHz: 2800 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2x512 MB, PC3200 DDR SDRAM CL2.0 Disk Subsystem: SATA, Western Digital WD740 Other Hardware: None

Software

Operating System: Microsoft Windows XP Pro SP2 Compiler: Intel C++ 8.0 build 20040714Z, Intel Fortran 8.1 build 20041019Z,

PGI Fortran compiler 5.2-4 for Windows XP, AMD Core Math library Version 2.1 (ACML), Microsoft Visual Studio .NET 7.0.9466 (libraries), MicroQuill Smartheap Library 7.0

File System: NTFS System State: Default

Notes/Tuning Information

  +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
  +ACML is linking with AMD Core Math Library V2.1
  ONESTEP is set for all peak runs.
  ifort is the Intel Fortran compiler, icl is the Intel C++ compiler and
  pgf90 is the PGI Fortran compiler.
  The Intel C++ 8.0 and the Intel Fortran 8.1 compilers are setup in the following order:
     "c:program filesintel�ortrancompiler80ia32�inifortvars.bat"
     "c:program filesintelcppcompiler80ia32�iniclvars.bat"
  To make sure that the correct libraries are selected, the following link option is
  added for the peak runs where Intel Fortran 8.1 compiler is used:
      LDOPT = -Fe$@ -link -LIBPATH:"c:program filesintel�ortrancompiler80ia32lib"
   (denoted by +LIBPATH:INTEL8.1 in the optimization flags listed below)
  Portability:
    178.galgel: -Mfixed
  Baseline: C      : icl   -fast -arch:SSE2 -QaxW +FDO
  Baseline: Fortran: pgf90 -fastsse -Mipa=fast,inline
  Peak tuning:

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Advanced Micro Devices

ASUS A8N-SLI Deluxe, AMD Athlon (TM) 64 FX-57

SPECfp2000 = SPECfp_base2000 =

1894 1814

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Jun-2005 Hardware Avail: Jun-2005 Software Avail: Jan-2005

Notes/Tuning Information (Continued)

  168.wupwise:       pgf90 basepeak=yes
  171.swim:          ifort -Qipo  -O3  -QaxN -QxW +FDO -Qunroll0     +LIBPATH:INTEL8.1
  172.mgrid:         pgf90 basepeak=yes
  173.applu:         ifort -Qipo  -O3  -QaxN -QxW +FDO -auto         +LIBPATH:INTEL8.1
  177.mesa:          icl   -Qipo -arch:SSE2       +FDO -Qunroll1 -Qansi_alias
                           -Qoption,f,-ip_ninl_max_stats=1500,-ip_ninl_max_total_stats=4500
  179.art:           icl   -Qipo             -Zp4 +FDO
  183.equake:        icl   basepeak=yes
  178.galgel:        pgf90 -fastsse -Mipa=fast,safe RM_SOURCES=lapak.f90 -Munix +ACML
  187.facerec:       ifort -Qipo             -QxW +FDO -Qunroll3     +LIBPATH:INTEL8.1
                           -Qoption,f,-ip_ninl_max_stats=2500,-ip_ninl_max_total_stats=7000
  188.ammp:          icl   -Oa   -arch:SSE2  -Zp4      -Qansi_alias
  189.lucas:         ifort -Qipo             -QxW      -Qunroll1     +LIBPATH:INTEL8.1
  191.fma3d:         ifort -Qipo       -QaxN -QxW +FDO -Qansi-alias- +LIBPATH:INTEL8.1
  200.sixtrack:      pgf90 basepeak=yes
  301.apsi:          pgf90 basepeak=yes
 The tested system can be assembled using a standard ATX form factor, an Antec True 550
 EPS12V power supply, and a PCI or PCIe graphics card.
 Memory timings manually set in BIOS: CAS=2, TRCD=2, TRAS=5, TRP=2
 Memory used is Corsair CMX512-3200XLPRO configured in dual channel mode.
 BIOS version V6.00PG