Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation IBM 4812-001 (2.0 GHz Pentium M)

SPECint_rate2000 = SPECint_rate_base2000 =

16.6 16.5

SPEC license #: 11 Tested by: IBM, Rochester, MN Test date: Aug-2004 Hardware Avail: Oct-2004 Software Avail: Oct-2004

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 3 6 9 12 15 18 21 24 27 164.gzip 4 497 13.1 4 497 13.1

175.vpr 4 443 14.7 4 443 14.7

176.gcc 4 262 19.5 4 262 19.5

181.mcf 4 768 10.9 4 768 10.9

186.crafty 4 291 15.9 4 291 16.0

197.parser 4 558 15.0 4 558 15.0

252.eon 4 303 19.9 4 282 21.4

253.perlbmk 4 486 17.2 4 487 17.1

254.gap 4 327 15.6 4 327 15.6

255.vortex 4 331 26.6 4 331 26.6

256.bzip2 4 559 12.4 4 537 13.0

300.twolf 4 592 23.5 4 592 23.5

Hardware

CPU: Intel Pentium M 400/200 Mhz System/Memory buses CPU MHz: 2000 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 32K(I) micro-ops + 32KB(D) on chip Secondary Cache: 2MB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 1 x 1024MB DDR200 Registered ECC Disk Subsystem: 1 iSeries 2757-001 Disk IOA,

16 x 35.18GB 3516 15k RPM, unprotected. Other Hardware: 4812 attached within iSeries 9406-810, cpu 25F0-000

Software

Operating System: Windows Server 2003 Standard Edition Build 3790 Compiler: Intel C++ Compiler 8.0 (20031017Z) Microsoft Visual Studio .NET (7.0.9466) File System: NTFS System State: Default

Notes/Tuning Information

 PORTABILITY FLAGS
   176.gcc:     -Dalloca=_alloca /F10000000
   186.crafty:  -DNT_i386
   253.perlbmk: -DSPEC_CPU2000_NTOS -DPERLDLL /MT
   254.gap:     -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO
 FEEDBACK DIRECTED OPTIMIZATION
   ONESTEP=yes
 BASE TUNING
   C:           -QxW -Qipo -O3 +FDO
   C++:         -QxW -Qipo -GX -GR
 PEAK TUNING
   164.gzip:    -QxW -Qipo -Oa -O3 +FDO
   175.vpr:     -QxW -Qipo     -O3 +FDO
   176.gcc:     -QxW -Qipo     -O3 +FDO
   181.mcf:     -QxW -Qipo     -O3 +FDO
   186.crafty:  -QxW -Qipo     -O3 +FDO
   197.parser:  -QxW -Qipo     -O3 +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation IBM 4812-001 (2.0 GHz Pentium M)

SPECint_rate2000 = SPECint_rate_base2000 =

16.6 16.5

SPEC license #: 11 Tested by: IBM, Rochester, MN Test date: Aug-2004 Hardware Avail: Oct-2004 Software Avail: Oct-2004

Notes/Tuning Information (Continued)

   252.eon:     -QxW -Qipo     -O3 +FDO
   253.perlbmk: -QxW -Qipo     -O3 +FDO
   254.gap:     basepeak=yes
   255.vortex   basepeak=yes
   256.bzip2:   -Qipo -Oa -Qunroll1 +FDO
   300.twolf:   basepeak=yes
 EXTRA LIBRARIES
This system is a fully contained Intel based processor board.
It supports all non-PCI devices directly on the board e.g
 memory, keyboard, mouse, display.
It attaches to the system as another PCI device.  The Windows
OS is provided PCI device drivers to allow the system to use
the PCI devices attached to the host iSeries system.  The host
OS then supports the use by Windows of the devices such as disks.

More information about the xSeries board in iSeries systems can
been found at http://www.ibm.com/servers/eserver/iseries/library
In particular, there is a Redbook available titled:
"Microsoft Windows Server 2003 Integration with iSeries"
that provides lots more detailed information.