Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Advanced Micro Devices

TYAN S2865 K8E Tomcat, AMD Opteron (TM) 152

SPECfp2000 = SPECfp_base2000 =

2045 1901

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Jul-2005 Hardware Avail: Aug-2005 Software Avail: Aug-2005

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 56.6 2826 52.8 3032

171.swim 3100 148 2099 145 2137

172.mgrid 1800 109 1652 102 1773

173.applu 2100 99.7 2107 92.2 2277

177.mesa 1400 69.3 2020 65.3 2143

178.galgel 2900 95.1 3048 86.4 3357

179.art 2600 98.0 2652 71.7 3627

183.equake 1300 77.9 1668 70.8 1835

187.facerec 1900 82.1 2314 78.0 2436

188.ammp 2200 145 1512 135 1628

189.lucas 2000 106 1891 106 1891

191.fma3d 2100 130 1614 129 1623

200.sixtrack 1100 131 838 124 884

301.apsi 2600 162 1602 156 1663

Hardware

CPU: AMD Opteron (TM) 152 (939-pin) CPU MHz: 2600 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB (I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 4x512 MB, DDR400 CL2.0 Disk Subsystem: IDE, Western Digital WD2000JB, 7200 rpm Other Hardware: None

Software

Operating System: SuSE Linux Enterprise Server 9 (SP2) for AMD64 Compiler: PathScale EKOPath(TM) Compiler Suite, Release 2.1 File System: Linux/ext3 System State: Multi-user, run level 3

Notes/Tuning Information

Tested by AMD

 +FDO: PASS1= -fb_create fbdata  PASS2= -fb_opt fbdata
 +ACML  means -L/opt/acml2.5.1/pathscale64/lib -lacml,
        which causes linking with AMD Core Math Library V2.5.1

 Baseline optimization
   C programs:       -Ofast -WOPT:mem_opnds=on +FDO
   Fortran programs: -Ofast -LNO:fusion=2 -OPT:fast_complex=on +FDO
 Portability Flags:
   178.galgel:  -fixedform

Peak Tuning:
 168.wupwise:   -Ofast -LNO:prefetch_ahead=5:prefetch=3
                -OPT:unroll_times_max=8:unroll_size=128:IEEE_NaN_Inf=off:ro=3
                -IPA:linear=on:plimit=50000:callee_limit=5000
                -INLINE:aggressive=on

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Advanced Micro Devices

TYAN S2865 K8E Tomcat, AMD Opteron (TM) 152

SPECfp2000 = SPECfp_base2000 =

2045 1901

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Jul-2005 Hardware Avail: Aug-2005 Software Avail: Aug-2005

Notes/Tuning Information (Continued)

 171.swim:      -Ofast -LNO:fusion=2 -m3dnow
 172.mgrid:     -O3 -LNO:fusion=2:blocking=off
                -OPT:Ofast:unroll_times_max=8:unroll_size=256:ro=3
                -CG:gcm=off:cflow=off -m3dnow
 173.applu:     -Ofast -CG:local_fwd_sched=on
                -LNO:fusion=2:fission=2:full_unroll_size=10000:prefetch=3
                -OPT:ro=3 -TENV:X=3
 177.mesa:      -O2 -ipa -OPT:Ofast -fno-math-errno -CG:local_fwd_sched=on +FDO
 178.galgel:    -Ofast -OPT:fast_complex=on +ACML
 179.art:       -O3 -OPT:ro=2:div_split=on:alias=typed -fno-math-errno -m32
 183.equake:    -Ofast -CG:load_exe=2 -OPT:treeheight=on -WOPT:mem_opnds=on
                -m32 +FDO
 187.facerec:   -Ofast -OPT:IEEE_NaN_Inf=off:ro=3 -LNO:fusion=2
                -IPA:plimit=1500 +FDO
 188.ammp:      -O3 -OPT:alias=disjoint:unroll_times_max=8:Ofast:ro=3
                -fno-math-errno -TENV:X=4 +FDO
 189.lucas:      basepeak = true
 191.fma3d:     -O2 -ipa -CG:load_exe=1 -OPT:Ofast:IEEE_arith=3:ro=3
                -WOPT:mem_opnds=on:retype_expr=on -IPA:pu_reorder=1 +FDO
 200.sixtrack:= -O3 -OPT:Ofast:Olimit=6000 -fno-math-errno -CG:load_exe=1 +FDO
 301.apsi:      -Ofast -TENV:X=4 -LNO:fusion=2:prefetch=0
 The tested system can be assembled using a standard ATX footprint, an Antec True 550
 Watt EPS12V power supply, and a PCI or PCIe graphics card.
 All memory slots were populated with Corsair CMX512-3200XL.
 Memory timings manually set in BIOS: CAS=2, TRCD=2, TRAS=5, TRP=2
 BIOS version 1.01