Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Supermicro PDSMi Motherboard

SPECfp2000 = SPECfp_base2000 =

1740 1732

SPEC license #:001176 Tested by: Supermicro Test date: Aug-2005 Hardware Avail: Aug-2005 Software Avail: Apr-2005

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 61.5 2602 61.5 2602

171.swim 3100 119 2600 119 2600

172.mgrid 1800 125 1443 125 1444

173.applu 2100 133 1575 130 1610

177.mesa 1400 98.8 1416 98.8 1416

178.galgel 2900 110 2636 110 2637

179.art 2600 77.1 3371 77.1 3371

183.equake 1300 50.8 2561 49.0 2654

187.facerec 1900 101 1877 101 1881

188.ammp 2200 238 925 237 929

189.lucas 2000 92.7 2157 92.6 2159

191.fma3d 2100 142 1476 142 1476

200.sixtrack 1100 173 635 173 635

301.apsi 2600 207 1256 207 1257

Hardware

CPU: Intel Pentium D 840 Processor ( 3.2GHz, 800 MHz bus) CPU MHz: 3200 FPU: Integrated CPU(s) enabled: 2 cores, 1 chip, 2 cores/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 12k micro-ops I + 16KBD/core on chip Secondary Cache: 1024KB/core on chip L3 Cache: N/A Other Cache: N/A Memory: 4 X 1024MB DDR2-667 ECC Unbuffered Disk Subsystem: 1 X IDE Maxtor DiamondMax Plus 9 250GB Other Hardware: N/A

Software

Operating System: Windows 2003 Enterprise Server Compiler: Intel C++ and Fortran Compiler 9.0 Build 20050430Z (32-bit)

Microsoft Visual Studio .Net 2003(for libraries) SmartHeap Library Version 7.4 from http://www.microquill.com/

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=  -Qprof_gen  PASS2=-Qprof_use
 Base tuning for Fortran programs:  -fast -Qansi_alias +FDO
 Base tuning for 177.mesa:  -fast shlW32M.lib +FDO
 Base tuning for 179.art:  -fast shlW32M.lib +FDO
 Base tuning for 183.equake:  -fast shlW32M.lib +FDO
 Base tuning for 188.ammp:  -fast shlW32M.lib +FDO
 Portability:
 178.galgel:   -FI /F32000000
 191.fmma3d approved windowsdp src.alt used
 Peak tuning:
 168.wupwise:  -fast -Qansi_alias +FDO
 171.swim:     -fast -Qansi_alias +FDO
 172.mgrid:    -fast -Qansi_alias +FDO
 173.applu:  -fast -Qscalar_rep- -Qauto  +FDO
 177.mesa:   basepeak=yes
 178.galgel:   -fast -Qansi_alias +FDO
 179.art:      basepeak=yes

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Supermicro PDSMi Motherboard

SPECfp2000 = SPECfp_base2000 =

1740 1732

SPEC license #:001176 Tested by: Supermicro Test date: Aug-2005 Hardware Avail: Aug-2005 Software Avail: Apr-2005

Notes/Tuning Information (Continued)

 183.equake:   -QxP -Oa -Qrcd -Qipo shlW32M.lib +FDO
 187.facerec:  -fast -Qunroll1 -Qscalar_rep- +FDO
 188.ammp:     -fast -Oa +FDO shlW32M.lib
 189.lucas:    -fast -Qprefetch- +FDO
 191.fma3d:    basepeak=yes
 200.sixtrack: -Qipo -QxP +FDO

 Tested system was built with Mini 1U SC512C-260 Chassis.  Use only with Supermicro chassis recommended

 Product description located as of:
 http://www.supermicro.com/products/motherboard/DualCore/E7230/PDSMi.cfm
 The system bus runs at 800MHz