Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Dell PowerEdge 1800 (3.8GHz Intel Xeon)

SPECfp2000 = SPECfp_base2000 =

1842 1834

SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Aug-2005 Hardware Avail: Oct-2005 Software Avail: Mar-2005

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 2000 4000 6000 8000

168.wupwise 1600 60.0 2667 60.0 2667

171.swim 3100 134 2313 134 2313

172.mgrid 1800 114 1572 114 1572

173.applu 2100 136 1540 137 1538

177.mesa 1400 84.9 1650 84.9 1650

178.galgel 2900 79.0 3670 79.0 3670

179.art 2600 63.6 4088 63.6 4088

183.equake 1300 64.6 2014 64.6 2014

187.facerec 1900 103 1840 103 1840

188.ammp 2200 177 1245 170 1297

189.lucas 2000 99.5 2010 98.4 2032

191.fma3d 2100 138 1521 138 1521

200.sixtrack 1100 160 686 159 694

301.apsi 2600 191 1358 191 1358

Hardware

CPU: Intel Xeon (3.8GHz, 2MB L2, 800MHz system bus) CPU MHz: 3800 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip (Hyper-Threading Technology disabled) CPU(s) orderable: 1,2 Parallel: No Primary Cache: 12KB(I) + 16KB(D) on chip Secondary Cache: 2048KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 4x2GB (dual-ranked) ECC 400MHz DDR2 SDRAM Disk Subsystem: 1 x 36GB 15000RPM SCSI Other Hardware: None

Software

Operating System: Windows Server 2003, Standard Edition, Service Pack 1 Compiler: Intel C/C++/FORTRAN Compiler 8.1 for IA32 (20041119Z)

Microsoft Visual Studio .NET 2003(7.1.3088, for libraries)

File System: NTFS System State: Default

Notes/Tuning Information

 GENERAL
   ONESTEP=yes
   +FDO:   PASS1=-Qprof_gen  PASS2=-Qprof_use
 PORTABILITY
   178.galgel:   -FI /F32000000
   191.fma3d:    srcalt=windowsdp
 BASE TUNING
   C/F77/F90:    -fast -Qansi_alias +FDO
 PEAK TUNING
   168.wupwise:  basepeak=yes
   171.swim:     basepeak=yes
   172.mgrid:    basepeak=yes
   173.applu:    -fast -Qansi_alias -Qscalar_rep- -Qauto +FDO
   177.mesa:     basepeak=yes
   178.galgel:   basepeak=yes
   179.art:      basepeak=yes
   183.equake:   -fast -Qansi_alias -Oa -Qrcd +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Dell PowerEdge 1800 (3.8GHz Intel Xeon)

SPECfp2000 = SPECfp_base2000 =

1842 1834

SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Aug-2005 Hardware Avail: Oct-2005 Software Avail: Mar-2005

Notes/Tuning Information (Continued)

   187.facerec:  -fast -Qunroll1 -Qscalar_rep- +FDO
   188.ammp:     -Oa -QxP
   189.lucas:    -fast
   191.fma3d:    basepeak=yes
   200.sixtrack: -QxP -Qipo +FDO*
   301.apsi:     basepeak=yes
 NOTES
   *+FDO does not include -QxP for PASS1 to enable cross-compilation.