Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Acer Incorporated

Acer Altos R510 Mk2 (3.0 GHz Intel Xeon processor, 2MB L2, 800MHz system bus)

SPECint_rate2000 = SPECint_rate_base2000 =

33.0 33.0

SPEC license #: 97 Tested by: Acer Incorporated Test date: Dec-2005 Hardware Avail: Jan-2006 Software Avail: Apr-2005

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 10 20 30 40 50 60 164.gzip 2 142 22.9 2 142 22.9

175.vpr 2 142 22.8 2 140 23.1

176.gcc 2 64.0 39.9 2 64.0 39.9

181.mcf 2 123 34.1 2 123 34.1

186.crafty 2 90.1 25.8 2 90.1 25.8

197.parser 2 145 28.7 2 145 28.7

252.eon 2 69.2 43.6 2 69.4 43.5

253.perlbmk 2 99.5 42.0 2 99.8 41.8

254.gap 2 74.7 34.2 2 74.7 34.2

255.vortex 2 77.8 56.6 2 77.8 56.6

256.bzip2 2 137 25.3 2 137 25.3

300.twolf 2 196 35.6 2 196 35.6

Hardware

CPU: Intel Xeon (3.0 GHz, 2MB L2, 800MHz system bus) CPU MHz: 3000 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip(Hyper-Threading Technology Disabled) CPU(s) orderable: 1,2 Parallel: No Primary Cache: 12KB(I) micro-ops + 16KB(D) on chip Secondary Cache: 2048KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 6 x 512MB ECC DDR2-400 SDRAM Disk Subsystem: 1 x 160GB 7200RPM SATA HDD Other Hardware:

Software

Operating System: Microsoft Windows Server 2003 Enterprise Edition (Build 3790) Compiler: Intel C++ Compiler 9.0 Build 20050430Z for IA32

Microsoft Visual Studio .Net 2003(7.1.3091, for libraries) shlW32M.lib is SmartHeap Library Version 7.4 from http://www.microquill.com/

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
 Base tuning for C programs:   -fast +FDO shlW32M.lib
 Base tuning for C++ programs: -fast -Qcxx_features +FDO shlW32M.lib
 Portability flags:
 176.gcc: -Dalloca=_alloca /F10000000
 186.crafy: -DNT_i386
 252.eon:   Approved stdcpp src.alt used
 253.perlbmk: -DSPEC_CPU2000_NTOS -DPERLDLL /MT
 254.gap: -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO
 Peak tuning:
 164.gzip:     basepeak=yes
 175.vpr:      -fast -Qansi_alias +FDO
 176.gcc:      basepeak=yes
 181.mcf:      basepeak=yes
 186.crafty:   basepeak=yes
 197.parser:   -fast -Qansi_alias  +FDO
 252.eon:      -fast +FDO
 253.perlbmk:  -fast -Qansi_alias +FDO shlW32M.lib
 254.gap:      basepeak=yes
 255.vortex    basepeak=yes

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Acer Incorporated

Acer Altos R510 Mk2 (3.0 GHz Intel Xeon processor, 2MB L2, 800MHz system bus)

SPECint_rate2000 = SPECint_rate_base2000 =

33.0 33.0

SPEC license #: 97 Tested by: Acer Incorporated Test date: Dec-2005 Hardware Avail: Jan-2006 Software Avail: Apr-2005

Notes/Tuning Information (Continued)

 256.bzip2:   -fast -Oa -Qunroll1 +FDO
 300.twolf:    -fast  +FDO shlW32M.lib
 Enable hardware prefetching and adjacent cache line prefetch BIOS setting
 Product description located at http://www.acer.com