Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

IBM Corporation

IBM System p5 575 (1900 MHz, 1 CPU)

SPECfp2000 = SPECfp_base2000 =

3042 2830

SPEC license #: 11 Tested by: IBM Test date: Dec-2005 Hardware Avail: Feb-2006 Software Avail: Feb-2006

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 10000 20000 30000

168.wupwise 1600 61.9 2584 54.6 2933

171.swim 3100 75.6 4098 75.6 4098

172.mgrid 1800 70.1 2566 66.0 2726

173.applu 2100 99.1 2119 87.2 2407

177.mesa 1400 108 1299 105 1328

178.galgel 2900 49.3 5888 34.2 8483

179.art 2600 16.7 15586 16.0 16261

183.equake 1300 22.1 5873 21.7 5978

187.facerec 1900 72.9 2607 71.2 2670

188.ammp 2200 157 1401 140 1575

189.lucas 2000 36.6 5460 32.8 6107

191.fma3d 2100 121 1736 121 1740

200.sixtrack 1100 130 846 130 846

301.apsi 2600 146 1784 146 1783

Hardware

CPU: POWER5+ CPU MHz: 1900 FPU: Integrated CPU(s) enabled: 1 core, 8 chips, 2 cores/chip (SMT off) CPU(s) orderable: 8,16 Parallel: No Primary Cache: 64KBI+32KBD (on chip)/core Secondary Cache: 1920KB unified, shared (on chip)/chip L3 Cache: 36MB unified (off-chip)/DCM, 8 DCMs/SUT Other Cache: None Memory: 64x2GB Disk Subsystem: 2x73GB SCSI, 15K RPM Other Hardware: None

Software

Operating System: AIX 5L V5.3 Compiler: XL C/C++ Enterprise Edition Version 8.0 for AIX

XL Fortran Enterprise Edition Version 10.1 for AIX Other Software: ESSL 4.2.0.2

File System: AIX/JFS2 System State: Multi-user

Notes/Tuning Information

  Portability Flags:
       -qfixed used in:        168.wupwise, 171.swim, 172.mgrid, 173.applu,
                               178.galgel, 200.sixtrack, 301.apsi
       -qsuffix=f=f90 used in: 178.galgel, 187.facerec, 189.lucas, 191.fma3d

  Base Optimization Flags:
    Fortran:    -O5 -lhmu -blpdata -lmass
    C:          -qpdf1/pdf2
                -O5 -blpdata -qalign=natural

  Peak Optimization Flags
    168.wupwise:  -O5 -qsave -blpdata -lhmu -lmass
    171.swim:     basepeak=1
    172.mgrid:    -qpdf1/pdf2
                  -O4 -qipa=partition=large -q64 -blpdata
    173.applu:    -O5 -qarch=pwr3 -qtune=pwr3 -qalign=struct=natural -qfdpr -q64 -blpdata
                   fdpr -q -O3

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

IBM Corporation

IBM System p5 575 (1900 MHz, 1 CPU)

SPECfp2000 = SPECfp_base2000 =

3042 2830

SPEC license #: 11 Tested by: IBM Test date: Dec-2005 Hardware Avail: Feb-2006 Software Avail: Feb-2006

Notes/Tuning Information (Continued)

    177.mesa:     -qpdf1/pdf2
                   -O5 -qfdpr
                   fdpr -q -O3
    178.galgel:   -qpdf1/pdf2
                  -O5 -qfdpr -lhmu -blpdata -lmass -qessl -lessl
                  fdpr -q -O3
    179.art:      -qpdf1/pdf2
                  -O5 -qhot=arraypad -Q -qalign=natural -blpdata -lhmu
    183.equake:   -qpdf1/pdf2
                  -O3 -qarch=auto -qtune=auto -qipa=level=2 -blpdata
    187.facerec:  -O5 -qsave -blpdata
    188.ammp:     -O5 -qalign=natural -qfdpr -blpdata -lhmu
                  fdpr -q -O3
    189.lucas:    -O3 -qarch=auto -qtune=auto -qfdpr -blpdata -qessl -lessl
                  fdpr -q -O3
    191.fma3d:    -qpdf1/pdf2
                  -O3 -qarch=auto -qtune=auto -qipa=level=2 -q64 -lhmu -blpdata -lmass
    200.sixtrack: -qpdf1/pdf2
                  -O4 -qfdpr
                  fdpr -q -O3
    301.apsi:     -O5

 _{The installed OS level is AIX 5L for POWER version 5.3 with the 5300-04 Recommended Technology Level.}

  SMT:  Acronym for "Simultaneous Multi-Threading". A processor technology that allows
        the simultaneous execution of multiple thread contexts within a single processor
        core. (Enabled by default)
  DCM:  Acronym for "Dual-Chip Module" (one dual-core processor chip + one L3-cache chip)
  SUT:  Acronym for "System Under Test"
  ESSL: Engineering and Scientific Subroutine Library

  ANSI C89:       IBM XL C for AIX invoked as xlc
  Fortran 77:     IBM XL Fortran for AIX invoked as xlf90
  Fortran 90:     IBM XL Fortran for AIX invoked as xlf90

  ulimits set to unlimited.
  Large page mode and memory affinity were set as follows:
      vmo -r -o lgpg_regions=1600 -o lgpg_size=16777216
      chuser capabilities=CAP_BYPASS_RAC_VMM,CAP_PROPAGATE $USER
      shutdown -rF
      export MEMORY_AFFINITY=MCM

  The following config-file entry was used to assign each benchmark process to a core:
       submit = bindprocessor $$ $SPECUSERNUM; $command
  The "bindprocessor" AIX command binds a process to a CPU core.
  Fifteen cores were deconfigured and SMT disabled using the AIX commands
       smtctl -m off -w boot
       bosboot -aD
       shutdown -rF
       drmgr -r -c cpu
       drmgr -r -c cpu
       drmgr -r -c cpu
       drmgr -r -c cpu
       drmgr -r -c cpu
       drmgr -r -c cpu

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

IBM Corporation

IBM System p5 575 (1900 MHz, 1 CPU)

SPECfp2000 = SPECfp_base2000 =

3042 2830

SPEC license #: 11 Tested by: IBM Test date: Dec-2005 Hardware Avail: Feb-2006 Software Avail: Feb-2006

Notes/Tuning Information (Continued)

       drmgr -r -c cpu
       drmgr -r -c cpu
       drmgr -r -c cpu
       drmgr -r -c cpu
       drmgr -r -c cpu
       drmgr -r -c cpu
       drmgr -r -c cpu
       drmgr -r -c cpu
       drmgr -r -c cpu